ARM®-based Cortex®-M4 32b MCU+FPU, up to 256KB Flash+ 48KB SRAM, 4 ADCs, 2 DAC ch., 7 comp, 4 PGA, timers, 2.0-3.6 V

**Datasheet** - **production data**

## Features



* Core: ARM® Cortex®-M4 32-bit CPU with FPU (72 MHz max), single-cycle multiplication and HW division, 90 DMIPS (from CCM), DSP instruction and MPU (memory protection unit)
* Operating conditions:
  + VDD, VDDA voltage range: 2.0 V to 3.6 V
* Memories
  + 128 to 256 Kbytes of Flash memory
  + Up to 40 Kbytes of SRAM, with HW parity check implemented on the first 16 Kbytes.
  + Routine booster: 8 Kbytes of SRAM on instruction and data bus, with HW parity check (CCM)
* CRC calculation unit
* Reset and supply management
  + Power-on/Power-down reset (POR/PDR)
  + Programmable voltage detector (PVD)
  + Low-power modes: Sleep, Stop and Standby
  + VBAT supply for RTC and backup registers
* Clock management
  + 4 to 32 MHz crystal oscillator
  + 32 kHz oscillator for RTC with calibration
  + Internal 8 MHz RC with x 16 PLL option
  + Internal 40 kHz oscillator
* Up to 87 fast I/Os
  + All mappable on external interrupt vectors
  + Several 5 V-tolerant
* Interconnect matrix
* 12-channel DMA controller
* Four ADCs 0.20 µS (up to 39 channels) with selectable resolution of 12/10/8/6 bits, 0 to

3.6 V conversion range, single ended/differential input, separate analog supply from 2 to 3.6 V

* Two 12-bit DAC channels with analog supply

from 2.4 to 3.6 V

* Seven fast rail-to-rail analog comparators with analog supply from 2 to 3.6 V
* Four operational amplifiers that can be used in PGA mode, all terminals accessible with analog supply from 2.4 to 3.6 V
* Up to 24 capacitive sensing channels supporting touchkey, linear and rotary touch sensors



LQFP48 (7 × 7 mm)

LQFP64 (10 × 10 mm) WLCSP100 (0.4 mm pitch)

LQFP100 (14 × 14 mm)

* Up to 13 timers
  + One 32-bit timer and two 16-bit timers with up to 4 IC/OC/PWM or pulse counter and quadrature (incremental) encoder input
  + Two 16-bit 6-channel advanced-control timers, with up to 6 PWM channels, deadtime generation and emergency stop
  + One 16-bit timer with 2 IC/OCs, 1 OCN/PWM, deadtime generation and emergency stop
  + Two 16-bit timers with IC/OC/OCN/PWM, deadtime generation and emergency stop
  + Two watchdog timers (independent, window)
  + SysTick timer: 24-bit downcounter
  + Two 16-bit basic timers to drive the DAC
* Calendar RTC with Alarm, periodic wakeup from Stop/Standby
* Communication interfaces
  + CAN interface (2.0B Active)
  + Two I2C Fast mode plus (1 Mbit/s) with

20 mA current sink, SMBus/PMBus, wakeup from STOP

* + Up to five USART/UARTs (ISO 7816 interface, LIN, IrDA, modem control)
  + Up to three SPIs, two with multiplexed half/full duplex I2S interface, 4 to 16 programmable bit frames
  + USB 2.0 full speed interface
  + Infrared transmitter
* Serial wire debug, Cortex®-M4 with FPU ETM, JTAG
* 96-bit unique ID

###### Table 1. Device summary

|  |  |
| --- | --- |
| **Reference** | **Part number** |
| STM32F303xB | STM32F303CB, STM32F303RB, STM32F303VB |
| STM32F303xC | STM32F303CC, STM32F303RC, STM32F303VC |

**Contents**

1. [Introduction 9](#_bookmark2)
2. [Description 10](#_bookmark4)
3. [Functional overview 13](#_bookmark9)
   1. [ARM](#_bookmark10)® Cortex®-M4 core with FPU with embedded Flash and SRAM 13
   2. [Memory protection unit (MPU) 13](#_bookmark11)
   3. [Embedded Flash memory 13](#_bookmark13)
   4. [Embedded SRAM 14](#_bookmark14)
   5. [Boot modes 14](#_bookmark16)
   6. [Cyclic redundancy check (CRC) 14](#_bookmark17)
   7. [Power management 15](#_bookmark18)
      1. [Power supply schemes 15](#_bookmark19)
      2. [Power supply supervision 15](#_bookmark21)
      3. [Voltage regulator 15](#_bookmark22)
      4. [Low-power modes 16](#_bookmark23)
   8. [Interconnect matrix 16](#_bookmark24)
   9. [Clocks and startup 17](#_bookmark27)
   10. [General-purpose input/outputs (GPIOs) 19](#_bookmark31)
   11. [Direct memory access (DMA) 19](#_bookmark33)
   12. [Interrupts and events 19](#_bookmark34)
       1. [Nested vectored interrupt controller (NVIC) 19](#_bookmark35)
   13. [Fast analog-to-digital converter (ADC) 20](#_bookmark36)
       1. [Temperature sensor 20](#_bookmark38)
       2. [Internal voltage reference (V](#_bookmark40)REFINT) 20
       3. [V](#_bookmark42)BAT battery voltage monitoring 21
       4. [OPAMP reference voltage (VREFOPAMP) 21](#_bookmark44)
   14. [Digital-to-analog converter (DAC) 21](#_bookmark45)
   15. [Operational amplifier (OPAMP) 21](#_bookmark47)
   16. [Fast comparators (COMP) 22](#_bookmark48)
   17. [Timers and watchdogs 22](#_bookmark49)
       1. [Advanced timers (TIM1, TIM8) 23](#_bookmark51)
       2. [Basic timers (TIM6, TIM7) 23](#_bookmark53)
       3. [Independent watchdog (IWDG) 24](#_bookmark54)
       4. [Window watchdog (WWDG) 24](#_bookmark55)
       5. [SysTick timer 24](#_bookmark56)
   18. [Real-time clock (RTC) and backup registers 24](#_bookmark57)
   19. [Inter-integrated circuit interface (I](#_bookmark59)2C) 25
   20. [Universal synchronous/asynchronous receiver transmitter (USART) 26](#_bookmark64)
   21. [Universal asynchronous receiver transmitter (UART) 26](#_bookmark65)
   22. [Serial peripheral interface (SPI)/Inter-integrated sound interfaces (I2S) . 27](#_bookmark68)
   23. [Controller area network (CAN) 27](#_bookmark71)
   24. [Universal serial bus (USB) 27](#_bookmark72)
   25. [Infrared Transmitter 28](#_bookmark74)
   26. [Touch sensing controller (TSC) 28](#_bookmark76)
   27. [Development support 30](#_bookmark81)
       1. [Serial wire JTAG debug port (SWJ-DP) 30](#_bookmark82)
       2. [Embedded trace macrocell™ 30](#_bookmark83)
4. [Pinouts and pin description 31](#_bookmark84)
5. [Memory mapping 52](#_bookmark105)
6. [Electrical characteristics 55](#_bookmark108)
   1. [Parameter conditions 55](#_bookmark109)
      1. [Minimum and maximum values 55](#_bookmark110)
      2. [Typical values 55](#_bookmark111)
      3. [Typical curves 55](#_bookmark112)
      4. [Loading capacitor 55](#_bookmark113)
      5. [Pin input voltage 55](#_bookmark114)
      6. [Power supply scheme 56](#_bookmark117)
      7. [Current consumption measurement 57](#_bookmark120)
   2. [Absolute maximum ratings 57](#_bookmark122)
   3. [Operating conditions 59](#_bookmark128)
      1. [General operating conditions 59](#_bookmark129)
      2. [Operating conditions at power-up / power-down 60](#_bookmark133)
      3. [Embedded reset and power control block characteristics 60](#_bookmark136)
      4. [Embedded reference voltage 62](#_bookmark140)
      5. [Supply current characteristics 62](#_bookmark145)
      6. [Wakeup time from low-power mode 73](#_bookmark168)
      7. [External clock source characteristics 74](#_bookmark172)
      8. [Internal clock source characteristics 79](#_bookmark183)
      9. [PLL characteristics 81](#_bookmark190)
      10. [Memory characteristics 81](#_bookmark192)
      11. [EMC characteristics 82](#_bookmark196)
      12. [Electrical sensitivity characteristics 83](#_bookmark200)
      13. [I/O current injection characteristics 84](#_bookmark205)
      14. [I/O port characteristics 86](#_bookmark208)
      15. [NRST pin characteristics 91](#_bookmark223)
      16. [Timer characteristics 92](#_bookmark227)
      17. [Communications interfaces 94](#_bookmark232)
      18. [ADC characteristics 103](#_bookmark253)
      19. [DAC electrical specifications 116](#_bookmark278)
      20. [Comparator characteristics 118](#_bookmark283)
      21. [Operational amplifier characteristics 120](#_bookmark289)
      22. [Temperature sensor characteristics 122](#_bookmark293)
      23. [V](#_bookmark297)BAT monitoring characteristics 123
7. [Package information 124](#_bookmark299)
   1. [LQFP100 – 14 x 14 mm, low-profile quad flat package](#_bookmark302)

[information 124](#_bookmark302)

* 1. [LQFP64 – 10 x 10 mm, low-profile quad flat package](#_bookmark308)

[information 127](#_bookmark308)

* 1. [LQFP48 – 7 x 7 mm, low-profile quad flat package](#_bookmark314)

[information 130](#_bookmark314)

* 1. [WLCSP100 - 0.4 mm pitch wafer level chip scale package information 133](#_bookmark319)
  2. [Thermal characteristics 137](#_bookmark326)
     1. [Reference document 137](#_bookmark330)
     2. [Selecting the product temperature range 138](#_bookmark331)

1. [Part numbering 140](#_bookmark332)
2. [Revision history 141](#_bookmark335)

**List of tables**

[Table 1. Device summary 1](#_bookmark1)

[Table 2. STM32F303xB/STM32F303xC family device features and peripheral counts 11](#_bookmark5)

[Table 3. External analog supply values for analog peripherals 15](#_bookmark20)

[Table 4. STM32F303xB/STM32F303xC peripheral interconnect matrix 16](#_bookmark26)

[Table 5. Timer feature comparison 22](#_bookmark50)

[Table 6. Comparison of I2C analog and digital filters 25](#_bookmark60)

[Table 7. STM32F303xB/STM32F303xC I](#_bookmark62)2C implementation 25

[Table 8. USART features 26](#_bookmark66)

[Table 9. STM32F303xB/STM32F303xC SPI/I2S implementation 27](#_bookmark69)

[Table 10. Capacitive sensing GPIOs available on STM32F303xB/STM32F303xC devices 29](#_bookmark78)

[Table 11. No. of capacitive sensing channels available on STM32F303xB/STM32F303xC devices. 29](#_bookmark80) [Table 12. Legend/abbreviations used in the pinout table 35](#_bookmark94)

[Table 13. STM32F303xB/STM32F303xC pin definitions 36](#_bookmark95)

[Table 14. Alternate functions for port A 44](#_bookmark99)

[Table 15. Alternate functions for port B 46](#_bookmark100)

[Table 16. Alternate functions for port C 48](#_bookmark101)

[Table 17. Alternate functions for port D 49](#_bookmark102)

[Table 18. Alternate functions for port E 50](#_bookmark103)

[Table 19. Alternate functions for port F 51](#_bookmark104)

[Table 20. STM32F303xB/STM32F303xC memory map, peripheral register boundary addresses 53](#_bookmark107)

[Table 21. Voltage characteristics 57](#_bookmark123)

[Table 22. Current characteristics 58](#_bookmark125)

[Table 23. Thermal characteristics 58](#_bookmark127)

[Table 24. General operating conditions 59](#_bookmark130)

[Table 25. Operating conditions at power-up / power-down 60](#_bookmark134)

[Table 26. Embedded reset and power control block characteristics 60](#_bookmark137)

[Table 27. Programmable voltage detector characteristics 61](#_bookmark138)

[Table 28. Embedded internal reference voltage 62](#_bookmark141)

[Table 29. Internal reference voltage calibration values 62](#_bookmark143)

[Table 30. Typical and maximum current consumption from V](#_bookmark146)DD supply at VDD = 3.6V 63

[Table 31. Typical and maximum current consumption from the V](#_bookmark149)DDA supply 64

[Table 32. Typical and maximum V](#_bookmark152)DD consumption in Stop and Standby modes 65

[Table 33. Typical and maximum V](#_bookmark154)DDA consumption in Stop and Standby modes 65

[Table 34. Typical and maximum current consumption from V](#_bookmark156)BAT supply 66

[Table 35. Typical current consumption in Run mode, code with data processing running from Flash67](#_bookmark160)

[Table 36. Typical current consumption in Sleep mode, code running from Flash or RAM 68](#_bookmark162)

[Table 37. Switching output I/O current consumption 70](#_bookmark164)

[Table 38. Peripheral current consumption 71](#_bookmark166)

[Table 39. Low-power mode wakeup timings 73](#_bookmark170)

[Table 40. High-speed external user clock characteristics 74](#_bookmark173)

[Table 41. Low-speed external user clock characteristics 75](#_bookmark175)

[Table 42. HSE oscillator characteristics 76](#_bookmark177)

[Table 43. LSE oscillator characteristics (f](#_bookmark180)LSE = 32.768 kHz) 78

[Table 44. HSI oscillator characteristics 79](#_bookmark184)

[Table 45. LSI oscillator characteristics 80](#_bookmark189)

[Table 46. PLL characteristics 81](#_bookmark191)

[Table 47. Flash memory characteristics 81](#_bookmark193)

[Table 48. Flash memory endurance and data retention 81](#_bookmark195)

[Table 49. EMS characteristics 82](#_bookmark197)

[Table 50. EMI characteristics 83](#_bookmark198)

[Table 51. ESD absolute maximum ratings 83](#_bookmark201)

[Table 52. Electrical sensitivities 84](#_bookmark203)

[Table 53. I/O current injection susceptibility 85](#_bookmark206)

[Table 54. I/O static characteristics 86](#_bookmark210)

[Table 55. Output voltage characteristics 89](#_bookmark217)

[Table 56. I/O AC characteristics 90](#_bookmark219)

[Table 57. NRST pin characteristics 91](#_bookmark224)

[Table 58. TIMx characteristics 92](#_bookmark228)

[Table 59. IWDG min/max timeout period at 40 kHz (LSI) 93](#_bookmark230)

[Table 60. WWDG min-max timeout value @72 MHz (PCLK) 93](#_bookmark231)

[Table 61. I2C timings specification (see I2C specification, rev.03, June 2007) 94](#_bookmark234)

[Table 62. I2C analog filter characteristics 95](#_bookmark236)

[Table 63. SPI characteristics 96](#_bookmark240)

[Table 64. I](#_bookmark245)2S characteristics 99

[Table 65. USB startup time 101](#_bookmark249)

[Table 66. USB DC electrical characteristics 101](#_bookmark250)

[Table 67. USB: Full-speed electrical characteristics 102](#_bookmark252)

[Table 68. ADC characteristics 103](#_bookmark254)

[Table 69. Maximum ADC RAIN 105](#_bookmark260)

[Table 70. ADC accuracy - limited test conditions, 100-pin packages 107](#_bookmark262)

[Table 71. ADC accuracy, 100-pin packages 109](#_bookmark266)

[Table 72. ADC accuracy - limited test conditions, 64-pin packages 111](#_bookmark269)

[Table 73. ADC accuracy, 64-pin packages 113](#_bookmark271)

[Table 74. ADC accuracy at 1MSPS 114](#_bookmark274)

[Table 75. DAC characteristics 116](#_bookmark279)

[Table 76. Comparator characteristics 118](#_bookmark285)

[Table 77. Operational amplifier characteristics 120](#_bookmark290)

[Table 78. TS characteristics 122](#_bookmark294)

[Table 79. Temperature sensor calibration values 122](#_bookmark295)

[Table 80. V](#_bookmark298)BAT monitoring characteristics 123

[Table 81. LQPF100 – 14 x 14 mm, low-profile quad flat package mechanical data 124](#_bookmark304)

[Table 82. LQFP64 – 10 x 10 mm, low-profile quad flat package mechanical data 127](#_bookmark310)

[Table 83. LQFP48 – 7 x 7 mm, low-profile quad flat package mechanical data 130](#_bookmark316)

[Table 84. WLCSP100 – 100L, 4.166 x 4.628 mm 0.4 mm pitch wafer level chip scale](#_bookmark322)

[package mechanical data 134](#_bookmark322)

[Table 85. WLCSP100 recommended PCB design rules (0.4 mm pitch) 135](#_bookmark324)

[Table 86. Package thermal characteristics 137](#_bookmark328)

[Table 87. Ordering information scheme 140](#_bookmark333)

[Table 88. Document revision history 141](#_bookmark336)

**List of figures**

[Figure 1. STM32F303xB/STM32F303xC block diagram 12](#_bookmark7)

[Figure 2. Clock tree 18](#_bookmark29)

[Figure 3. Infrared transmitter 28](#_bookmark75)

[Figure 4. STM32F303xB/STM32F303xC LQFP48 pinout 31](#_bookmark86)

[Figure 5. STM32F303xB/STM32F303xC LQFP64 pinout 32](#_bookmark88)

[Figure 6. STM32F303xB/STM32F303xC LQFP100 pinout 33](#_bookmark90)

[Figure 7. STM32F303xB/STM32F303xC WLCSP100 pinout 34](#_bookmark92)

[Figure 8. STM32F303xB/STM32F303xC memory map 52](#_bookmark106)

[Figure 9. Pin loading conditions 55](#_bookmark115)

[Figure 10. Pin input voltage 55](#_bookmark116)

[Figure 11. Power supply scheme 56](#_bookmark118)

[Figure 12. Current consumption measurement scheme 57](#_bookmark121)

[Figure 13. Typical V](#_bookmark158)BAT current consumption (LSE and RTC ON/LSEDRV[1:0] = ’00’) 66

[Figure 14. High-speed external clock source AC timing diagram 74](#_bookmark174)

[Figure 15. Low-speed external clock source AC timing diagram 75](#_bookmark176)

[Figure 16. Typical application with an 8 MHz crystal 77](#_bookmark179)

[Figure 17. Typical application with a 32.768 kHz crystal 79](#_bookmark181)

[Figure 18. HSI oscillator accuracy characterization results for soldered parts 80](#_bookmark187)

[Figure 19. TC and TTa I/O input characteristics - CMOS port 87](#_bookmark212)

[Figure 20. TC and TTa I/O input characteristics - TTL port 87](#_bookmark213)

[Figure 21. Five volt tolerant (FT and FTf) I/O input characteristics - CMOS port 88](#_bookmark214)

[Figure 22. Five volt tolerant (FT and FTf) I/O input characteristics - TTL port 88](#_bookmark215)

[Figure 23. I/O AC characteristics definition 91](#_bookmark222)

[Figure 24. Recommended NRST pin protection 92](#_bookmark226)

[Figure 25. I](#_bookmark238)2C bus AC waveforms and measurement circuit 95

[Figure 26. SPI timing diagram - slave mode and CPHA = 0 97](#_bookmark242)

[Figure 27. SPI timing diagram - slave mode and CPHA = 1](#_bookmark243)(1) 97

[Figure 28. SPI timing diagram - master mode](#_bookmark244)(1) 98

[Figure 29. I](#_bookmark247)2S slave timing diagram (Philips protocol)(1) 100

[Figure 30. I](#_bookmark248)2S master timing diagram (Philips protocol)(1) 100

[Figure 31. USB timings: definition of data signal rise and fall time 101](#_bookmark251)

[Figure 32. ADC typical current consumption on VDDA pin 104](#_bookmark256)

[Figure 33. ADC typical current consumption on VREF+ pin 105](#_bookmark258)

[Figure 34. ADC accuracy characteristics 115](#_bookmark276)

[Figure 35. Typical connection diagram using the ADC 115](#_bookmark277)

[Figure 36. 12-bit buffered /non-buffered DAC 117](#_bookmark282)

[Figure 37. Maximum VREFINT scaler startup time from power down 119](#_bookmark287)

[Figure 38. OPAMP voltage noise versus frequency 122](#_bookmark292)

[Figure 39. LQFP100 – 14 x 14 mm, low-profile quad flat package outline 124](#_bookmark303)

[Figure 40. LQFP100 – 14 x 14 mm, low-profile quad flat package recommended footprint 125](#_bookmark305)

[Figure 41. LQFP100 – 14 x 14 mm, low-profile quad flat package top view example 126](#_bookmark306)

[Figure 42. LQFP64 – 10 x 10 mm, low-profile quad flat package outline 127](#_bookmark309)

[Figure 43. LQFP64 – 10 x 10 mm, low-profile quad flat package recommended footprint 128](#_bookmark312)

[Figure 44. LQFP64 – 10 x 10 mm, low-profile quad flat package top view example 129](#_bookmark313)

[Figure 45. LQFP48 – 7 x 7 mm, low-profile quad flat package outline 130](#_bookmark315)

[Figure 46. LQFP48 - 7 x 7 mm, low-profile quad flat package recommended footprint 131](#_bookmark317)

[Figure 47. LQFP48 - 7 x 7 mm, low-profile quad flat package top view example 132](#_bookmark318)

[Figure 48. WLCSP100 – 100L, 4.166 x 4.628 mm 0.4 mm pitch wafer level chip scale](#_bookmark321)

[package outline 133](#_bookmark321)

[Figure 49. WLCSP100 – 100L, 4.166 x 4.628 mm 0.4 mm pitch wafer level chip scale](#_bookmark323)

[package recommended footprint 135](#_bookmark323)

[Figure 50. WLCSP100, 0.4 mm pitch wafer level chip scale package](#_bookmark325)

[top view example 136](#_bookmark325)

# Introduction

This datasheet provides the ordering information and mechanical device characteristics of the STM32F303xB/STM32F303xC microcontrollers.

This STM32F303xB/STM32F303xC datasheet should be read in conjunction with the STM32F303x, STM32F358xC and STM32F328x4/6/8 reference manual (RM0316). The reference manual is available from the STMicroelectronics website [*www.st.com*.](http://www.st.com/)

For information on the Cortex®-M4 core with FPU, please refer to:

* + **Cortex**®**-M4 with FPU Technical Reference Manual**, available from ARM website [www.arm.com.](http://www.arm.com/)

###### STM32F3xxx and STM32F4xxx Cortex®-M4 programming manual (PM0214)

available from our website [*www.st.com*.](http://www.st.com/)



# Description

The STM32F303xB/STM32F303xC family is based on the high-performance

ARM® Cortex®-M4 32-bit RISC core with FPU operating at a frequency of up to 72 MHz, and embedding a floating point unit (FPU), a memory protection unit (MPU) and an embedded trace macrocell (ETM). The family incorporates high-speed embedded memories (up to 256 Kbytes of Flash memory, up to 40 Kbytes of SRAM) and an extensive range of enhanced I/Os and peripherals connected to two APB buses.

The devices offer up to four fast 12-bit ADCs (5 Msps), seven comparators, four operational amplifiers, up to two DAC channels, a low-power RTC, up to five general-purpose 16-bit timers, one general-purpose 32-bit timer, and two timers dedicated to motor control. They also feature standard and advanced communication interfaces: up to two I2Cs, up to three SPIs (two SPIs are with multiplexed full-duplex I2Ss), three USARTs, up to two UARTs, CAN and USB. To achieve audio class accuracy, the I2S peripherals can be clocked via an external PLL.

The STM32F303xB/STM32F303xC family operates in the -40 to +85 °C and -40 to +105 °C temperature ranges from a 2.0 to 3.6 V power supply. A comprehensive set of power-saving mode allows the design of low-power applications.

The STM32F303xB/STM32F303xC family offers devices in three packages ranging from 48 pins to 100 pins.

The set of included peripherals changes with the device chosen.

###### Table 2. STM32F303xB/STM32F303xC family device features and peripheral counts

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Peripheral** | | **STM32F303Cx** | | **STM32F303Rx** | | **STM32F303Vx** | |
| Flash (Kbytes) | | 128 | 256 | 128 | 256 | 128 | 256 |
| SRAM (Kbytes) on data bus | | 32 | 40 | 32 | 40 | 32 | 40 |
| CCM (Core Coupled Memory) RAM (Kbytes) | | 8 | | | | | |
| Timers | Advanced control | 2 (16-bit) | | | | | |
| General purpose | 5 (16-bit)  1 (32-bit) | | | | | |
| Basic | 2 (16-bit) | | | | | |
| PWM channels (all) (1) | | 31 | | 33 | | | |
| PWM channels (except complementary) | | 22 | | 24 | | | |
| Communication interfaces | SPI (I2S)(2) | 3(2) | | | | | |
| I2C | 2 | | | | | |
| USART | 3 | | | | | |
| UART | 0 | | 2 | | | |
| CAN | 1 | | | | | |
| USB | 1 | | | | | |
| GPIOs | Normal I/Os (TC, TTa) | 20 | | 27 | | 45 in LQFP100  37 in WLCSP100 | |
| 5-volt tolerant I/Os (FT, FTf) | 17 | | 25 | | 42 in LQFP100  40 in WLCSP100 | |
| DMA channels | | 12 | | | | | |
| Capacitive sensing channels | | 17 | | 18 | | 24 | |
| 12-bit ADCs Number of channels | | 4 | | | | | |
| 15 | | 22 | | 39 in LQFP100  32 in WLCSP100 | |
| 12-bit DAC channels | | 2 | | | | | |
| Analog comparator | | 7 | | | | | |
| Operational amplifiers | | 4 | | | | | |
| CPU frequency | | 72 MHz | | | | | |
| Operating voltage | | 2.0 to 3.6 V | | | | | |
| Operating temperature | | Ambient operating temperature: - 40 to 85 °C / - 40 to 105 °C Junction temperature: - 40 to 125 °C | | | | | |
| Packages | | LQFP48 | | LQFP64 | | LQFP100 WLCSP100 | |

1. This total number considers also the PWMs generated on the complementary output channels
2. The SPI interfaces can work in an exclusive way in either the SPI mode or the I2S audio mode.

###### Figure 1. STM32F303xB/STM32F303xC block diagram

TPIU

ETM

VDD18

Power

VDDIO = 2 to 3.6 V

3.3 V to 1.8V

Voltage reg.

TRADECLK TRACED[O-3]

as AF

JTRST JTDI JTCK/SWCLK JTMS/SWDIO

JTDO As AF

SWJTAG Trace/Trig MPU/FPU

Cortex M4 CPU Fmax: 72 MHz

NVIC

Ibus

Dbus

System

FLASH 256 KB

64 bits

OBL

Flash interface

CCM RAM 8KB

SRAM 4O KB

@VDDA

POR

Reset Int.

@VDDIO

Supply Supervision

POR /PDR

PVD @VDDA

VSS

NRESET VDDA VSSA

**GP DMA1**

7 channels

**GP DMA2**

5 channels

Temp. sensor 12-bit ADC1

RC HS 8MHz

RC LS PLL

BusMatrix

AHBPCLK APBP1CLK

@VDDIO

XTAL OSC 4 -32 MHz

Ind. WDG32K

Standby interface

OSC\_IN OSC\_OUT

VBAT = 1.65V to 3.6V

VREF+ VREF-

IF

12-bit ADC2

AHB3

Reset & clock control

APBP2CLK HCLK FCLK

USARTCLK

@VSW XTAL 32kHz

Backup

OSC32\_IN OSC32\_OUT

12-bit ADC3

IF

12-bit ADC4

CRC

I2CCLK ADC SAR 1/2/3/4 CLK

RTC AWU

Reg (64Byte) Backup interface

ANTI-TAMP

PA[15:O]

PB[15:O]

PC[15:O]

PD[15:O]

PE[15:O]

PF[7:O]

XX Groups of 4 channels as AF

GPIO PORT A  GPIO PORT B  GPIO PORT C  GPIO PORT D  GPIO PORT E

GPIO PORT F

Touch Sensing Controller

AHB2 APB1

AHB2 APB2

TIMER2

(32-bit/PWM)

AHB2

TIMER 3

TIMER 4

SPI2/I2S

SPI3/I2S

USART2

USART3

UART4

4 Channels, ETR as AF 4 Channels, ETR as AF

4 Channels, ETR as AF

MOSI/SD, MISO/ext\_SD, SCK/CK, NSS/WS, MCLK as AF

MOSI/SD, MISO/ext\_SD, SCK/CK, NSS/WS, MCLK as AF

RX, TX, CTS, RTS, as AF

RX, TX, CTS, RTS, as AF RX, TX as AF

RX, TX as AF

SCL, SDA, SMBA as AF

I2C1

UART5

APB1 Fmax = 36 MHz

XX AF

2 Channels,1 Comp Channel, BRK as AF

1 Channel, 1 Comp Channel, BRK as AF

1 Channel, 1 Comp Channel, BRK as AF

4 Channels,

4 Comp channels, ETR, BRK as AF

4 Channels,

4 Comp channels, ETR, BRK as AF

MOSI, MISO, SCK,NSS as AF

RX, TX, CTS, RTS,

SmartCard as AF

EXT.IT WKUP

APB2 fmax = 72 MHz

|  |
| --- |
| TIMER 15 |
|  |
| TIMER 16 |
|  |
| TIMER 17 |

TIMER 1 / PWM

TIMER 8 / PWM

SPI1

USART1

WinWATCHDOG

USB SRAM 512B

TIMER6

TIMER7

SYSCFG CTL

@VDDA

GP Comparator 7 GP Comparator...

GP Comparator 1

I2C2

bx CAN & 512B SRAM

USB 2.O FS

IF

12bit DAC1

@VDDA

INTERFACE

OpAmp1

OpAmp2

OpAmp3

OpAmp4

@VDDA

SCL, SDA, SMBA as AF

CAN TX, CAN RX USB\_DP, USB\_DM

DAC1\_CH1 as AF DAC1\_CH2 as AF

INxx / OUTxx INxx / OUTxx INxx / OUTxx INxx / OUTxx



1. AF: alternate function on I/O pins.

Xx Ins, 7 OUTs as AF

MS1896OV4

# Functional overview

## ARM® Cortex®-M4 core with FPU with embedded Flash and SRAM

The ARM Cortex-M4 processor with FPU is the latest generation of ARM processors for embedded systems. It was developed to provide a low-cost platform that meets the needs of MCU implementation, with a reduced pin count and low-power consumption, while delivering outstanding computational performance and an advanced response to interrupts.

The ARM Cortex-M4 32-bit RISC processor with FPU features exceptional code-efficiency, delivering the high-performance expected from an ARM core in the memory size usually associated with 8- and 16-bit devices.

The processor supports a set of DSP instructions which allow efficient signal processing and complex algorithm execution.

Its single precision FPU speeds up software development by using metalanguage development tools, while avoiding saturation.

With its embedded ARM core, the STM32F303xB/STM32F303xC family is compatible with all ARM tools and software.

[*Figure 1*](#_bookmark7)shows the general block diagram of the STM32F303xB/STM32F303xC family devices.

## Memory protection unit (MPU)

The memory protection unit (MPU) is used to separate the processing of tasks from the data protection. The MPU can manage up to 8 protection areas that can all be further divided up into 8 subareas. The protection area sizes are between 32 bytes and the whole 4 gigabytes of addressable memory.

The memory protection unit is especially helpful for applications where some critical or certified code has to be protected against the misbehavior of other tasks. It is usually managed by an RTOS (real-time operating system). If a program accesses a memory location that is prohibited by the MPU, the RTOS can detect it and take action. In an RTOS environment, the kernel can dynamically update the MPU area setting, based on the process to be executed.

The MPU is optional and can be bypassed for applications that do not need it.

## Embedded Flash memory

All STM32F303xB/STM32F303xC devices feature up to 256 Kbytes of embedded Flash memory available for storing programs and data. The Flash memory access time is adjusted to the CPU clock frequency (0 wait state from 0 to 24 MHz, 1 wait state from 24 to 48 MHz and 2 wait states above).

## Embedded SRAM

STM32F303xB/STM32F303xC devices feature up to 48 Kbytes of embedded SRAM with hardware parity check. The memory can be accessed in read/write at CPU clock speed with 0 wait states, allowing the CPU to achieve 90 Dhrystone Mips at 72 MHz (when running code from the CCM (Core Coupled Memory) RAM).

* 8 Kbytes of CCM RAM mapped on both instruction and data bus, used to execute critical routines or to access data (parity check on all of CCM RAM).
* 40 Kbytes of SRAM mapped on the data bus (parity check on first 16 Kbytes of SRAM).

## Boot modes

At startup, Boot0 pin and Boot1 option bit are used to select one of three boot options:

* Boot from user Flash
* Boot from system memory
* Boot from embedded SRAM

The boot loader is located in the system memory. It is used to reprogram the Flash memory by using USART1 (PA9/PA10), USART2 (PD5/PD6) or USB (PA11/PA12) through DFU

(device firmware upgrade).

## Cyclic redundancy check (CRC)

The CRC (cyclic redundancy check) calculation unit is used to get a CRC code using a configurable generator polynomial value and size.

Among other applications, CRC-based techniques are used to verify data transmission or storage integrity. In the scope of the EN/IEC 60335-1 standard, they offer a means of verifying the Flash memory integrity. The CRC calculation unit helps compute a signature of the software during runtime, to be compared with a reference signature generated at linktime and stored at a given memory location.

## Power management

#### Power supply schemes

* + - * VSS, VDD = 2.0 to 3.6 V: external power supply for I/Os and the internal regulator. It is provided externally through VDD pins.
      * VSSA, VDDA = 2.0 to 3.6 V: external analog power supply for ADC, DACs, comparators operational amplifiers, reset blocks, RCs and PLL. The minimum voltage to be applied to VDDA differs from one analog peripheral to another. [*Table 3*](#_bookmark20)provides the summary of the VDDA ranges for analog peripherals. The VDDA voltage level must be always greater or equal to the VDD voltage level and must be provided first.
      * VBAT = 1.65 to 3.6 V: power supply for RTC, external clock 32 kHz oscillator and backup registers (through power switch) when VDD is not present.

**Table 3. External analog supply values for analog peripherals**

|  |  |  |
| --- | --- | --- |
| **Analog peripheral** | **Minimum VDDA supply** | **Maximum VDDA supply** |
| ADC / COMP | 2.0 V | 3.6 V |
| DAC / OPAMP | 2.4 V | 3.6V |

#### Power supply supervision

The device has an integrated power-on reset (POR) and power-down reset (PDR) circuits. They are always active, and ensure proper operation above a threshold of 2 V. The device remains in reset mode when the monitored supply voltage is below a specified threshold, VPOR/PDR, without the need for an external reset circuit.

* + - * The POR monitors only the VDD supply voltage. During the startup phase it is required that VDDA should arrive first and be greater than or equal to VDD.
      * The PDR monitors both the VDD and VDDA supply voltages, however the VDDA power supply supervisor can be disabled (by programming a dedicated Option bit) to reduce the power consumption if the application design ensures that VDDA is higher than or equal to VDD.

The device features an embedded programmable voltage detector (PVD) that monitors the VDD power supply and compares it to the VPVD threshold. An interrupt can be generated when VDD drops below the VPVD threshold and/or when VDD is higher than the VPVD threshold. The interrupt service routine can then generate a warning message and/or put the MCU into a safe state. The PVD is enabled by software.

#### Voltage regulator

The regulator has three operation modes: main (MR), low-power (LPR), and power-down.

* + - * The MR mode is used in the nominal regulation mode (Run)
      * The LPR mode is used in Stop mode.
      * The power-down mode is used in Standby mode: the regulator output is in high impedance, and the kernel circuitry is powered down thus inducing zero consumption.

The voltage regulator is always enabled after reset. It is disabled in Standby mode.

#### Low-power modes

The STM32F303xB/STM32F303xC supports three low-power modes to achieve the best compromise between low-power consumption, short startup time and available wakeup sources:

* + - * Sleep mode

In Sleep mode, only the CPU is stopped. All peripherals continue to operate and can wake up the CPU when an interrupt/event occurs.

* + - * Stop mode

Stop mode achieves the lowest power consumption while retaining the content of SRAM and registers. All clocks in the 1.8 V domain are stopped, the PLL, the HSI RC and the HSE crystal oscillators are disabled. The voltage regulator can also be put either in normal or in low-power mode.

The device can be woken up from Stop mode by any of the EXTI line. The EXTI line source can be one of the 16 external lines, the PVD output, the USB wakeup, the RTC alarm, COMPx, I2Cx or U(S)ARTx.

* + - * Standby mode

The Standby mode is used to achieve the lowest power consumption. The internal voltage regulator is switched off so that the entire 1.8 V domain is powered off. The PLL, the HSI RC and the HSE crystal oscillators are also switched off. After entering Standby mode, SRAM and register contents are lost except for registers in the Backup domain and Standby circuitry.

The device exits Standby mode when an external reset (NRST pin), an IWDG reset, a rising edge on the WKUP pin or an RTC alarm occurs.

*Note: The RTC, the IWDG and the corresponding clock sources are not stopped by entering Stop or Standby mode.*

## Interconnect matrix

Several peripherals have direct connections between them. This allows autonomous communication between peripherals, saving CPU resources thus power supply consumption. In addition, these hardware connections allow fast and predictable latency.

###### Table 4. STM32F303xB/STM32F303xC peripheral interconnect matrix

|  |  |  |
| --- | --- | --- |
| **Interconnect source** | **Interconnect destination** | **Interconnect action** |
| TIMx | TIMx | Timers synchronization or chaining |
| ADCx DAC1 | Conversion triggers |
| DMA | Memory to memory transfer trigger |
| Compx | Comparator output blanking |
| COMPx | TIMx | Timer input: OCREF\_CLR input, input capture |
| ADCx | TIMx | Timer triggered by analog watchdog |

**Table 4. STM32F303xB/STM32F303xC peripheral interconnect matrix (continued)**

|  |  |  |
| --- | --- | --- |
| **Interconnect source** | **Interconnect destination** | **Interconnect action** |
| GPIO RTCCLK HSE/32 MC0 | TIM16 | Clock source used as input channel for HSI and LSI calibration |
| CSS  CPU (hard fault) COMPx  PVD GPIO | TIM1, TIM8, TIM15, 16, 17 | Timer break |
| GPIO | TIMx | External trigger, timer break |
| ADCx DAC1 | Conversion external trigger |
| DAC1 | COMPx | Comparator inverting input |

*Note: For more details about the interconnect actions, please refer to the corresponding sections in the reference manual (RM0316).*

## Clocks and startup

System clock selection is performed on startup, however the internal RC 8 MHz oscillator is selected as default CPU clock on reset. An external 4-32 MHz clock can be selected, in which case it is monitored for failure. If failure is detected, the system automatically switches back to the internal RC oscillator. A software interrupt is generated if enabled. Similarly, full interrupt management of the PLL clock entry is available when necessary (for example with failure of an indirectly used external oscillator).

Several prescalers allow to configure the AHB frequency, the high speed APB (APB2) and the low speed APB (APB1) domains. The maximum frequency of the AHB and the high speed APB domains is 72 MHz, while the maximum allowed frequency of the low speed APB domain is 36 MHz.

AHB

**Figure 2.** **Clock tree**

HSI LSE

to APB2 peripherals

SYSCLK

IWDGCLK

to IWDG

LSI

LSI RC

4OkHz

to TIM 15,16,17

If (APB2 prescaler

=1) x1 else x2

PCLK2

LSE

RTCSEL[1:O]

to RTC

RTCCLK

LSE OSC 32.768kHz

/32

OSC32\_IN

OSC32\_OUT

MS19989V5

to USART1

/2

PLLCLK

HSI LSI HSE

SYSCLK

x2

TIM1/8

MCO

Prescaler

ADC

/1,2,4

Main clock output

MCO

to ADCxy (xy = 12, 34)

/1,2,4,6,8,1O,12,16, 32,64,128,256

Prescaler

ADC

/8

FLITFCLK

to Flash programming interface

HSI

SYSCLK

to I2Cx (x = 1,2)

I2SSRC

SYSCLK

to I2Sx (x = 2,3)

I2S\_CKIN

Ext. clock

HSI

USB

prescaler

/1,1.5

USBCLK

to USB interface

/2

HCLK

PLLSRC

PLLMUL

PLL x2,x3,..

x16

SW

HSI PLLCLK

PCLK2

to AHB bus, core, memory and DMA

to cortex System timer FHCLK Cortex free running clock

to APB1 peripherals

HSE

AHB

prescaler

/1,2,..512

SYSCLK

APB1

prescaler

/1,2,4,8,16

PCLK1

/2,/3,...

/16

CSS

If (APB1 prescaler

=1) x1 else x2

PCLK1

to TIM 2,3,4,6,7

OSC\_OUT

OSC\_IN

SYSCLK to U(S)ARTx (x = 2..5)

4-32 MHz HSE OSC

HSI LSE

APB2

prescaler

/1,2,4,8,16



8 MHz HSI RC

## General-purpose input/outputs (GPIOs)

Each of the GPIO pins can be configured by software as output (push-pull or open-drain), as input (with or without pull-up or pull-down) or as peripheral alternate function. Most of the GPIO pins are shared with digital or analog alternate functions. All GPIOs are high current capable except for analog inputs.

The I/Os alternate function configuration can be locked if needed following a specific sequence in order to avoid spurious writing to the I/Os registers.

Fast I/O handling allows I/O toggling up to 36 MHz.

## Direct memory access (DMA)

The flexible general-purpose DMA is able to manage memory-to-memory, peripheral-to- memory and memory-to-peripheral transfers. The DMA controller supports circular buffer management, avoiding the generation of interrupts when the controller reaches the end of the buffer.

Each of the 12 DMA channels is connected to dedicated hardware DMA requests, with software trigger support for each channel. Configuration is done by software and transfer sizes between source and destination are independent.

The DMA can be used with the main peripherals: SPI, I2C, USART, general-purpose timers, DAC and ADC.

## Interrupts and events

#### Nested vectored interrupt controller (NVIC)

The STM32F303xB/STM32F303xC devices embed a nested vectored interrupt controller (NVIC) able to handle up to 66 maskable interrupt channels and 16 priority levels.

The NVIC benefits are the following:

* + - * Closely coupled NVIC gives low latency interrupt processing
      * Interrupt entry vector table address passed directly to the core
      * Closely coupled NVIC core interface
      * Allows early processing of interrupts
      * Processing of late arriving higher priority interrupts
      * Support for tail chaining
      * Processor state automatically saved
      * Interrupt entry restored on interrupt exit with no instruction overhead

The NVIC hardware block provides flexible interrupt management features with minimal interrupt latency.

## Fast analog-to-digital converter (ADC)

four fast analog-to-digital converters 5 MSPS, with selectable resolution between 12 and 6 bit, are embedded in the STM32F303xB/STM32F303xC family devices. The ADCs have up to 39 external channels. Some of the external channels are shared between ADC1&2 and between ADC3&4. Channels can be configured to be either single-ended input or differential input. The ADCs can perform conversions in single-shot or scan modes. In scan mode, automatic conversion is performed on a selected group of analog inputs.

The ADCs have also internal channels: Temperature sensor connected to ADC1 channel 16, VBAT/2 connected to ADC1 channel 17, Voltage reference VREFINT connected to the 4 ADCs channel 18, VOPAMP1 connected to ADC1 channel 15, VOPAMP2 connected to ADC2 channel 17, VREFOPAMP3 connected to ADC3 channel 17 and VREFOPAMP4 connected to ADC4 channel 17.

Additional logic functions embedded in the ADC interface allow:

* Simultaneous sample and hold
* Interleaved sample and hold
* Single-shunt phase current reading techniques.

The ADC can be served by the DMA controller. 3 analog watchdogs per ADC are available.

An analog watchdog feature allows very precise monitoring of the converted voltage of one, some or all selected channels. An interrupt is generated when the converted voltage is outside the programmed thresholds.

The events generated by the general-purpose timers and the advanced-control timers (TIM1 and TIM8) can be internally connected to the ADC start trigger and injection trigger, respectively, to allow the application to synchronize A/D conversion and timers.

#### Temperature sensor

The temperature sensor (TS) generates a voltage VSENSE that varies linearly with temperature.

The temperature sensor is internally connected to the ADC1\_IN16 input channel which is used to convert the sensor output voltage into a digital value.

The sensor provides good linearity but it has to be calibrated to obtain good overall accuracy of the temperature measurement. As the offset of the temperature sensor varies from chip to chip due to process variation, the uncalibrated internal temperature sensor is suitable for applications that detect temperature changes only.

To improve the accuracy of the temperature sensor measurement, each device is individually factory-calibrated by ST. The temperature sensor factory calibration data are stored by ST in the system memory area, accessible in read-only mode.

#### Internal voltage reference (VREFINT)

The internal voltage reference (VREFINT) provides a stable (bandgap) voltage output for the ADC and Comparators. VREFINT is internally connected to the ADCx\_IN18, x=1...4 input channel. The precise voltage of VREFINT is individually measured for each part by ST during production test and stored in the system memory area. It is accessible in read-only mode.

#### VBAT battery voltage monitoring

This embedded hardware feature allows the application to measure the VBAT battery voltage using the internal ADC channel ADC1\_IN17. As the VBAT voltage may be higher than VDDA, and thus outside the ADC input range, the VBAT pin is internally connected to a bridge divider by 2. As a consequence, the converted digital value is half the VBAT voltage.

#### OPAMP reference voltage (VREFOPAMP)

Every OPAMP reference voltage can be measured using a corresponding ADC internal channel: VREFOPAMP1 connected to ADC1 channel 15, VREFOPAMP2 connected to ADC2 channel 17, VREFOPAMP3 connected to ADC3 channel 17, VREFOPAMP4 connected to ADC4 channel 17.

## Digital-to-analog converter (DAC)

Two 12-bit buffered DAC channels can be used to convert digital signals into analog voltage signal outputs. The chosen design structure is composed of integrated resistor strings and an amplifier in inverting configuration.

This digital interface supports the following features:

* Two DAC output channels
* 8-bit or 10-bit monotonic output
* Left or right data alignment in 12-bit mode
* Synchronized update capability
* Noise-wave generation
* Triangular-wave generation
* Dual DAC channel independent or simultaneous conversions
* DMA capability (for each channel)
* External triggers for conversion

## Operational amplifier (OPAMP)

The STM32F303xB/STM32F303xC embeds four operational amplifiers with external or internal follower routing and PGA capability (or even amplifier and filter capability with external components). When an operational amplifier is selected, an external ADC channel is used to enable output measurement.

The operational amplifier features:

* 8.2 MHz bandwidth
* 0.5 mA output capability
* Rail-to-rail input/output
* In PGA mode, the gain can be programmed to be 2, 4, 8 or 16.

## Fast comparators (COMP)

The STM32F303xB/STM32F303xC devices embed seven fast rail-to-rail comparators with programmable reference voltage (internal or external), hysteresis and speed (low speed for low-power) and with selectable output polarity.

The reference voltage can be one of the following:

* External I/O
* DAC output pin
* Internal reference voltage or submultiple (1/4, 1/2, 3/4). Refer to [*Table 28: Embedded*](#_bookmark142)[*internal reference voltage on page 62*](#_bookmark142)for the value and precision of the internal reference voltage.

All comparators can wake up from STOP mode, generate interrupts and breaks for the timers and can be also combined per pair into a window comparator

## Timers and watchdogs

The STM32F303xB/STM32F303xC includes two advanced control timers, up to six general- purpose timers, two basic timers, two watchdog timers and a SysTick timer. The table below compares the features of the advanced control, general purpose and basic timers.

###### Table 5. Timer feature comparison

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Timer type** | **Timer** | **Counter resolution** | **Counter type** | **Prescaler factor** | **DMA**  **request generation** | **Capture/ compare Channels** | **Complementary outputs** |
| Advanced | TIM1, TIM8 | 16-bit | Up, Down, Up/Down | Any integer between 1  and 65536 | Yes | 4 | Yes |
| General- purpose | TIM2 | 32-bit | Up, Down, Up/Down | Any integer between 1  and 65536 | Yes | 4 | No |
| General- purpose | TIM3, TIM4 | 16-bit | Up, Down, Up/Down | Any integer between 1  and 65536 | Yes | 4 | No |
| General- purpose | TIM15 | 16-bit | Up | Any integer between 1  and 65536 | Yes | 2 | 1 |
| General- purpose | TIM16, TIM17 | 16-bit | Up | Any integer between 1  and 65536 | Yes | 1 | 1 |
| Basic | TIM6, TIM7 | 16-bit | Up | Any integer between 1  and 65536 | Yes | 0 | No |

*Note: TIM1/8 can have PLL as clock source, and therefore can be clocked at 144 MHz.*

#### Advanced timers (TIM1, TIM8)

The advanced-control timers (TIM1 and TIM8) can each be seen as a three-phase PWM multiplexed on six channels. They have complementary PWM outputs with programmable inserted dead-times. They can also be seen as complete general-purpose timers. The four independent channels can be used for:

* + - * Input capture
      * Output compare
      * PWM generation (edge or center-aligned modes) with full modulation capability (0- 100%)
      * One-pulse mode output

In debug mode, the advanced-control timer counter can be frozen and the PWM outputs disabled to turn off any power switches driven by these outputs.

Many features are shared with those of the general-purpose TIM timers (described in [*Section 3.17.2*](#_bookmark52)using the same architecture, so the advanced-control timers can work together with the TIM timers via the Timer Link feature for synchronization or event chaining.

#### General-purpose timers (TIM2, TIM3, TIM4, TIM15, TIM16, TIM17)

There are up to six synchronizable general-purpose timers embedded in the STM32F303xB/STM32F303xC (see [*Table 5*](#_bookmark50)for differences). Each general-purpose timer can be used to generate PWM outputs, or act as a simple time base.

* + - * TIM2, 3, and TIM4

These are full-featured general-purpose timers:

* + - * + TIM2 has a 32-bit auto-reload up/downcounter and 32-bit prescaler
        + TIM3 and 4 have 16-bit auto-reload up/downcounters and 16-bit prescalers.

These timers all feature 4 independent channels for input capture/output compare, PWM or one-pulse mode output. They can work together, or with the other general- purpose timers via the Timer Link feature for synchronization or event chaining.

The counters can be frozen in debug mode.

All have independent DMA request generation and support quadrature encoders.

* + - * TIM15, 16 and 17

These three timers general-purpose timers with mid-range features: They have 16-bit auto-reload upcounters and 16-bit prescalers.

* + - * + TIM15 has 2 channels and 1 complementary channel
        + TIM16 and TIM17 have 1 channel and 1 complementary channel

All channels can be used for input capture/output compare, PWM or one-pulse mode output.

The timers can work together via the Timer Link feature for synchronization or event chaining. The timers have independent DMA request generation.

The counters can be frozen in debug mode.

#### Basic timers (TIM6, TIM7)

These timers are mainly used for DAC trigger generation. They can also be used as a generic 16-bit time base.

#### Independent watchdog (IWDG)

The independent watchdog is based on a 12-bit downcounter and 8-bit prescaler. It is clocked from an independent 40 kHz internal RC and as it operates independently from the main clock, it can operate in Stop and Standby modes. It can be used either as a watchdog to reset the device when a problem occurs, or as a free running timer for application timeout management. It is hardware or software configurable through the option bytes. The counter can be frozen in debug mode.

#### Window watchdog (WWDG)

The window watchdog is based on a 7-bit downcounter that can be set as free running. It can be used as a watchdog to reset the device when a problem occurs. It is clocked from the main clock. It has an early warning interrupt capability and the counter can be frozen in debug mode.

#### SysTick timer

This timer is dedicated to real-time operating systems, but could also be used as a standard down counter. It features:

* + - * A 24-bit down counter
      * Autoreload capability
      * Maskable system interrupt generation when the counter reaches 0.
      * Programmable clock source

## Real-time clock (RTC) and backup registers

The RTC and the 16 backup registers are supplied through a switch that takes power from either the VDD supply when present or the VBAT pin. The backup registers are sixteen 32-bit registers used to store 64 bytes of user application data when VDD power is not present.

They are not reset by a system or power reset, or when the device wakes up from Standby mode.

The RTC is an independent BCD timer/counter.It supports the following features:

* Calendar with subsecond, seconds, minutes, hours (12 or 24 format), week day, date, month, year, in BCD (binary-coded decimal) format.
* Reference clock detection: a more precise second source clock (50 or 60 Hz) can be used to enhance the calendar precision.
* Automatic correction for 28, 29 (leap year), 30 and 31 days of the month.
* Two programmable alarms with wake up from Stop and Standby mode capability.
* On-the-fly correction from 1 to 32767 RTC clock pulses. This can be used to synchronize it with a master clock.
* Digital calibration circuit with 1 ppm resolution, to compensate for quartz crystal inaccuracy.
* Three anti-tamper detection pins with programmable filter. The MCU can be woken up from Stopand Standby modes on tamper event detection.
* Timestamp feature which can be used to save the calendar content. This function can be triggered by an event on the timestamp pin, or by a tamper event. The MCU can be woken up from Stop and Standby modes on timestamp event detection.
* 17-bit Auto-reload counter for periodic interrupt with wakeup from STOP/STANDBY capability.

The RTC clock sources can be:

* A 32.768 kHz external crystal
* A resonator or oscillator
* The internal low-power RC oscillator (typical frequency of 40 kHz)
* The high-speed external clock divided by 32.

## Inter-integrated circuit interface (I2C)

Up to two I2C bus interfaces can operate in multimaster and slave modes. They can support standard (up to 100 KHz), fast (up to 400 KHz) and fast mode + (up to 1 MHz) modes.

Both support 7-bit and 10-bit addressing modes, multiple 7-bit slave addresses

(2 addresses, 1 with configurable mask). They also include programmable analog and digital noise filters.

###### Table 6. Comparison of I2C analog and digital filters

|  |  |  |
| --- | --- | --- |
|  | **Analog filter** | **Digital filter** |
| Pulse width of suppressed spikes | 50 ns | Programmable length from 1 to 15 I2C peripheral clocks |
| Benefits | Available in Stop mode | 1. Extra filtering capability vs. standard requirements. 2. Stable length |
| Drawbacks | Variations depending on temperature, voltage, process | Wakeup from Stop on address match is not available when digital filter is enabled. |

In addition, they provide hardware support for SMBUS 2.0 and PMBUS 1.1: ARP capability, Host notify protocol, hardware CRC (PEC) generation/verification, timeouts verifications and ALERT protocol management. They also have a clock domain independent from the CPU clock, allowing the I2Cx (x=1,2) to wake up the MCU from Stop mode on address match.

The I2C interfaces can be served by the DMA controller. Refer to [*Table 7*](#_bookmark62)for the features available in I2C1 and I2C2.

###### Table 7. STM32F303xB/STM32F303xC I2C implementation

|  |  |  |
| --- | --- | --- |
| **I2C features(1)** | **I2C1** | **I2C2** |
| 7-bit addressing mode | X | X |
| 10-bit addressing mode | X | X |
| Standard mode (up to 100 kbit/s) | X | X |
| Fast mode (up to 400 kbit/s) | X | X |
| Fast Mode Plus with 20mA output drive I/Os (up to 1 Mbit/s) | X | X |
| Independent clock | X | X |

**Table 7. STM32F303xB/STM32F303xC I2C implementation (continued)**

|  |  |  |
| --- | --- | --- |
| **I2C features(1)** | **I2C1** | **I2C2** |
| SMBus | X | X |
| Wakeup from STOP | X | X |

**1. X = supported.**

## Universal synchronous/asynchronous receiver transmitter (USART)

The STM32F303xB/STM32F303xC devices have three embedded universal synchronous/asynchronous receiver transmitters (USART1, USART2 and USART3).

The USART interfaces are able to communicate at speeds of up to 9 Mbits/s.

They provide hardware management of the CTS and RTS signals, they support IrDA SIR ENDEC, the multiprocessor communication mode, the single-wire half-duplex communication mode and have LIN Master/Slave capability. The USART interfaces can be served by the DMA controller.

## Universal asynchronous receiver transmitter (UART)

The STM32F303xB/STM32F303xC devices have 2 embedded universal asynchronous receiver transmitters (UART4, and UART5). The UART interfaces support IrDA SIR ENDEC, multiprocessor communication mode and single-wire half-duplex communication mode. The UART4 interface can be served by the DMA controller.

Refer to [*Table 8*](#_bookmark66)for the features available in all U(S)ART interfaces.

###### Table 8. USART features

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **USART modes/features(1)** | **USART1** | **USART2** | **USART3** | **UART4** | **UART5** |
| Hardware flow control for modem | X | X | X | - | - |
| Continuous communication using DMA | X | X | X | X | - |
| Multiprocessor communication | X | X | X | X | X |
| Synchronous mode | X | X | X | - | - |
| Smartcard mode | X | X | X | - | - |
| Single-wire half-duplex communication | X | X | X | X | X |
| IrDA SIR ENDEC block | X | X | X | X | X |
| LIN mode | X | X | X | X | X |
| Dual clock domain and wakeup from Stop mode | X | X | X | X | X |
| Receiver timeout interrupt | X | X | X | X | X |
| Modbus communication | X | X | X | X | X |
| Auto baud rate detection | X | X | X | - | - |
| Driver Enable | X | X | X | - | - |

**1. X = supported.**

## Serial peripheral interface (SPI)/Inter-integrated sound interfaces (I2S)

Up to three SPIs are able to communicate up to 18 Mbits/s in slave and master modes in full-duplex and half-duplex communication modes. The 3-bit prescaler gives 8 master mode frequencies and the frame size is configurable from 4 bits to 16 bits.

Two standard I2S interfaces (multiplexed with SPI2 and SPI3) supporting four different audio standards can operate as master or slave at half-duplex and full duplex communication modes. They can be configured to transfer 16 and 24 or 32 bits with 16-bit or 32-bit data resolution and synchronized by a specific signal. Audio sampling frequency from 8 kHz up to 192 kHz can be set by 8-bit programmable linear prescaler. When operating in master mode it can output a clock for an external audio component at 256 times the sampling frequency.

Refer to [*Table 9*](#_bookmark69)for the features available in SPI1, SPI2 and SPI3.

###### Table 9. STM32F303xB/STM32F303xC SPI/I2S implementation

|  |  |  |  |
| --- | --- | --- | --- |
| **SPI features(1)** | **SPI1** | **SPI2** | **SPI3** |
| Hardware CRC calculation | X | X | X |
| Rx/Tx FIFO | X | X | X |
| NSS pulse mode | X | X | X |
| I2S mode | - | X | X |
| TI mode | X | X | X |

**1. X = supported.**

## Controller area network (CAN)

The CAN is compliant with specifications 2.0A and B (active) with a bit rate up to 1 Mbit/s. It can receive and transmit standard frames with 11-bit identifiers as well as extended frames with 29-bit identifiers. It has three transmit mailboxes, two receive FIFOs with 3 stages and 14 scalable filter banks.

## Universal serial bus (USB)

The STM32F303xB/STM32F303xC devices embed an USB device peripheral compatible with the USB full-speed 12 Mbs. The USB interface implements a full-speed (12 Mbit/s) function interface. It has software-configurable endpoint setting and suspend/resume support. The dedicated 48 MHz clock is generated from the internal main PLL (the clock source must use a HSE crystal oscillator). The USB has a dedicated 512-bytes SRAM memory for data transmission and reception.

## Infrared Transmitter

The STM32F303xB/STM32F303xC devices provide an infrared transmitter solution. The solution is based on internal connections between TIM16 and TIM17 as shown in the figure below.

TIM17 is used to provide the carrier frequency and TIM16 provides the main signal to be sent. The infrared output signal is available on PB9 or PA13.

To generate the infrared remote control signals, TIM16 channel 1 and TIM17 channel 1 must be properly configured to generate correct waveforms. All standard IR pulse modulation modes can be obtained by programming the two timers output compare channels.

**Figure 3. Infrared transmitter**



MSv3O365V1

(for carrier)

OC

TIMER 17

PB9/PA13

(for envelop)

OC

TIMER 16

## Touch sensing controller (TSC)

The STM32F303xB/STM32F303xC devices provide a simple solution for adding capacitive sensing functionality to any application. These devices offer up to 24 capacitive sensing channels distributed over 8 analog I/O groups.

Capacitive sensing technology is able to detect the presence of a finger near a sensor which is protected from direct touch by a dielectric (glass, plastic, ...). The capacitive variation introduced by the finger (or any conductive object) is measured using a proven implementation based on a surface charge transfer acquisition principle. It consists of charging the sensor capacitance and then transferring a part of the accumulated charges into a sampling capacitor until the voltage across this capacitor has reached a specific threshold. To limit the CPU bandwidth usage this acquisition is directly managed by the hardware touch sensing controller and only requires few external components to operate.

The touch sensing controller is fully supported by the STMTouch touch sensing firmware library which is free to use and allows touch sensing functionality to be implemented reliably in the end application.

**Table 10.** **Capacitive sensing GPIOs available on STM32F303xB/STM32F303xC devices**

|  |  |  |
| --- | --- | --- |
| **Group** | **Capacitive sensing signal name** | **Pin name** |
| 1 | TSC\_G1\_IO1 | PA0 |
| TSC\_G1\_IO2 | PA1 |
| TSC\_G1\_IO3 | PA2 |
| TSC\_G1\_IO4 | PA3 |
| 2 | TSC\_G2\_IO1 | PA4 |
| TSC\_G2\_IO2 | PA5 |
| TSC\_G2\_IO3 | PA6 |
| TSC\_G2\_IO4 | PA7 |
| 3 | TSC\_G3\_IO1 | PC5 |
| TSC\_G3\_IO2 | PB0 |
| TSC\_G3\_IO3 | PB1 |
| TSC\_G3\_IO4 | PB2 |
| 4 | TSC\_G4\_IO1 | PA9 |
| TSC\_G4\_IO2 | PA10 |
| TSC\_G4\_IO3 | PA13 |
| TSC\_G4\_IO4 | PA14 |

|  |  |  |
| --- | --- | --- |
| **Group** | **Capacitive sensing signal name** | **Pin name** |
| 5 | TSC\_G5\_IO1 | PB3 |
| TSC\_G5\_IO2 | PB4 |
| TSC\_G5\_IO3 | PB6 |
| TSC\_G5\_IO4 | PB7 |
| 6 | TSC\_G6\_IO1 | PB11 |
| TSC\_G6\_IO2 | PB12 |
| TSC\_G6\_IO3 | PB13 |
| TSC\_G6\_IO4 | PB14 |
| 7 | TSC\_G7\_IO1 | PE2 |
| TSC\_G7\_IO2 | PE3 |
| TSC\_G7\_IO3 | PE4 |
| TSC\_G7\_IO4 | PE5 |
| 8 | TSC\_G8\_IO1 | PD12 |
| TSC\_G8\_IO2 | PD13 |
| TSC\_G8\_IO3 | PD14 |
| TSC\_G8\_IO4 | PD15 |

**Table 11. No. of capacitive sensing channels available on STM32F303xB/STM32F303xC devices**

|  |  |  |  |
| --- | --- | --- | --- |
| **Analog I/O group** | **Number of capacitive sensing channels** | | |
| **STM32F303Vx** | **STM32F303Rx** | **STM32F303Cx** |
| G1 | 3 | 3 | 3 |
| G2 | 3 | 3 | 3 |
| G3 | 3 | 3 | 2 |
| G4 | 3 | 3 | 3 |
| G5 | 3 | 3 | 3 |
| G6 | 3 | 3 | 3 |
| G7 | 3 | 0 | 0 |
| G8 | 3 | 0 | 0 |
| Number of capacitive sensing channels | 24 | 18 | 17 |

## Development support

#### Serial wire JTAG debug port (SWJ-DP)

The ARM SWJ-DP Interface is embedded, and is a combined JTAG and serial wire debug port that enables either a serial wire debug or a JTAG probe to be connected to the target.

The JTAG TMS and TCK pins are shared respectively with SWDIO and SWCLK and a specific sequence on the TMS pin is used to switch between JTAG-DP and SW-DP.

#### Embedded trace macrocell™

The ARM embedded trace macrocell provides a greater visibility of the instruction and data flow inside the CPU core by streaming compressed data at a very high rate from the STM32F303xB/STM32F303xC through a small number of ETM pins to an external hardware trace port analyzer (TPA) device. The TPA is connected to a host computer using a high-speed channel. Real-time instruction and data flow activity can be recorded and then formatted for display on the host computer running debugger software. TPA hardware is commercially available from common development tool vendors. It operates with third party debugger software tools.

# Pinouts and pin description

PA3 PA4 PA5 PA6 PA7 PBO PB1 PB2 PB1O PB11 VSS

VDD

**Figure 4. STM32F303xB/STM32F303xC** **LQFP48 pinout**

VBAT PC13

PC14/OSC32\_IN PC15/OSC32\_OUT

PFO/OSC\_IN PF1/OSC\_OUT

NRST VSSA/VREF-

VDDA PAO PA1

PA2

1

2

3

4

5

6

7

8

9

48 47 46 45 44 43 42 41 4O 39 38 37

36

35

34

33

32

31

LQFP48

1O

11

12

3O

29

28

27

26

25

VDD VSS PA13 PA12 PA11 PA1O PA9 PA8 PB15 PB14 PB13

PB12

13 14 15 16 17 18 19 2O 21 22 23 24

MSv4O448V1

VDD VSS PB9 PB8 BOOTO PB7 PB6 PB5 PB4 PB3 PA15

PA14

PA3 VSS VDD

PA4

PA5 PA6 PA7 PC4 PC5 PBO PB1 PB2 PB1O PB11 VSS VDD

**Figure 5.** **STM32F303xB/STM32F303xC LQFP64 pinout**

VBAT PC13 PC14/OSC32\_IN PC15/OSC32\_OUT

PFO/OSC\_IN

PF1/OSC\_OUT

NRST PCO PC1 PC2 PC3

VSSA/VREF-

VDDA PAO PA1 PA2

VDD VSS PA13

PA12 PA11 PA1O PA9

PA8 PC9

PC8 PC7 PC6 PB15 PB14 PB13 PB12

MS4O449V1

VDD VSS PB9 PB8

BOOTO PB7 PB6 PB5 PB4 PB3 PD2 PC12 PC11 PC1O PA15 PA14

1

2

3

4

5

6

7

8

9

64 63 62 61 6O 59 58 57 56 55 54 53 52 51 5O 49

48

47

46

45

44

43

42

41

LQFP64

1O

11

12

13

14

15

4O

39

38

37

36

35

34

16

17 18 19 2O 21 22 23 24 25 26 27 28 29 3O 31 32

33

PA3 PF4 VDD PA4 PA5 PA6 PA7 PC4 PC5 PBO PB1 PB2 PE7 PE8 PE9 PE1O PE11 PE12 PE13 PE14 PE15 PB1O PB11 VSS VDD

26

27

28

29

3O

31

32

33

34

35

36

37

38

39

4O

41

42

43

44

45

46

47

48

49

5O

**Figure 6.** **STM32F303xB/STM32F303xC LQFP100 pinout**

PE2 PE3 PE4 PE5 PE6 VBAT PC13

PC14/OSC32\_IN PC15/OSC32\_OUT

PF9 PF1O PFO/OSC\_IN PF1/OSC\_OUT

NRST

PCO PC1 PC2 PC3 PF2

VSSA/VREF-

VREF+ VDDA PAO PA1 PA2

1

2

3

4

5

6

7

8

9

1O

11

12

13

14

15

16

17

18

19

2O

21

22

23

24

25

LQFP1OO

75 VDD

74 VSS

73 PF6

72 PA13

71 PA12

7O PA11

69 PA1O

68 PA9

67 PA8

66 PC9

65 PC8

64 PC7

63 PC6

62 PD15

61 PD14

6O PD13

59 PD12

58 PD11

57 PD1O

56 PD9

55 PD8

54 PB15

53 PB14

52 PB13

51 PB12

MS4O45OV1

1OO

99

98

97

96

95

94

93

92

91

9O

89

88

87

86

85

84

83

82

81

8O

79

78

77

76

VDD VSS PE1 PEO PB9 PB8 BOOTO PB7 PB6 PB5 PB4 PB3 PD7 PD6 PD5 PD4 PD3 PD2 PD1 PDO PC12 PC11 PC1O PA15 PA14

**Figure 7.** **STM32F303xB/STM32F303xC WLCSP100 pinout**



9

1O

VDD

VDD

PE5

VDD

PC13

PC14 OSC32IN

PC15 OSC32OUT

NRST

PF9

PF1O

PF1 PFO OSCOUT OSCIN

PC1

PCO

H

PD12

PD11

PD1O

PB15

PE11

PA6

PA5

VSSA PAO

PC3

J

VSS

PB14

PB13

PB12

VDD

PBO

PA4

VREF+

PA1

VDDA

K

VSS

VSS

PB11

PB1O

PB2

PB1

PA7

VDD

VSS

VSS

MSv4O453V1

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 |
| A | VSS | VSS | PC12 | PD2 | PB3 | PB5 | BOOTO | PE1 |
| B | VSS | PA15 | PDO | PD3 | PB4 | PB6 | PEO | VDD |
| C | PF6 | PA14 | PD1 | PD4 | PB7 | PB9 | VSS | PE4 |
| D | PA12 | VDD | PC11 | PD7 | PB8 | PE2 | PE3 | VBAT |
| E | PA1O | PA11 | PA13 | PC1O | PA9 | PE8 | PE6 | PF2 |
| F | PC8 | PC7 | PC9 | PC6 | PA8 | PC5 | PA2 | PE7 |
| G | PD15 | PD14 | PD13 | PD9 | PE12 | PC4 | PA3 | PC2 |

**Table 12. Legend/abbreviations used in the pinout table**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | | **Abbreviation** | **Definition** |
| Pin name | | Unless otherwise specified in brackets below the pin name, the pin function during and after reset is the same as the actual pin name | |
| Pin type | | S | Supply pin |
| I | Input only pin |
| I/O | Input / output pin |
| I/O structure | | FT | 5 V tolerant I/O |
| FTf | 5 V tolerant I/O, FM+ capable |
| TTa | 3.3 V tolerant I/O directly connected to ADC |
| TC | Standard 3.3V I/O |
| B | Dedicated BOOT0 pin |
| RST | Bidirectional reset pin with embedded weak pull-up resistor |
| Notes | | Unless otherwise specified by a note, all I/Os are set as floating inputs during and after reset | |
| Pin functions | Alternate functions | Functions selected through GPIOx\_AFR registers | |
| Additional functions | Functions directly selected/enabled through peripheral registers | |

**Ta****ble 13. STM32F303xB/STM32F303xC pin definitions**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin number** | | | | **Pin name (function after reset)** | **Pin type** | **I/O structure** | **Notes** | **Pin functions** | |
| **WLCSP100** | **LQFP100** | **LQFP64** | **LQFP48** | **Alternate functions** | **Additional functions** |
| D6 | 1 | - | - | PE2 | I/O | FT | (1) | TRACECK, TIM3\_CH1, TSC\_G7\_IO1, EVENTOUT | - |
| D7 | 2 | - | - | PE3 | I/O | FT | (1) | TRACED0, TIM3\_CH2, TSC\_G7\_IO2, EVENTOUT | - |
| C8 | 3 | - | - | PE4 | I/O | FT | (1) | TRACED1, TIM3\_CH3, TSC\_G7\_IO3, EVENTOUT | - |
| B9 | 4 | - | - | PE5 | I/O | FT | (1) | TRACED2, TIM3\_CH4, TSC\_G7\_IO4, EVENTOUT | - |
| E7 | 5 | - | - | PE6 | I/O | FT | (1) | TRACED3, EVENTOUT | WKUP3, RTC\_TAMP3 |
| D8 | 6 | 1 | 1 | VBAT | S | - | - | Backup power supply | |
| C9 | 7 | 2 | 2 | PC13(2) | I/O | TC | - | TIM1\_CH1N | WKUP2, RTC\_TAMP1, RTC\_TS, RTC\_OUT |
| C10 | 8 | 3 | 3 | PC14[(2)](#_bookmark97) OSC32\_IN (PC14) | I/O | TC | - | - | OSC32\_IN |
| D9 | 9 | 4 | 4 | PC15[(2)](#_bookmark97) OSC32\_ OUT (PC15) | I/O | TC | - | - | OSC32\_OUT |
| D10 | 10 | - | - | PF9 | I/O | FT | (1) | TIM15\_CH1, SPI2\_SCK, EVENTOUT | - |
| E10 | 11 | - | - | PF10 | I/O | FT | (1) | TIM15\_CH2, SPI2\_SCK, EVENTOUT | - |
| F10 | 12 | 5 | 5 | PF0- OSC\_IN (PF0) | I/O | FTf | - | TIM1\_CH3N, I2C2\_SDA, | OSC\_IN |
| F9 | 13 | 6 | 6 | PF1- OSC\_OUT (PF1) | I/O | FTf | - | I2C2\_SCL | OSC\_OUT |
| E9 | 14 | 7 | 7 | NRST | I/O | RS T |  | Device reset input / internal reset output (active low) | |
| G10 | 15 | 8 | - | PC0 | I/O | TTa | (1) | EVENTOUT | ADC12\_IN6, COMP7\_INM |
| G9 | 16 | 9 | - | PC1 | I/O | TTa | (1) | EVENTOUT | ADC12\_IN7, COMP7\_INP |
| G8 | 17 | 10 | - | PC2 | I/O | TTa | (1) | COMP7\_OUT, EVENTOUT | ADC12\_IN8 |
| H10 | 18 | 11 | - | PC3 | I/O | TTa | (1) | TIM1\_BKIN2, EVENTOUT | ADC12\_IN9 |
| E8 | 19 | - | - | PF2 | I/O | TTa | (1) | EVENTOUT | ADC12\_IN10 |

**Table 13. STM32F303xB/STM32F303xC pin definitions (continued)**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin number** | | | | **Pin name (function after reset)** | **Pin type** | **I/O structure** | **Notes** | **Pin functions** | |
| **WLCSP100** | **LQFP100** | **LQFP64** | **LQFP48** | **Alternate functions** | **Additional functions** |
| H8 | 20 | 12 | 8 | VSSA/ VREF- | S | - | - | Analog ground/Negative reference voltage | |
| J8 | 21 | - | - | VREF+(3) | S | - | - | Positive reference voltage | |
| J10 | 22 | - | - | VDDA | S | - | - | Analog power supply | |
| - | - | 13 | 9 | VDDA/ VREF+ | S | - | - | Analog power supply/Positive reference voltage | |
| H9 | 23 | 14 | 10 | PA0 | I/O | TTa | - | USART2\_CTS, TIM2\_CH1\_ETR,TIM8\_BKIN, TIM8\_ETR,TSC\_G1\_IO1, COMP1\_OUT, EVENTOUT | ADC1\_IN1, COMP1\_INM, RTC\_ TAMP2, WKUP1, COMP7\_INP |
| J9 | 24 | 15 | 11 | PA1 | I/O | TTa | - | USART2\_RTS\_DE, TIM2\_CH2, TSC\_G1\_IO2, TIM15\_CH1N, RTC\_REFIN, EVENTOUT | ADC1\_IN2, COMP1\_INP, OPAMP1\_VINP, OPAMP3\_VINP |
| F7 | 25 | 16 | 12 | PA2 | I/O | TTa | [(4)](#_bookmark98) | USART2\_TX, TIM2\_CH3, TIM15\_CH1, TSC\_G1\_IO3, COMP2\_OUT, EVENTOUT | ADC1\_IN3, COMP2\_INM, OPAMP1\_VOUT |
| G7 | 26 | 17 | 13 | PA3 | I/O | TTa | - | USART2\_RX, TIM2\_CH4, TIM15\_CH2, TSC\_G1\_IO4, EVENTOUT | ADC1\_IN4, OPAMP1\_VINP, COMP2\_INP, OPAMP1\_VINM |
| - | 27 | 18 | - | PF4 | I/O | TTa | **(1)** | COMP1\_OUT, EVENTOUT | ADC1\_IN5 |
| K8 | 28 | 19 | - | VDD | S | **-** | **-** | - | - |
| J7 | 29 | 20 | 14 | PA4 | I/O | TTa | (4) | SPI1\_NSS, SPI3\_NSS,I2S3\_WS, USART2\_CK, TSC\_G2\_IO1, TIM3\_CH2, EVENTOUT | ADC2\_IN1, DAC1\_OUT1, OPAMP4\_VINP, COMP1\_INM, COMP2\_INM, COMP3\_INM, COMP4\_INM, COMP5\_INM, COMP6\_INM, COMP7\_INM |
| H7 | 30 | 21 | 15 | PA5 | I/O | TTa | [(4)](#_bookmark98) | SPI1\_SCK, TIM2\_CH1\_ETR, TSC\_G2\_IO2, EVENTOUT | ADC2\_IN2, DAC1\_OUT2 OPAMP1\_VINP, OPAMP2\_VINM, OPAMP3\_VINP COMP1\_INM, COMP2\_INM, COMP3\_INM, COMP4\_INM, COMP5\_INM, COMP6\_INM, COMP7\_INM |

**Table 13. STM32F303xB/STM32F303xC pin definitions (continued)**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin number** | | | | **Pin name (function after reset)** | **Pin type** | **I/O structure** | **Notes** | **Pin functions** | |
| **WLCSP100** | **LQFP100** | **LQFP64** | **LQFP48** | **Alternate functions** | **Additional functions** |
| H6 | 31 | 22 | 16 | PA6 | I/O | TTa | [(4)](#_bookmark98) | SPI1\_MISO, TIM3\_CH1, TIM8\_BKIN, TIM1\_BKIN, TIM16\_CH1, COMP1\_OUT, TSC\_G2\_IO3, EVENTOUT | ADC2\_IN3, OPAMP2\_VOUT |
| K7 | 32 | 23 | 17 | PA7 | I/O | TTa | - | SPI1\_MOSI, TIM3\_CH2, TIM17\_CH1, TIM1\_CH1N, TIM8\_CH1N, TSC\_G2\_IO4, COMP2\_OUT, EVENTOUT | ADC2\_IN4, COMP2\_INP, OPAMP2\_VINP, OPAMP1\_VINP |
| G6 | 33 | 24 | - | PC4 | I/O | TTa | **(1)** | USART1\_TX, EVENTOUT | ADC2\_IN5 |
| F6 | 34 | 25 | - | PC5 | I/O | TTa | **(1)** | USART1\_RX, TSC\_G3\_IO1, EVENTOUT | ADC2\_IN11, OPAMP2\_VINM, OPAMP1\_VINM |
| J6 | 35 | 26 | 18 | PB0 | I/O | TTa | - | TIM3\_CH3, TIM1\_CH2N, TIM8\_CH2N,TSC\_G3\_IO2, EVENTOUT | ADC3\_IN12, COMP4\_INP, OPAMP3\_VINP, OPAMP2\_VINP |
| K6 | 36 | 27 | 19 | PB1 | I/O | TTa | [(4)](#_bookmark98) | TIM3\_CH4, TIM1\_CH3N, TIM8\_CH3N, COMP4\_OUT, TSC\_G3\_IO3, EVENTOUT | ADC3\_IN1, OPAMP3\_VOUT- |
| K5 | 37 | 28 | 20 | PB2 | I/O | TTa | - | TSC\_G3\_IO4, EVENTOUT | ADC2\_IN12, COMP4\_INM, OPAMP3\_VINM |
| F8 | 38 | - | - | PE7 | I/O | TTa | **(1)** | TIM1\_ETR, EVENTOUT | ADC3\_IN13, COMP4\_INP |
| E6 | 39 | - | - | PE8 | I/O | TTa | **(1)** | TIM1\_CH1N, EVENTOUT | COMP4\_INM, ADC34\_IN6 |
| - | 40 | - | - | PE9 | I/O | TTa | **(1)** | TIM1\_CH1, EVENTOUT | ADC3\_IN2 |
| - | 41 | - | - | PE10 | I/O | TTa | **(1)** | TIM1\_CH2N, EVENTOUT | ADC3\_IN14 |
| H5 | 42 | - | - | PE11 | I/O | TTa | **(1)** | TIM1\_CH2, EVENTOUT | ADC3\_IN15 |
| G5 | 43 | - | - | PE12 | I/O | TTa | **(1)** | TIM1\_CH3N, EVENTOUT | ADC3\_IN16 |
| - | 44 | - | - | PE13 | I/O | TTa | **(1)** | TIM1\_CH3, EVENTOUT | ADC3\_IN3 |
| - | 45 | - | - | PE14 | I/O | TTa | **(1)** | TIM1\_CH4, TIM1\_BKIN2, EVENTOUT | ADC4\_IN1 |
| - | 46 | - | - | PE15 | I/O | TTa | **(1)** | USART3\_RX, TIM1\_BKIN, EVENTOUT | ADC4\_IN2 |
| K4 | 47 | 29 | 21 | PB10 | I/O | TTa | - | USART3\_TX, TIM2\_CH3, TSC\_SYNC, EVENTOUT | COMP5\_INM, OPAMP4\_VINM, OPAMP3\_VINM |
| K3 | 48 | 30 | 22 | PB11 | I/O | TTa | - | USART3\_RX, TIM2\_CH4, TSC\_G6\_IO1, EVENTOUT | COMP6\_INP, OPAMP4\_VINP |

**Table 13. STM32F303xB/STM32F303xC pin definitions (continued)**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin number** | | | | **Pin name (function after reset)** | **Pin type** | **I/O structure** | **Notes** | **Pin functions** | |
| **WLCSP100** | **LQFP100** | **LQFP64** | **LQFP48** | **Alternate functions** | **Additional functions** |
| K1,  J1, K2 | 49 | 31 | 23 | VSS | S | - | - | Digital ground | |
| J5 | 50 | 32 | 24 | VDD | S | - | - | Digital power supply | |
| J4 | 51 | 33 | 25 | PB12 | I/O | TTa | [(4)](#_bookmark98) | SPI2\_NSS,I2S2\_WS,I2C2\_S MBA, USART3\_CK, TIM1\_BKIN, TSC\_G6\_IO2, EVENTOUT | ADC4\_IN3, COMP3\_INM, OPAMP4\_VOUT |
| J3 | 52 | 34 | 26 | PB13 | I/O | TTa | - | SPI2\_SCK,I2S2\_CK,USART 3\_CTS, TIM1\_CH1N, TSC\_G6\_IO3, EVENTOUT | ADC3\_IN5, COMP5\_INP, OPAMP4\_VINP, OPAMP3\_VINP |
| J2 | 53 | 35 | 27 | PB14 | I/O | TTa | - | SPI2\_MISO,I2S2ext\_SD, USART3\_RTS\_DE, TIM1\_CH2N, TIM15\_CH1,  TSC\_G6\_IO4, EVENTOUT | COMP3\_INP, ADC4\_IN4, OPAMP2\_VINP |
| H4 | 54 | 36 | 28 | PB15 | I/O | TTa | - | SPI2\_MOSI, I2S2\_SD, TIM1\_CH3N, RTC\_REFIN, TIM15\_CH1N, TIM15\_CH2, EVENTOUT | ADC4\_IN5, COMP6\_INM |
| - | 55 | - | - | PD8 | I/O | TTa | **(1)** | USART3\_TX, EVENTOUT | ADC4\_IN12, OPAMP4\_VINM |
| G4 | 56 | - | - | PD9 | I/O | TTa | **(1)** | USART3\_RX, EVENTOUT | ADC4\_IN13 |
| H3 | 57 | - | - | PD10 | I/O | TTa | **(1)** | USART3\_CK, EVENTOUT | ADC34\_IN7, COMP6\_INM |
| H2 | 58 | - | - | PD11 | I/O | TTa | **(1)** | USART3\_CTS, EVENTOUT | ADC34\_IN8, COMP6\_INP, OPAMP4\_VINP |
| H1 | 59 | - | - | PD12 | I/O | TTa | **(1)** | USART3\_RTS\_DE, TIM4\_CH1, TSC\_G8\_IO1, EVENTOUT | ADC34\_IN9, COMP5\_INP |
| G3 | 60 | - | - | PD13 | I/O | TTa | **(1)** | TIM4\_CH2, TSC\_G8\_IO2, EVENTOUT | ADC34\_IN10, COMP5\_INM |
| G2 | 61 | - | - | PD14 | I/O | TTa | **(1)** | TIM4\_CH3, TSC\_G8\_IO3, EVENTOUT | COMP3\_INP, ADC34\_IN11, OPAMP2\_VINP |
| G1 | 62 | - | - | PD15 | I/O | TTa | **(1)** | SPI2\_NSS, TIM4\_CH4, TSC\_G8\_IO4, EVENTOUT | COMP3\_INM |
| F4 | 63 | 37 | - | PC6 | I/O | FT | **(1)** | I2S2\_MCK, COMP6\_OUT, TIM8\_CH1, TIM3\_CH1, EVENTOUT | - |

**Table 13. STM32F303xB/STM32F303xC pin definitions (continued)**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin number** | | | | **Pin name (function after reset)** | **Pin type** | **I/O structure** | **Notes** | **Pin functions** | |
| **WLCSP100** | **LQFP100** | **LQFP64** | **LQFP48** | **Alternate functions** | **Additional functions** |
| F2 | 64 | 38 | - | PC7 | I/O | FT | **(1)** | I2S3\_MCK, TIM8\_CH2, TIM3\_CH2, COMP5\_OUT, EVENTOUT | - |
| F1 | 65 | 39 | - | PC8 | I/O | FT | **(1)** | TIM8\_CH3, TIM3\_CH3, COMP3\_OUT, EVENTOUT | - |
| F3 | 66 | 40 | - | PC9 | I/O | FT | **(1)** | TIM8\_CH4, TIM8\_BKIN2,TIM3\_CH4, I2S\_CKIN, EVENTOUT | - |
| F5 | 67 | 41 | 29 | PA8 | I/O | FT | - | I2C2\_SMBA,I2S2\_MCK, USART1\_CK, TIM1\_CH1, TIM4\_ETR, MCO, COMP3\_OUT, EVENTOUT | - |
| E5 | 68 | 42 | 30 | PA9 | I/O | FTf | - | I2C2\_SCL,I2S3\_MCK, USART1\_TX, TIM1\_CH2, TIM2\_CH3, TIM15\_BKIN, TSC\_G4\_IO1, COMP5\_OUT, EVENTOUT | - |
| E1 | 69 | 43 | 31 | PA10 | I/O | FTf | - | I2C2\_SDA, USART1\_RX, TIM1\_CH3, TIM2\_CH4, TIM8\_BKIN, TIM17\_BKIN, TSC\_G4\_IO2, COMP6\_OUT, EVENTOUT | - |
| E2 | 70 | 44 | 32 | PA11 | I/O | FT | - | USART1\_CTS, USB\_DM, CAN\_RX, TIM1\_CH1N, TIM1\_CH4, TIM1\_BKIN2, TIM4\_CH1, COMP1\_OUT, EVENTOUT | - |
| D1 | 71 | 45 | 33 | PA12 | I/O | FT | - | USART1\_RTS\_DE, USB\_DP, CAN\_TX, TIM1\_CH2N, TIM1\_ETR, TIM4\_CH2, TIM16\_CH1, COMP2\_OUT, EVENTOUT | - |
| E3 | 72 | 46 | 34 | PA13 | I/O | FT | - | USART3\_CTS, TIM4\_CH3, TIM16\_CH1N, TSC\_G4\_IO3, IR\_OUT, SWDIO-JTMS, EVENTOUT | - |
| C1 | 73 | - | - | PF6 | I/O | FTf | **(1)** | I2C2\_SCL, USART3\_RTS\_DE, TIM4\_CH4, EVENTOUT | - |

**Table 13. STM32F303xB/STM32F303xC pin definitions (continued)**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin number** | | | | **Pin name (function after reset)** | **Pin type** | **I/O structure** | **Notes** | **Pin functions** | |
| **WLCSP100** | **LQFP100** | **LQFP64** | **LQFP48** | **Alternate functions** | **Additional functions** |
| A1,  A2, B1 | 74 | 47 | 35 | VSS | S | - | - | Ground | |
| D2 | 75 | 48 | 36 | VDD | S | - | - | Digital power supply | |
| C2 | 76 | 49 | 37 | PA14 | I/O | FTf | - | I2C1\_SDA, USART2\_TX, TIM8\_CH2,TIM1\_BKIN, TSC\_G4\_IO4, SWCLK-JTCK, EVENTOUT | - |
| B2 | 77 | 50 | 38 | PA15 | I/O | FTf | - | I2C1\_SCL, SPI1\_NSS, SPI3\_NSS, I2S3\_WS, JTDI, USART2\_RX, TIM1\_BKIN, TIM2\_CH1\_ETR, TIM8\_CH1, EVENTOUT | - |
| E4 | 78 | 51 | - | PC10 | I/O | FT | **(1)** | SPI3\_SCK, I2S3\_CK, USART3\_TX, UART4\_TX, TIM8\_CH1N, EVENTOUT | - |
| D3 | 79 | 52 | - | PC11 | I/O | FT | **(1)** | SPI3\_MISO, I2S3ext\_SD, USART3\_RX, UART4\_RX, TIM8\_CH2N, EVENTOUT | - |
| A3 | 80 | 53 | - | PC12 | I/O | FT | **(1)** | SPI3\_MOSI, I2S3\_SD, USART3\_CK, UART5\_TX, TIM8\_CH3N, EVENTOUT | - |
| B3 | 81 | - | - | PD0 | I/O | FT | **(1)** | CAN\_RX, EVENTOUT | - |
| C3 | 82 | - | - | PD1 | I/O | FT | **(1)** | CAN\_TX, TIM8\_CH4, TIM8\_BKIN2,EVENTOUT | - |
| A4 | 83 | 54 | - | PD2 | I/O | FT | **(1)** | UART5\_RX, TIM3\_ETR, TIM8\_BKIN, EVENTOUT | - |
| B4 | 84 | - | - | PD3 | I/O | FT | **(1)** | USART2\_CTS, TIM2\_CH1\_ETR, EVENTOUT | - |
| C4 | 85 | - | - | PD4 | I/O | FT | **(1)** | USART2\_RTS\_DE, TIM2\_CH2, EVENTOUT | - |
| - | 86 | - | - | PD5 | I/O | FT | **(1)** | USART2\_TX, EVENTOUT | - |
| - | 87 | - | - | PD6 | I/O | FT | **(1)** | USART2\_RX, TIM2\_CH4, EVENTOUT | - |
| D4 | 88 | - | - | PD7 | I/O | FT | **(1)** | USART2\_CK, TIM2\_CH3, EVENTOUT | - |

**Table 13. STM32F303xB/STM32F303xC pin definitions (continued)**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin number** | | | | **Pin name (function after reset)** | **Pin type** | **I/O structure** | **Notes** | **Pin functions** | |
| **WLCSP100** | **LQFP100** | **LQFP64** | **LQFP48** | **Alternate functions** | **Additional functions** |
| A5 | 89 | 55 | 39 | PB3 | I/O | FT | - | SPI3\_SCK, I2S3\_CK, SPI1\_SCK, USART2\_TX, TIM2\_CH2, TIM3\_ETR, TIM4\_ETR, TIM8\_CH1N, TSC\_G5\_IO1, JTDO- TRACESWO, EVENTOUT | - |
| B5 | 90 | 56 | 40 | PB4 | I/O | FT | - | SPI3\_MISO, I2S3ext\_SD, SPI1\_MISO, USART2\_RX, TIM3\_CH1, TIM16\_CH1, TIM17\_BKIN, TIM8\_CH2N, TSC\_G5\_IO2, NJTRST, EVENTOUT | - |
| A6 | 91 | 57 | 41 | PB5 | I/O | FT | - | SPI3\_MOSI, SPI1\_MOSI, I2S3\_SD, I2C1\_SMBA, USART2\_CK, TIM16\_BKIN, TIM3\_CH2, TIM8\_CH3N, TIM17\_CH1, EVENTOUT | - |
| B6 | 92 | 58 | 42 | PB6 | I/O | FTf | - | I2C1\_SCL, USART1\_TX, TIM16\_CH1N, TIM4\_CH1, TIM8\_CH1,TSC\_G5\_IO3, TIM8\_ETR, TIM8\_BKIN2, EVENTOUT | - |
| C5 | 93 | 59 | 43 | PB7 | I/O | FTf | - | I2C1\_SDA, USART1\_RX, TIM3\_CH4, TIM4\_CH2, TIM17\_CH1N, TIM8\_BKIN, TSC\_G5\_IO4, EVENTOUT | - |
| A7 | 94 | 60 | 44 | BOOT0 | I | B | - | Boot memory selection | |
| D5 | 95 | 61 | 45 | PB8 | I/O | FTf | - | I2C1\_SCL, CAN\_RX, TIM16\_CH1, TIM4\_CH3, TIM8\_CH2, TIM1\_BKIN, TSC\_SYNC, COMP1\_OUT, EVENTOUT | - |
| C6 | 96 | 62 | 46 | PB9 | I/O | FTf | - | I2C1\_SDA, CAN\_TX, TIM17\_CH1, TIM4\_CH4, TIM8\_CH3, IR\_OUT, COMP2\_OUT, EVENTOUT | - |
| B7 | 97 | - | - | PE0 | I/O | FT | **(1)** | USART1\_TX, TIM4\_ETR, TIM16\_CH1, EVENTOUT | - |
| A8 | 98 | - | - | PE1 | I/O | FT | **(1)** | USART1\_RX, TIM17\_CH1, EVENTOUT | - |

**Table 13. STM32F303xB/STM32F303xC pin definitions (continued)**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin number** | | | | **Pin name (function after reset)** | **Pin type** | **I/O structure** | **Notes** | **Pin functions** | |
| **WLCSP100** | **LQFP100** | **LQFP64** | **LQFP48** | **Alternate functions** | **Additional functions** |
| C7 | 99 | 63 | 47 | VSS | S | - | - | Ground | |
| A10, B10 | 100 | 64 | 48 | VDD | S | - | - | Digital power supply | |

1. Function availability depends on the chosen device.

When using the small packages (48 and 64 pin packages), the GPIO pins which are not present on these packages, must not be configured in analog mode.

1. PC13, PC14 and PC15 are supplied through the power switch. Since the switch sinks only a limited amount of current (3 mA), the use of GPIO PC13 to PC15 in output mode is limited:
   * The speed should not exceed 2 MHz with a maximum load of 30 pF
   * These GPIOs must not be used as current sources (e.g. to drive an LED).

After the first backup domain power-up, PC13, PC14 and PC15 operate as GPIOs. Their function then depends on the content of the Backup registers which is not reset by the main reset. For details on how to manage these GPIOs, refer to the Battery backup domain and BKP register description sections in the RM0316 reference manual.

1. The VREF+ functionality is available only on the 100 pin package. On the 64-pin and 48-pin packages, the VREF+ is internally connected to VDDA.
2. These GPIOs offer a reduced touch sensing sensitivity. It is thus recommended to use them as sampling capacitor I/O.

**Table 14. Alternate functions for port A**



**Pinouts and pin description**

**STM32F303xB STM32F303xC**

44/134

DocID023353 Rev 12

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Port & Pin**  **Name** | **AF0** | **AF1** | **AF2** | **AF3** | **AF4** | **AF5** | **AF6** | **AF7** | **AF8** | **AF9** | **AF10** | **AF11** | **AF12** | **AF14** | **AF15** |
| PA0 | - | TIM2\_ CH1\_ ETR | - | TSC\_ G1\_IO1 | - | - | - | USART2\_ CTS | COMP1  \_OUT | TIM8\_ BKIN | TIM8\_ ETR | - | - | - | EVENT OUT |
| PA1 | RTC\_ REFIN | TIM2\_ CH2 | - | TSC\_ G1\_IO2 | - | - | - | USART2\_ RTS\_DE |  | TIM15\_ CH1N | - | - | - | - | EVENT OUT |
| PA2 | - | TIM2\_ CH3 | - | TSC\_ G1\_IO3 | - | - | - | USART2\_ TX | COMP2  \_OUT | TIM15\_ CH1 | - | - | - | - | EVENT OUT |
| PA3 | - | TIM2\_ CH4 | - | TSC\_ G1\_IO4 | - | - | - | USART2\_ RX | - | TIM15\_ CH2 | - | - | - | - | EVENT OUT |
| PA4 | - | - | TIM3\_ CH2 | TSC\_ G2\_IO1 | - | SPI1\_ NSS | SPI3\_NSS, I2S3\_WS | USART2\_ CK | - | - | - | - | - | - | EVENT OUT |
| PA5 | - | TIM2\_ CH1\_ ETR | - | TSC\_ G2\_IO2 | - | SPI1\_ SCK | - | - | - | - | - | - | - | - | EVENT OUT |
| PA6 | - | TIM16\_ CH1 | TIM3\_ CH1 | TSC\_ G2\_IO3 | TIM8\_ BKIN | SPI1\_ MISO | TIM1\_BKIN | - | COMP1  \_OUT | - | - | - | - | - | EVENT OUT |
| PA7 | - | TIM17\_ CH1 | TIM3\_ CH2 | TSC\_ G2\_IO4 | TIM8\_ CH1N | SPI1\_ MOSI | TIM1\_CH1N | - | COMP2  \_OUT | - | - | - | - | - | EVENT OUT |
| PA8 | MCO | - | - | - | I2C2\_ SMBA | I2S2\_ MCK | TIM1\_CH1 | USART1\_ CK | COMP3  \_OUT | - | TIM4\_ ETR | - | - | - | EVENT OUT |
| PA9 | - | - | - | TSC\_ G4\_IO1 | I2C2\_ SCL | I2S3\_ MCK | TIM1\_CH2 | USART1\_ TX | COMP5  \_OUT | TIM15\_ BKIN | TIM2\_ CH3 | - | - | - | EVENT OUT |
| PA10 | - | TIM17\_ BKIN | - | TSC\_ G4\_IO2 | I2C2\_ SDA | - | TIM1\_CH3 | USART1\_ RX | COMP6  \_OUT | - | TIM2\_ CH4 | TIM8\_BKIN | - | - | EVENT OUT |
| PA11 | - | - | - | - | - | - | TIM1\_CH1N | USART1\_ CTS | COMP1  \_OUT | CAN\_RX | TIM4\_ CH1 | TIM1\_CH4 | TIM1\_ BKIN2 | USB\_ DM | EVENT OUT |

**Table 14. Alternate functions for port A (continued)**



**STM32F303xB STM32F303xC**

**Pinouts and pin description**

DocID023353 Rev 12

45/134

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Port & Pin**  **Name** | **AF0** | **AF1** | **AF2** | **AF3** | **AF4** | **AF5** | **AF6** | **AF7** | **AF8** | **AF9** | **AF10** | **AF11** | **AF12** | **AF14** | **AF15** |
| PA12 | - | TIM16\_ CH1 | - | - | - | - | TIM1\_CH2N | USART1\_ RTS\_DE | COMP2  \_OUT | CAN\_TX | TIM4\_ CH2 | TIM1\_ETR | - | USB\_ DP | EVENT OUT |
| PA13 | SWDIO  -JTMS | TIM16\_ CH1N | - | TSC\_ G4\_IO3 | - | IR\_ OUT | - | USART3\_ CTS | - | - | TIM4\_ CH3 | - | - | - | EVENT OUT |
| PA14 | SWCLK  -JTCK | - | - | TSC\_ G4\_IO4 | I2C1\_ SDA | TIM8\_ CH2 | TIM1\_BKIN | USART2\_ TX | - | - | - | - | - | - | EVENT OUT |
| PA15 | JTDI | TIM2\_ CH1\_ ETR | TIM8\_ CH1 | - | I2C1\_ SCL | SPI1\_ NSS | SPI3\_NSS, I2S3\_WS | USART2\_ RX | - | TIM1\_ BKIN | - | - | - | - | EVENT OUT |

**Table 15. Alternate functions for port B**



**Pinouts and pin description**

**STM32F303xB STM32F303xC**

46/134

DocID023353 Rev 12

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Port & Pin**  **Name** | **AF0** | **AF1** | **AF2** | **AF3** | **AF4** | **AF5** | **AF6** | **AF7** | **AF8** | **AF9** | **AF10** | **AF12** | **AF15** |
| PB0 | - | - | TIM3\_ CH3 | TSC\_ G3\_IO2 | TIM8\_ CH2N | - | TIM1\_CH2N | - | - | - | - | - | EVENT OUT |
| PB1 | - | - | TIM3\_ CH4 | TSC\_ G3\_IO3 | TIM8\_ CH3N | - | TIM1\_CH3N | - | COMP4\_ OUT | - | - | - | EVENT OUT |
| PB2 | - | - | - | TSC\_ G3\_IO4 | - | - | - | - | - | - | - | - | EVENT OUT |
| PB3 | JTDO- TRACES WO | TIM2\_ CH2 | TIM4\_ ETR | TSC\_ G5\_IO1 | TIM8\_ CH1N | SPI1\_ SCK | SPI3\_SCK, I2S3\_CK | USART2\_ TX | - | - | TIM3\_ ETR | - | EVENT OUT |
| PB4 | NJTRST | TIM16\_ CH1 | TIM3\_ CH1 | TSC\_ G5\_IO2 | TIM8\_ CH2N | SPI1\_ MISO | SPI3\_MISO,  I2S3ext\_SD | USART2\_ RX | - | - | TIM17\_ BKIN | - | EVENT OUT |
| PB5 | - | TIM16\_ BKIN | TIM3\_ CH2 | TIM8\_ CH3N | I2C1\_ SMBA | SPI1\_ MOSI | SPI3\_MOSI, I2S3\_SD | USART2\_ CK | - | - | TIM17\_ CH1 | - | EVENT OUT |
| PB6 | - | TIM16\_ CH1N | TIM4\_ CH1 | TSC\_ G5\_IO3 | I2C1\_SCL | TIM8\_CH1 | TIM8\_ ETR | USART1\_ TX | - | - | TIM8\_ BKIN2 | - | EVENT OUT |
| PB7 | - | TIM17\_ CH1N | TIM4\_ CH2 | TSC\_ G5\_IO4 | I2C1\_ SDA | TIM8\_ BKIN | - | USART1\_ RX | - | - | TIM3\_ CH4 | - | EVENT OUT |
| PB8 | - | TIM16\_ CH1 | TIM4\_ CH3 | TSC\_ SYNC | I2C1\_SCL | - | - | - | COMP1\_ OUT | CAN\_RX | TIM8\_ CH2 | TIM1\_ BKIN | EVENT OUT |
| PB9 | - | TIM17\_ CH1 | TIM4\_ CH4 |  | I2C1\_ SDA | - | IR\_OUT | - | COMP2\_ OUT | CAN\_TX | TIM8\_ CH3 | - | EVENT OUT |
| PB10 | - | TIM2\_ CH3 | - | TSC\_ SYNC | - | - | - | USART3\_ TX | - | - | - | - | EVENT OUT |
| PB11 | - | TIM2\_ CH4 | - | TSC\_ G6\_IO1 | - | - | - | USART3\_ RX | - | - | - | - | EVENT OUT |
| PB12 | - | - | - | TSC\_ G6\_IO2 | I2C2\_ SMBA | SPI2\_NSS, I2S2\_WS | TIM1\_ BKIN | USART3\_ CK | - | - | - | - | EVENT OUT |

**Table 15. Alternate functions for port B (continued)**



**STM32F303xB STM32F303xC**

**Pinouts and pin description**

DocID023353 Rev 12

47/134

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Port & Pin**  **Name** | **AF0** | **AF1** | **AF2** | **AF3** | **AF4** | **AF5** | **AF6** | **AF7** | **AF8** | **AF9** | **AF10** | **AF12** | **AF15** |
| PB13 | - | - | - | TSC\_ G6\_IO3 | - | SPI2\_SCK, I2S2\_CK | TIM1\_ CH1N | USART3\_ CTS | - | - | - | - | EVENT OUT |
| PB14 | - | TIM15\_ CH1 | - | TSC\_ G6\_IO4 | - | SPI2\_MISO,  I2S2ext\_SD | TIM1\_ CH2N | USART3\_ RTS\_DE | - | - | - | - | EVENT OUT |
| PB15 | RTC\_ REFIN | TIM15\_ CH2 | TIM15\_ CH1N | - | TIM1\_ CH3N | SPI2\_MOSI, I2S2\_SD | - | - | - | - | - | - | EVENT OUT |

**Table 16. Alternate functions for port C**



**Pinouts and pin description**

**STM32F303xB STM32F303xC**

48/134

DocID023353 Rev 12

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Port & Pin Name** | **AF1** | **AF2** | **AF3** | **AF4** | **AF5** | **AF6** | **AF7** |
| PC0 | EVENTOUT | - | - | - | - | - | - |
| PC1 | EVENTOUT | - | - | - | - | - | - |
| PC2 | EVENTOUT | - | COMP7\_OUT | - | - | - | - |
| PC3 | EVENTOUT | - | - | - | - | TIM1\_BKIN2 | - |
| PC4 | EVENTOUT | - | - | - | - | - | USART1\_TX |
| PC5 | EVENTOUT | - | TSC\_G3\_IO1 | - | - | - | USART1\_RX |
| PC6 | EVENTOUT | TIM3\_CH1 | - | TIM8\_CH1 | - | I2S2\_MCK | COMP6\_OUT |
| PC7 | EVENTOUT | TIM3\_CH2 | - | TIM8\_CH2 | - | I2S3\_MCK | COMP5\_OUT |
| PC8 | EVENTOUT | TIM3\_CH3 | - | TIM8\_CH3 | - | - | COMP3\_OUT |
| PC9 | EVENTOUT | TIM3\_CH4 | - | TIM8\_CH4 | I2S\_CKIN | TIM8\_BKIN2 | - |
| PC10 | EVENTOUT | - | - | TIM8\_CH1N | UART4\_TX | SPI3\_SCK, I2S3\_CK | USART3\_TX |
| PC11 | EVENTOUT | - | - | TIM8\_CH2N | UART4\_RX | SPI3\_MISO, I2S3ext\_SD | USART3\_RX |
| PC12 | EVENTOUT | - | - | TIM8\_CH3N | UART5\_TX | SPI3\_MOSI, I2S3\_SD | USART3\_CK |
| PC13 | - | - | - | TIM1\_CH1N | - | - | - |
| PC14 | - | - | - | - | - | - | - |
| PC15 | - | - | - | - | - | - | - |

**Table 17. Alternate functions for port D**



**STM32F303xB STM32F303xC**

**Pinouts and pin description**

DocID023353 Rev 12

49/134

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Port & Pin Name** | **AF1** | **AF2** | **AF3** | **AF4** | **AF5** | **AF6** | **AF7** |
| PD0 | EVENTOUT | - | - | - | - | - | CAN\_RX |
| PD1 | EVENTOUT | - | - | TIM8\_CH4 | - | TIM8\_BKIN2 | CAN\_TX |
| PD2 | EVENTOUT | TIM3\_ETR | - | TIM8\_BKIN | UART5\_RX | - | - |
| PD3 | EVENTOUT | TIM2\_CH1\_ETR | - | - | - | - | USART2\_CTS |
| PD4 | EVENTOUT | TIM2\_CH2 | - | - | - | - | USART2\_RTS\_DE |
| PD5 | EVENTOUT | - | - | - | - | - | USART2\_TX |
| PD6 | EVENTOUT | TIM2\_CH4 | - | - | - | - | USART2\_RX |
| PD7 | EVENTOUT | TIM2\_CH3 | - | - | - | - | USART2\_CK |
| PD8 | EVENTOUT | - | - | - | - | - | USART3\_TX |
| PD9 | EVENTOUT | - | - | - | - | - | USART3\_RX |
| PD10 | EVENTOUT | - | - | - | - | - | USART3\_CK |
| PD11 | EVENTOUT | - | - | - | - | - | USART3\_CTS |
| PD12 | EVENTOUT | TIM4\_CH1 | TSC\_G8\_IO1 | - | - | - | USART3\_RTS\_DE |
| PD13 | EVENTOUT | TIM4\_CH2 | TSC\_G8\_IO2 | - | - | - | - |
| PD14 | EVENTOUT | TIM4\_CH3 | TSC\_G8\_IO3 | - | - | - | - |
| PD15 | EVENTOUT | TIM4\_CH4 | TSC\_G8\_IO4 | - | - | SPI2\_NSS | - |

**Table 18. Alternate functions for port E**



**Pinouts and pin description**

**STM32F303xB STM32F303xC**

50/134

DocID023353 Rev 12

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Port & Pin Name** | **AF0** | **AF1** | **AF2** | **AF3** | **AF4** | **AF6** | **AF7** |
| PE0 | - | EVENTOUT | TIM4\_ETR | - | TIM16\_CH1 | - | USART1\_TX |
| PE1 | - | EVENTOUT | - | - | TIM17\_CH1 | - | USART1\_RX |
| PE2 | TRACECK | EVENTOUT | TIM3\_CH1 | TSC\_G7\_IO1 | - | - | - |
| PE3 | TRACED0 | EVENTOUT | TIM3\_CH2 | TSC\_G7\_IO2 | - | - | - |
| PE4 | TRACED1 | EVENTOUT | TIM3\_CH3 | TSC\_G7\_IO3 | - | - | - |
| PE5 | TRACED2 | EVENTOUT | TIM3\_CH4 | TSC\_G7\_IO4 | - | - | - |
| PE6 | TRACED3 | EVENTOUT |  | - | - | - | - |
| PE7 | - | EVENTOUT | TIM1\_ETR | - | - | - | - |
| PE8 | - | EVENTOUT | TIM1\_CH1N | - | - | - | - |
| PE9 | - | EVENTOUT | TIM1\_CH1 | - | - | - | - |
| PE10 | - | EVENTOUT | TIM1\_CH2N | - | - | - | - |
| PE11 | - | EVENTOUT | TIM1\_CH2 | - | - | - | - |
| PE12 | - | EVENTOUT | TIM1\_CH3N | - | - | - | - |
| PE13 | - | EVENTOUT | TIM1\_CH3 | - | - | - | - |
| PE14 | - | EVENTOUT | TIM1\_CH4 | - | - | TIM1\_BKIN2 | - |
| PE15 | - | EVENTOUT | TIM1\_BKIN | - | - | - | USART3\_RX |

**Table 19. Alternate functions for port F**



**STM32F303xB STM32F303xC**

**Pinouts and pin description**

DocID023353 Rev 12

51/134

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Port & Pin Name** | **AF1** | **AF2** | **AF3** | **AF4** | **AF5** | **AF6** | **AF7** |
| PF0 | - | - | - | I2C2\_SDA | - | TIM1\_CH3N | - |
| PF1 | - | - | - | I2C2\_SCL | - | - | - |
| PF2 | EVENTOUT | - | - | - | - | - | - |
| PF4 | EVENTOUT | COMP1\_OUT | - | - | - | - | - |
| PF6 | EVENTOUT | TIM4\_CH4 | - | I2C2\_SCL | - | - | USART3\_RTS\_DE |
| PF9 | EVENTOUT | - | TIM15\_CH1 | - | SPI2\_SCK | - | - |
| PF10 | EVENTOUT | - | TIM15\_CH2 | - | SPI2\_SCK | - | - |

# Memory mapping

OxFFFF FFFF

### 7

OxEOOO OOOO

### 6

OxCOOO OOOO

### 5

OxAOOO OOOO

### 4

Ox8OOO OOOO

### 3

Ox6OOO OOOO

### 2

Ox4OOO OOOO

### 1

Ox2OOO OOOO

### O

OxOOOO OOOO

###### Figure 8. STM32F303xB/STM32F303xC memory map

Ox5OOO 07FF

|  |
| --- |
| AHB3 |
| Reserved |
| AHB2 |
| Reserved |
| AHB1 |
| Reserved |
| APB2 |
| Reserved |
| APB1 |

Ox5OOO OOOO

|  |
| --- |
| Cortex-M4 with FPU Internal Peripherals |
|  |
|  |
|  |
|  |
|  |
| Peripherals |
|  |
| SRAM |
| CODE |

Ox48OO 18OO Ox48OO OOOO

Ox4OO2 43FF Ox4OO2 OOOO

Ox4OO1 6COO

Ox4OO1 OOOO

Ox4OOO AOOO Ox4OOO OOOO

Ox1FFF FFFF Ox1FFF F8OO

|  |
| --- |
| Option bytes |
| System memory |
| Reserved |
| CCM RAM |
| Reserved |
| Flash memory |
| Reserved |
| Flash, system memory or SRAM, depending on BOOT configuration |

Ox1FFF D8OO Ox1OOO 2OOO

Ox1OOO OOOO OxO8O4 OOOO

OxO8OO OOOO OxOOO4 OOOO

Reserved

OxOOOO OOOO

MSv3O355V2

**Table 20. STM32F303xB/STM32F303xC memory map, peripheral register boundary addresses**

|  |  |  |  |
| --- | --- | --- | --- |
| **Bus** | **Boundary address** | **Size (bytes)** | **Peripheral** |
| AHB3 | 0x5000 0400 - 0x5000 07FF | 1 K | ADC3 - ADC4 |
| 0x5000 0000 - 0x5000 03FF | 1 K | ADC1 - ADC2 |
|  | 0x4800 1800 - 0x4FFF FFFF | ~132 M | Reserved |
| AHB2 | 0x4800 1400 - 0x4800 17FF | 1 K | GPIOF |
| 0x4800 1000 - 0x4800 13FF | 1 K | GPIOE |
| 0x4800 0C00 - 0x4800 0FFF | 1 K | GPIOD |
| 0x4800 0800 - 0x4800 0BFF | 1 K | GPIOC |
| 0x4800 0400 - 0x4800 07FF | 1 K | GPIOB |
| 0x4800 0000 - 0x4800 03FF | 1 K | GPIOA |
|  | 0x4002 4400 - 0x47FF FFFF | ~128 M | Reserved |
| AHB1 | 0x4002 4000 - 0x4002 43FF | 1 K | TSC |
| 0x4002 3400 - 0x4002 3FFF | 3 K | Reserved |
| 0x4002 3000 - 0x4002 33FF | 1 K | CRC |
| 0x4002 2400 - 0x4002 2FFF | 3 K | Reserved |
| 0x4002 2000 - 0x4002 23FF | 1 K | Flash interface |
| 0x4002 1400 - 0x4002 1FFF | 3 K | Reserved |
| 0x4002 1000 - 0x4002 13FF | 1 K | RCC |
| 0x4002 0800 - 0x4002 0FFF | 2 K | Reserved |
| 0x4002 0400 - 0x4002 07FF | 1 K | DMA2 |
| 0x4002 0000 - 0x4002 03FF | 1 K | DMA1 |
|  | 0x4001 8000 - 0x4001 FFFF | 32 K | Reserved |
| APB2 | 0x4001 4C00 - 0x4001 7FFF | 13 K | Reserved |
| 0x4001 4800 - 0x4001 4BFF | 1 K | TIM17 |
| 0x4001 4400 - 0x4001 47FF | 1 K | TIM16 |
| 0x4001 4000 - 0x4001 43FF | 1 K | TIM15 |
| 0x4001 3C00 - 0x4001 3FFF | 1 K | Reserved |
| 0x4001 3800 - 0x4001 3BFF | 1 K | USART1 |
| 0x4001 3400 - 0x4001 37FF | 1 K | TIM8 |
| 0x4001 3000 - 0x4001 33FF | 1 K | SPI1 |
| 0x4001 2C00 - 0x4001 2FFF | 1 K | TIM1 |
| 0x4001 0800 - 0x4001 2BFF | 9 K | Reserved |
| 0x4001 0400 - 0x4001 07FF | 1 K | EXTI |
| 0x4001 0000 - 0x4001 03FF | 1 K | SYSCFG + COMP + OPAMP |

**Table 20. STM32F303xB/STM32F303xC memory map, peripheral register boundary addresses (continued)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Bus** | **Boundary address** | **Size (bytes)** | **Peripheral** |
|  | 0x4000 8000 - 0x4000 FFFF | 32 K | Reserved |
| APB1 | 0x4000 7800 - 0x4000 7FFF | 2 K | Reserved |
| 0x4000 7400 - 0x4000 77FF | 1 K | DAC (dual) |
| 0x4000 7000 - 0x4000 73FF | 1 K | PWR |
| 0x4000 6800 - 0x4000 6FFF | 2 K | Reserved |
| 0x4000 6400 - 0x4000 67FF | 1 K | bxCAN |
| 0x4000 6000 - 0x4000 63FF | 1 K | USB SRAM 512 bytes |
| 0x4000 5C00 - 0x4000 5FFF | 1 K | USB device FS |
| 0x4000 5800 - 0x4000 5BFF | 1 K | I2C2 |
| 0x4000 5400 - 0x4000 57FF | 1 K | I2C1 |
| 0x4000 5000 - 0x4000 53FF | 1 K | UART5 |
| 0x4000 4C00 - 0x4000 4FFF | 1 K | UART4 |
| 0x4000 4800 - 0x4000 4BFF | 1 K | USART3 |
| 0x4000 4400 - 0x4000 47FF | 1 K | USART2 |
| 0x4000 4000 - 0x4000 43FF | 1 K | I2S3ext |
| 0x4000 3C00 - 0x4000 3FFF | 1 K | SPI3/I2S3 |
| 0x4000 3800 - 0x4000 3BFF | 1 K | SPI2/I2S2 |
| 0x4000 3400 - 0x4000 37FF | 1 K | I2S2ext |
| 0x4000 3000 - 0x4000 33FF | 1 K | IWDG |
| 0x4000 2C00 - 0x4000 2FFF | 1 K | WWDG |
| 0x4000 2800 - 0x4000 2BFF | 1 K | RTC |
| 0x4000 1800 - 0x4000 27FF | 4 K | Reserved |
| 0x4000 1400 - 0x4000 17FF | 1 K | TIM7 |
| 0x4000 1000 - 0x4000 13FF | 1 K | TIM6 |
| 0x4000 0C00 - 0x4000 0FFF | 1 K | Reserved |
| 0x4000 0800 - 0x4000 0BFF | 1 K | TIM4 |
| 0x4000 0400 - 0x4000 07FF | 1 K | TIM3 |
| 0x4000 0000 - 0x4000 03FF | 1 K | TIM2 |

## Parameter conditions

Unless otherwise specified, all voltages are referenced to VSS.

#### Minimum and maximum values

Unless otherwise specified, the minimum and maximum values are guaranteed in the worst conditions of ambient temperature, supply voltage and frequencies by tests in production on 100% of the devices with an ambient temperature at TA = 25 °C and TA = TAmax (given by the selected temperature range).

Data based on characterization results, design simulation and/or technology characteristics are indicated in the table footnotes. Based on characterization, the minimum and maximum values refer to sample tests and represent the mean value plus or minus three times the standard deviation (mean±3).

#### Typical values

Unless otherwise specified, typical data are based on TA = 25 °C, VDD = VDDA = 3.3 V. They are given only as design guidelines and are not tested.

Typical ADC accuracy values are determined by characterization of a batch of samples from a standard diffusion lot over the full temperature range, where 95% of the devices have an error less than or equal to the value indicated (mean±2).

#### Typical curves

Unless otherwise specified, all typical curves are given only as design guidelines and are not tested.

#### Loading capacitor

The loading conditions used for pin parameter measurement are shown in [*Figure 9*](#_bookmark115).

#### Pin input voltage

The input voltage measurement on a pin of the device is described in [*Figure 10*](#_bookmark116).



**Figure 9. Pin loading conditions**

**Figure 10. Pin input voltage**

MCU pin

MCU pin

C = 5O pF

VIN

MS1921OV1

MS19211V1

#### Power supply scheme

###### Figure 11. Power supply scheme



MS19875V5

VSSA

Analog: RCs, PLL,comparators, OPAMP,

....

REF-

V

ADC/DAC

VREF+

1O nF

+ 1 µF

VDDA

VDDA

4 x VSS

Regulator

4 x 1OO nF

+ 1 x 4.7 µF

4 x VDD

Kernel logic (CPU,

digital

& memories)

VDD

IN

I/O logic

GP I/Os

OUT

Backup circuitry (LSE, RTC,

Wakeup logic, Backup registers)

Power switch

1.65 – 3.6 V

VBAT

Level shifter

* + - 1. Dotted lines represent the internal connections on low pin count packages, joining the dedicated supply pins.

**Caution:** Each power supply pair (VDD/VSS, VDDA/VSSA etc..) must be decoupled with filtering ceramic capacitors as shown above. These capacitors must be placed as close as possible to, or below the appropriate pins on the underside of the PCB to ensure the good functionality of the device.

#### Current consumption measurement

**Figure 12. Current consumption measurement scheme**



IDD\_VBAT

VBAT

IDD

VDD

IDDA

VDDA

MS19213V1

## Absolute maximum ratings

Stresses above the absolute maximum ratings listed in [*Table 21: Voltage characteristics*](#_bookmark123), [*Table 22: Current characteristics*](#_bookmark125), and [*Table 23: Thermal characteristics*](#_bookmark127)may cause permanent damage to the device. These are stress ratings only and functional operation of the device at these conditions is not implied. Exposure to maximum rating conditions for extended periods may affect device reliability.

###### Table 21. Voltage characteristics(1)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Symbol** | **Ratings** | **Min** | **Max** | **Unit** |
| VDD–VSS | External main supply voltage (including VDDA, VBAT and VDD) | -0.3 | 4.0 | V |
| VDD–VDDA | Allowed voltage difference for VDD > VDDA | - | 0.4 |
| VREF+–VDD (2)  A | Allowed voltage difference for VREF+ > VDDA | - | 0.4 |
| V (3) IN | Input voltage on FT and FTf pins | VSS  0.3 | VDD + 4.0 |
| Input voltage on TTa pins | VSS  0.3 | 4.0 |
| Input voltage on any other pin | VSS  0.3 | 4.0 |
| Input voltage on Boot0 pin | 0 | 9 |
| |VDDx| | Variations between different VDD power pins(4) | - | 50 | mV |
| |VSSX  VSS| | Variations between all the different ground pins | - | 50 |
| VESD(HBM) | Electrostatic discharge voltage (human body model) | see [*Section 6.3.12: Electrical*](#_bookmark200)[*sensitivity characteristics*](#_bookmark200) | | - |

1. All main power (VDD, VDDA) and ground (VSS, VSSA) pins must always be connected to the external power supply, in the permitted range. The following relationship must be respected between VDDA and VDD:

VDDA must power on before or at the same time as VDD in the power up sequence.

VDDA must be greater than or equal to VDD.

1. VREF+ must be always lower or equal than VDDA (VREF+  VDDA). If unused then it must be connected to VDDA.
2. VIN maximum must always be respected. Refer to [*Table 22: Current characteristics*](#_bookmark125)for the maximum allowed injected current values.
3. Include VREF- pin.

###### Table 22. Current characteristics

|  |  |  |  |
| --- | --- | --- | --- |
| **Symbol** | **Ratings** | **Max.** | **Unit** |
| IVDD | Total current into sum of all VDD power lines (source) | 160 | mA |
| IVSS | Total current out of sum of all VSS ground lines (sink) |  160 |
| IVDD | Maximum current into each VDD power line (source)(1) | 100 |
| IVSS | Maximum current out of each VSS ground line (sink)(1) |  100 |
| IIO(PIN) | Output current sunk by any I/O and control pin | 25 |
| Output current source by any I/O and control pin |  25 |
| IIO(PIN) | Total output current sunk by sum of all IOs and control pins(2) | 80 |
| Total output current sourced by sum of all IOs and control pins(2) |  80 |
| IINJ(PIN) | Injected current on FT, FTf and B pins(3) | -5/+0 |
| Injected current on TC and RST pin(4) | ± 5 |
| Injected current on TTa pins(5) | ± 5 |
| IINJ(PIN) | Total injected current (sum of all I/O and control pins)(6) | ± 25 |

1. All main power (VDD, VDDA) and ground (VSS and VSSA) pins must always be connected to the external power supply, in the permitted range.
2. This current consumption must be correctly distributed over all I/Os and control pins.The total output current must not be sunk/sourced between two consecutive power supply pins referring to high pin count LQFP packages.
3. Positive injection is not possible on these I/Os and does not occur for input voltages lower than the specified maximum value.
4. A positive injection is induced by VIN > VDD while a negative injection is induced by VIN< VSS. IINJ(PIN) must never be exceeded. Refer to [*Table 21: Voltage characteristics*](#_bookmark123)for the maximum allowed input voltage values.
5. A positive injection is induced by VIN > VDDA while a negative injection is induced by VIN< VSS. IINJ(PIN) must never be exceeded. Refer also to [*Table 21: Voltage characteristics*](#_bookmark123)for the maximum allowed input voltage values. Negative injection disturbs the analog performance of the device. See note [(2)](#_bookmark264) below [*Table 70*](#_bookmark262).
6. When several inputs are submitted to a current injection, the maximum IINJ(PIN) is the absolute sum of the positive and negative injected currents (instantaneous values).

**Table 23. Thermal characteristics**

|  |  |  |  |
| --- | --- | --- | --- |
| **Symbol** | **Ratings** | **Value** | **Unit** |
| TSTG | Storage temperature range | –65 to +150 | °C |
| TJ | Maximum junction temperature | 150 | °C |

## Operating conditions

#### General operating conditions

###### Table 24. General operating conditions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Max** | **Unit** |
| fHCLK | Internal AHB clock frequency | - | 0 | 72 | MHz |
| fPCLK1 | Internal APB1 clock frequency | - | 0 | 36 |
| fPCLK2 | Internal APB2 clock frequency | - | 0 | 72 |
| VDD | Standard operating voltage | - | 2 | 3.6 | V |
| VDDA | Analog operating voltage (OPAMP and DAC not used) | Must have a potential equal to or higher than VDD | 2 | 3.6 | V |
| Analog operating voltage (OPAMP and DAC used) | 2.4 | 3.6 |
| VBAT | Backup operating voltage | - | 1.65 | 3.6 | V |
| VIN | I/O input voltage | TC I/O | –0.3 | VDD+0.3 | V |
| TTa I/O | –0.3 | VDDA+0.3 |
| FT and FTf I/O(1) | –0.3 | 5.5 |
| BOOT0 | 0 | 5.5 |
| PD | Power dissipation at TA = 85 °C for suffix 6 or TA = 105 °C for suffix 7(2) | WLCSP100 | - | 500 | mW |
| LQFP100 | - | 488 |
| LQFP64 | - | 444 |
| LQFP48 | - | 364 |
| Ta | Ambient temperature for 6 suffix version | Maximum power dissipation | –40 | 85 | °C |
| Low-power dissipation(3) | –40 | 105 |
| Ambient temperature for 7 suffix version | Maximum power dissipation | –40 | 105 | °C |
| Low-power dissipation[(3)](#_bookmark132) | –40 | 125 |
| Tj | Junction temperature range | 6 suffix version | –40 | 105 | °C |
| 7 suffix version | –40 | 125 |

* + - 1. To sustain a voltage higher than VDD+0.3 V, the internal pull-up/pull-down resistors must be disabled.
      2. If TA is lower, higher PD values are allowed as long as TJ does not exceed TJmax (see [*Section 7.5: Thermal*](#_bookmark327)[*characteristics*](#_bookmark327)).
      3. In low-power dissipation state, TA can be extended to this range as long as TJ does not exceed TJmax (see

[*Section 7.5: Thermal characteristics*](#_bookmark327)).

#### Operating conditions at power-up / power-down

The parameters given in [*Table 25*](#_bookmark134)are derived from tests performed under the ambient temperature condition summarized in [*Table 24*](#_bookmark130).

**Table 25.** **Operating conditions at power-up / power-down**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Max** | **Unit** |
| tVDD | VDD rise time rate | - | 0 |  | µs/V |
| VDD fall time rate | 20 |  |
| tVDDA | VDDA rise time rate | - | 0 |  |
| VDDA fall time rate | 20 |  |

#### Embedded reset and power control block characteristics

The parameters given in [*Table 26*](#_bookmark137)are derived from tests performed under ambient temperature and VDD supply voltage conditions summarized in [*Table 24*](#_bookmark130).

###### Table 26. Embedded reset and power control block characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| V (1)  POR/PDR | Power on/power down reset threshold | Falling edge | 1.8(2) | 1.88 | 1.96 | V |
| Rising edge | 1.84 | 1.92 | 2.0 | V |
| VPDRhyst(1) | PDR hysteresis | - | - | 40 | - | mV |
| tRS (3)  TTEMPO | POR reset temporization | - | 1.5 | 2.5 | 4.5 | ms |

* + - 1. The PDR detector monitors VDD and also VDDA (if kept enabled in the option bytes). The POR detector monitors only VDD.
      2. The product behavior is guaranteed by design down to the minimum VPOR/PDR value.
      3. Guaranteed by design.

###### Table 27. Programmable voltage detector characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min(1)** | **Typ** | **Max**[**(1)**](#_bookmark139) | **Unit** |
| VPVD0 | PVD threshold 0 | Rising edge | 2.1 | 2.18 | 2.26 | V |
| Falling edge | 2 | 2.08 | 2.16 |
| VPVD1 | PVD threshold 1 | Rising edge | 2.19 | 2.28 | 2.37 |
| Falling edge | 2.09 | 2.18 | 2.27 |
| VPVD2 | PVD threshold 2 | Rising edge | 2.28 | 2.38 | 2.48 |
| Falling edge | 2.18 | 2.28 | 2.38 |
| VPVD3 | PVD threshold 3 | Rising edge | 2.38 | 2.48 | 2.58 |
| Falling edge | 2.28 | 2.38 | 2.48 |
| VPVD4 | PVD threshold 4 | Rising edge | 2.47 | 2.58 | 2.69 |
| Falling edge | 2.37 | 2.48 | 2.59 |
| VPVD5 | PVD threshold 5 | Rising edge | 2.57 | 2.68 | 2.79 |
| Falling edge | 2.47 | 2.58 | 2.69 |
| VPVD6 | PVD threshold 6 | Rising edge | 2.66 | 2.78 | 2.9 |
| Falling edge | 2.56 | 2.68 | 2.8 |
| VPVD7 | PVD threshold 7 | Rising edge | 2.76 | 2.88 | 3 |
| Falling edge | 2.66 | 2.78 | 2.9 |
| (2)  VPVDhyst | PVD hysteresis | - | - | 100 | - | mV |
| IDD(PVD) | PVD current consumption | - | - | 0.15 | 0.26 | µA |

1. Guaranteed by characterization results.
2. Guaranteed by design.

#### Embedded reference voltage

The parameters given in [*Table 28*](#_bookmark141)are derived from tests performed under ambient temperature and VDD supply voltage conditions summarized in [*Table 24*](#_bookmark130).

###### Table 28. Embedded internal reference voltage

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| VREFINT | Internal reference voltage | –40 °C < TA < +105 °C | 1.16 | 1.2 | 1.25 | V |
| –40 °C < TA < +85 °C | 1.16 | 1.2 | 1.24(1) | V |
| TS\_vrefint | ADC sampling time when reading the internal reference voltage | - | 2.2 | - | - | µs |
| VRERINT | Internal reference voltage spread over the temperature range | VDD = 3 V ±10 mV | - | - | 10(2) | mV |
| TCoeff | Temperature coefficient | - | - | - | 100(2) | ppm/°C |

* + - 1. Guaranteed by characterization results.
      2. Guaranteed by design.

**Table 29.** **Internal reference voltage calibration values**

|  |  |  |
| --- | --- | --- |
| **Calibration value name** | **Description** | **Memory address** |
| VREFINT\_CAL | Raw data acquired at temperature of 30 °C VDDA= 3.3 V | 0x1FFF F7BA - 0x1FFF F7BB |

#### Supply current characteristics

The current consumption is a function of several parameters and factors such as the operating voltage, ambient temperature, I/O pin loading, device software configuration, operating frequencies, I/O pin switching rate, program location in memory and executed binary code.

The current consumption is measured as described in [*Figure 12: Current consumption*](#_bookmark121)[*measurement scheme*](#_bookmark121).

All Run-mode current consumption measurements given in this section are performed with a reduced code that gives a consumption equivalent to CoreMark code.

##### Typical and maximum current consumption

The MCU is placed under the following conditions:

* All I/O pins are in input mode with a static value at VDD or VSS (no load)
* All peripherals are disabled except when explicitly mentioned
* The Flash memory access time is adjusted to the fHCLK frequency (0 wait state from 0 to 24 MHz,1 wait state from 24 to 48 MHz and 2 wait states from 48 to 72 MHz)
* Prefetch in ON (reminder: this bit must be set before clock setting and bus prescaling)
* When the peripherals are enabled fPCLK2 = fHCLK and fPCLK1 = fHCLK/2
* When fHCLK > 8 MHz, the PLL is ON and the PLL input is equal to HSI/2 (4 MHz) or HSE (8 MHz) in bypass mode.

The parameters given in [*Table 30*](#_bookmark146)to [*Table 34*](#_bookmark156)are derived from tests performed under ambient temperature and supply voltage conditions summarized in [*Table 24*](#_bookmark130).

###### Table 30. Typical and maximum current consumption from VDD supply at VDD = 3.6V

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **fHCLK** | **All peripherals enabled** | | | | **All peripherals disabled** | | | | **Unit** |
| **Typ** | **Max @ T (1)**  **A** | | | **Typ** | **Max @ TA**[**(1)**](#_bookmark148) | | |
| **25 °C** | **85 °C** | **105 °C** | **25 °C** | **85 °C** | **105 °C** |
| IDD | Supply current in Run mode, executing from Flash | External clock (HSE bypass) | 72 MHz | 61.2 | 65.8 | 67.6 | 68.5 | 27.8 | 30.3 | 30.7 | 31.5 | mA |
| 64 MHz | 54.7 | 59.1 | 60.2 | 61.1 | 24.6 | 27.2 | 27.6 | 28.3 |
| 48 MHz | 41.7 | 45.1 | 46.2 | 47.2 | 19.2 | 21.1 | 21.4 | 21.8 |
| 32 MHz | 28.1 | 31.5 | 32.5 | 32.7 | 12.9 | 14.6 | 14.8 | 15.3 |
| 24 MHz | 21.4 | 23.7 | 24.4 | 25.2 | 10.0 | 11.4 | 11.4 | 12.1 |
| 8 MHz | 7.4 | 8.4 | 8.6 | 9.4 | 3.6 | 4.1 | 4.4 | 5.0 |
| 1 MHz | 1.3 | 1.6 | 1.8 | 2.6 | 0.8 | 1.0 | 1.2 | 2.1 |
| Internal clock (HSI) | 64 MHz | 49.7 | 54.4 | 55.4 | 56.3 | 24.5 | 27.2 | 27.4 | 28.1 |
| 48 MHz | 37.9 | 42.2 | 43.0 | 43.5 | 18.9 | 21.4 | 21.5 | 21.6 |
| 32 MHz | 25.8 | 29.2 | 29.2 | 30.0 | 12.7 | 14.2 | 14.6 | 15.2 |
| 24 MHz | 19.7 | 22.3 | 22.6 | 23.2 | 6.7 | 7.7 | 7.9 | 8.5 |
| 8 MHz | 6.9 | 7.8 | 8.3 | 8.8 | 3.5 | 4.0 | 4.4 | 5.0 |
| Supply current in Run mode, executing from RAM | External clock (HSE bypass) | 72 MHz | 60.8 | 66.2(2) | 69.7 | 70.4(2) | 27.4 | 31.7(2) | 32.2 | 32.5(2) |
| 64 MHz | 54.3 | 59.1 | 62.2 | 63.3 | 24.3 | 28.3 | 28.7 | 28.8 |
| 48 MHz | 41.0 | 45.6 | 47.3 | 47.9 | 18.3 | 21.6 | 21.9 | 22.1 |
| 32 MHz | 27.6 | 32.4 | 32.4 | 32.9 | 12.3 | 15.0 | 15.2 | 15.4 |
| 24 MHz | 20.8 | 23.9 | 24.3 | 25.0 | 9.3 | 11.3 | 11.4 | 12.0 |
| 8 MHz | 6.9 | 7.8 | 8.7 | 9.0 | 3.1 | 3.7 | 4.2 | 4.9 |
| 1 MHz | 0.9 | 1.2 | 1.5 | 2.3 | 0.4 | 0.6 | 1.0 | 1.8 |
| Internal clock (HSI) | 64 MHz | 49.2 | 53.9 | 55.2 | 57.4 | 23.9 | 27.8 | 28.2 | 28.4 |
| 48 MHz | 37.3 | 40.8 | 41.4 | 44.1 | 18.2 | 21.0 | 21.6 | 21.9 |
| 32 MHz | 25.1 | 27.6 | 29.1 | 30.1 | 12.0 | 14.0 | 14.5 | 15.1 |
| 24 MHz | 19.0 | 21.6 | 22.1 | 22.9 | 6.3 | 7.2 | 7.7 | 8.1 |
| 8 MHz | 6.4 | 7.3 | 7.9 | 8.4 | 3.0 | 3.5 | 4.0 | 4.7 |

**Table 30. Typical and maximum current consumption from VDD supply at VDD = 3.6V (continued)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **fHCLK** | **All peripherals enabled** | | | | **All peripherals disabled** | | | | **Unit** |
| **Typ** | **Max @ T (1)**  **A** | | | **Typ** | **Max @ TA(1)** | | |
| **25 °C** | **85 °C** | **105 °C** | **25 °C** | **85 °C** | **105 °C** |
| IDD | Supply current in Sleep mode, executing from Flash or RAM | External clock (HSE bypass) | 72 MHz | 44.0 | 48.4 | 49.4 | 50.5 | 6.6 | 7.5 | 7.9 | 8.7 | mA |
| 64 MHz | 39.2 | 43.3 | 44.0 | 45.2 | 6.0 | 6.8 | 7.2 | 7.9 |
| 48 MHz | 29.6 | 32.7 | 33.3 | 34.3 | 4.5 | 5.2 | 5.6 | 6.3 |
| 32 MHz | 19.7 | 23.3 | 23.3 | 23.5 | 3.1 | 3.5 | 4.0 | 4.8 |
| 24 MHz | 14.9 | 17.6 | 17.8 | 18.3 | 2.4 | 2.8 | 3.3 | 3.9 |
| 8 MHz | 4.9 | 5.7 | 6.1 | 6.9 | 0.8 | 1.0 | 1.4 | 2.2 |
| 1 MHz | 0.6 | 0.9 | 1.2 | 2.1 | 0.1 | 0.3 | 0.6 | 1.5 |
| Internal clock (HSI) | 64 MHz | 34.2 | 38.1 | 39.2 | 40.3 | 5.7 | 6.3 | 6.8 | 7.5 |
| 48 MHz | 25.8 | 28.7 | 29.6 | 30.3 | 4.3 | 4.8 | 5.2 | 5.9 |
| 32 MHz | 17.4 | 19.4 | 19.9 | 20.7 | 2.9 | 3.2 | 3.7 | 4.5 |
| 24 MHz | 13.2 | 15.1 | 15.6 | 15.9 | 1.5 | 1.8 | 2.2 | 2.9 |
| 8 MHz | 4.5 | 5.0 | 5.6 | 6.2 | 0.7 | 0.9 | 1.2 | 2.1 |

1. Guaranteed by characterization results unless otherwise specified.
2. Data based on characterization results and tested in production with code executing from RAM.

###### Table 31. Typical and maximum current consumption from the VDDA supply

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions**  **(1)** | **fHCLK** | **VDDA = 2.4 V** | | | | **VDDA = 3.6 V** | | | | **Unit** |
| **Typ** | **Max @ T (2)**  **A** | | | **Typ** | **Max @ T** [**(2)**](#_bookmark151)  **A** | | |
| **25 °C** | **85 °C** | **105 °C** | **25 °C** | **85 °C** | **105 °C** |
| IDDA | Supply current in Run/Sleep mode, code executing from Flash or RAM | HSE  bypass | 72 MHz | 225 | 276 | 289 | 297 | 245 | 302 | 319 | 329 | µA |
| 64 MHz | 198 | 249 | 261 | 268 | 216 | 270 | 284 | 293 |
| 48 MHz | 149 | 195 | 204 | 211 | 159 | 209 | 222 | 230 |
| 32 MHz | 102 | 145 | 152 | 157 | 110 | 154 | 162 | 169 |
| 24 MHz | 80 | 119 | 124 | 128 | 86 | 126 | 131 | 135 |
| 8 MHz | 2 | 3 | 4 | 6 | 3 | 4 | 5 | 9 |
| 1 MHz | 2 | 3 | 5 | 7 | 3 | 4 | 6 | 9 |
| HSI clock | 64 MHz | 270 | 323 | 337 | 344 | 299 | 354 | 371 | 381 |
| 48 MHz | 220 | 269 | 280 | 286 | 244 | 293 | 309 | 318 |
| 32 MHz | 173 | 218 | 228 | 233 | 193 | 239 | 251 | 257 |
| 24 MHz | 151 | 194 | 200 | 204 | 169 | 211 | 219 | 225 |
| 8 MHz | 73 | 97 | 99 | 103 | 88 | 105 | 110 | 116 |

1. Current consumption from the VDDA supply is independent of whether the peripherals are on or off. Furthermore when the PLL is off, IDDA is independent from the frequency.
2. Guaranteed by characterization results.

###### Table 32. Typical and maximum VDD consumption in Stop and Standby modes

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Typ @VDD (VDD=VDDA)** | | | | | | **Max(1)** | | | **Unit** |
| **2.0 V** | **2.4 V** | **2.7 V** | **3.0 V** | **3.3 V** | **3.6 V** | **TA = 25 °C** | **TA = 85 °C** | **TA = 105 °C** |
| IDD | Supply current in Stop mode | Regulator in run mode, all oscillators OFF | 20.05 | 20.33 | 20.42 | 20.50 | 20.67 | 20.80 | 44.2(2) | 350 | 735(2) | µA |
| Regulator in low-power mode, all oscillators OFF | 7.63 | 7.77 | 7.90 | 8.07 | 8.17 | 8.33 | 30.6(2) | 335 | 720(2) |
| Supply | LSI ON and IWDG ON | 0.80 | 0.96 | 1.09 | 1.23 | 1.37 | 1.51 | - | - | - |
|  | current in |  |
|  |  |  |  |  |  |  |  |  |  |
|  | Standby mode | LSI OFF and IWDG OFF | 0.60 | 0.74 | 0.83 | 0.93 | 1.02 | 1.11 | 5.0(2) | 7.8 | 13.3(2) |  |

1. Guaranteed by characterization results unless otherwise specified.
2. Data based on characterization results and tested in production.

###### Table 33. Typical and maximum VDDA consumption in Stop and Standby modes

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | **Typ @VDD (VDD = VDDA)** | | | | | | **Max**(1) | | | **Unit** |
| **2.0 V** | **2.4 V** | **2.7 V** | **3.0 V** | **3.3 V** | **3.6 V** | **TA = 25 °C** | **TA = 85 °C** | **TA = 105 °C** |
| IDDA | Supply current in Stop mode | VDDA monitoring ON | Regulator in run mode, all oscillators OFF | 1.81 | 1.95 | 2.07 | 2.20 | 2.35 | 2.52 | 3.7 | 5.5 | 8.8 | µA |
| Regulator in low-power mode, all oscillators OFF | 1.81 | 1.95 | 2.07 | 2.20 | 2.35 | 2.52 | 3.7 | 5.5 | 8.8 |
| Supply current in Standby mode | LSI ON and IWDG ON | 2.22 | 2.42 | 2.59 | 2.78 | 3.0 | 3.24 | - | - | - |
| LSI OFF and IWDG OFF | 1.69 | 1.82 | 1.94 | 2.08 | 2.23 | 2.40 | 3.5 | 5.4 | 9.2 |
| Supply current in Stop mode | VDDA monitoring OFF | Regulator in run mode, all oscillators OFF | 1.05 | 1.08 | 1.10 | 1.15 | 1.22 | 1.29 | - | - | - |
| Regulator in low-power mode, all oscillators OFF | 1.05 | 1.08 | 1.10 | 1.15 | 1.22 | 1.29 | - | - | - |
| Supply current in Standby mode | LSI ON and IWDG ON | 1.44 | 1.52 | 1.60 | 1.71 | 1.84 | 1.98 | - | - | - |
| LSI OFF and IWDG OFF | 0.93 | 0.95 | 0.98 | 1.02 | 1.08 | 1.15 | - | - | - |

1. Guaranteed by characterization results.

*Note: The total consumption is the sum of IDD and IDDA.*

###### Table 34. Typical and maximum current consumption from VBAT supply

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Para meter** | **Conditions**  **(1)** | **Typ @VBAT** | | | | | | | | **Max @VBAT = 3.6 V(2)** | | | **Unit** |
| **1.65V** | **1.8V** | **2V** | **2.4V** | **2.7V** | **3V** | **3.3V** | **3.6V** | **TA = 25°C** | **TA = 85°C** | **TA = 105°C** |
| IDD\_VBAT | Backup domain supply current | LSE & RTC  ON; "Xtal mode" lower driving capability; LSEDRV[1: 0] = '00' | 0.48 | 0.50 | 0.52 | 0.58 | 0.65 | 0.72 | 0.80 | 0.90 | 1.1 | 1.5 | 2.0 | µA |
| LSE & RTC  ON; "Xtal mode" higher driving capability; LSEDRV[1: 0] = '11' | 0.83 | 0.86 | 0.90 | 0.98 | 1.03 | 1.10 | 1.20 | 1.30 | 1.5 | 2.2 | 2.9 |

1. Crystal used: Abracon ABS07-120-32.768 kHz-T with a CL of 6 pF for typical values.
2. Guaranteed by characterization results.

**Figure 13.** **Typical VBAT current consumption (LSE and RTC ON/LSEDRV[1:0] = ’00’)**

1.4

1.2

1

O.8

O.6

O.4

O.2

1.65 V

1.8 V

2 V

2.4 V

2.7 V

3 V

3.3 V

3.6 V

O

25°C

6O°C

85°C

1O5°C

TA (°C)

MS31124V1

IVBAT(µA)

##### Typical current consumption

The MCU is placed under the following conditions:

* + VDD = VDDA = 3.3 V
  + All I/O pins available on each package are in analog input configuration
  + The Flash access time is adjusted to fHCLK frequency (0 wait states from 0 to 24 MHz, 1 wait state from 24 to 48 MHz and 2 wait states from 48 MHz to 72 MHz), and Flash prefetch is ON
  + When the peripherals are enabled, fAPB1 = fAHB/2, fAPB2 = fAHB
  + PLL is used for frequencies greater than 8 MHz
  + AHB prescaler of 2, 4, 8,16 and 64 is used for the frequencies 4 MHz, 2 MHz, 1 MHz,

500 kHz and 125 kHz respectively.

###### Table 35. Typical current consumption in Run mode, code with data processing running from Flash

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **fHCLK** | **Typ** | | **Unit** |
| **Peripherals enabled** | **Peripherals disabled** |
|  |  |  | 72 MHz | 61.3 | 28.0 |  |
|  |  |  | 64 MHz | 54.8 | 25.4 |  |
|  |  |  | 48 MHz | 41.9 | 19.3 |  |
|  |  |  | 32 MHz | 28.5 | 13.3 |  |
|  | Supply current in |  | 24 MHz | 21.8 | 10.4 |  |
| 16 MHz | 14.9 | 7.2 |
| IDD | Run mode from VDD supply |  | mA |
| 8 MHz | 7.7 | 3.9 |
| 4 MHz | 4.5 | 2.5 |
|  |  |  | 2 MHz | 2.8 | 1.7 |  |
|  |  |  | 1 MHz | 1.9 | 1.3 |  |
|  |  | Running from HSE | 500 kHz | 1.4 | 1.1 |  |
| 125 kHz | 1.1 | 0.9 |
|  |  | crystal clock 8 MHz, |  |
|  |  | code executing from | 72 MHz | 240.3 | 239.5 |  |
|  |  | Flash |  |
| 64 MHz | 210.9 | 210.3 |
|  |  |  | 48 MHz | 155.8 | 155.6 |  |
|  |  |  | 32 MHz | 105.7 | 105.6 |  |
| IDDA(1) (2) | Supply current in Run mode from |  | 24 MHz | 82.1 | 82.0 | µA |
| 16 MHz | 58.8 | 58.8 |
| 8 MHz | 2.4 | 2.4 |
|  | VDDA supply |  |  |
| 4 MHz | 2.4 | 2.4 |
|  |  |  | 2 MHz | 2.4 | 2.4 |  |
|  |  |  | 1 MHz | 2.4 | 2.4 |  |
|  |  |  | 500 kHz | 2.4 | 2.4 |  |
|  |  |  | 125 kHz | 2.4 | 2.4 |  |

1. VDDA monitoring is ON.
2. When peripherals are enabled, the power consumption of the analog part of peripherals such as ADC, DAC, Comparators, OpAmp etc. is not included. Refer to the tables of characteristics in the subsequent sections.

###### Table 36. Typical current consumption in Sleep mode, code running from Flash or RAM

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **fHCLK** | **Typ** | | **Unit** |
| **Peripherals enabled** | **Peripherals disabled** |
|  |  |  | 72 MHz | 44.1 | 7.0 |  |
|  |  |  | 64 MHz | 39.7 | 6.3 |  |
|  |  |  | 48 MHz | 30.3 | 4.9 |  |
|  |  |  | 32 MHz | 20.5 | 3.5 |  |
|  | Supply current in |  | 24 MHz | 15.4 | 2.8 |  |
| 16 MHz | 10.6 | 2.0 |
| IDD | Sleep mode from VDD supply |  | mA |
| 8 MHz | 5.4 | 1.1 |
| 4 MHz | 3.2 | 1.0 |
|  |  |  | 2 MHz | 2.1 | 0.9 |  |
|  |  |  | 1 MHz | 1.5 | 0.8 |  |
|  |  | Running from HSE | 500 kHz | 1.2 | 0.8 |  |
| 125 kHz | 1.0 | 0.8 |
|  |  | crystal clock 8 MHz, |  |
|  |  | code executing from | 72 MHz | 239.7 | 238.5 |  |
|  |  | Flash or RAM |  |
| 64 MHz | 210.5 | 209.6 |
|  |  |  | 48 MHz | 155.0 | 155.6 |  |
|  |  |  | 32 MHz | 105.3 | 105.2 |  |
| IDDA(1) (2) | Supply current in Sleep mode from |  | 24 MHz | 81.9 | 81.8 | µA |
| 16 MHz | 58.7 | 58.6 |
| 8 MHz | 2.4 | 2.4 |
|  | VDDA supply |  |  |
| 4 MHz | 2.4 | 2.4 |
|  |  |  | 2 MHz | 2.4 | 2.4 |  |
|  |  |  | 1 MHz | 2.4 | 2.4 |  |
|  |  |  | 500 kHz | 2.4 | 2.4 |  |
|  |  |  | 125 kHz | 2.4 | 2.4 |  |

1. VDDA monitoring is ON.
2. When peripherals are enabled, the power consumption of the analog part of peripherals such as ADC, DAC, Comparators, OpAmp etc. is not included. Refer to the tables of characteristics in the subsequent sections.

##### I/O system current consumption

The current consumption of the I/O system has two components: static and dynamic.

###### I/O static current consumption

All the I/Os used as inputs with pull-up generate current consumption when the pin is externally held low. The value of this current consumption can be simply computed by using the pull-up/pull-down resistors values given in [*Table 54: I/O static characteristics*](#_bookmark210).

For the output pins, any external pull-down or external load must also be considered to estimate the current consumption.

Additional I/O current consumption is due to I/Os configured as inputs if an intermediate voltage level is externally applied. This current consumption is caused by the input Schmitt trigger circuits used to discriminate the input value. Unless this specific configuration is required by the application, this supply current consumption can be avoided by configuring these I/Os in analog mode. This is notably the case of ADC input pins which should be configured as analog inputs.

**Caution:** Any floating input pin can also settle to an intermediate voltage level or switch inadvertently, as a result of external electromagnetic noise. To avoid current consumption related to floating pins, they must either be configured in analog mode, or forced internally to a definite digital value. This can be done either by using pull-up/down resistors or by configuring the pins in output mode.

###### I/O dynamic current consumption

In addition to the internal peripheral current consumption (see[*Table 38: Peripheral current*](#_bookmark166)[*consumption*](#_bookmark166)), the I/Os used by an application also contribute to the current consumption. When an I/O pin switches, it uses the current from the MCU supply voltage to supply the I/O pin circuitry and to charge/discharge the capacitive load (internal or external) connected to the pin:

ISW = VDD  fSW  C

where

ISW is the current sunk by a switching I/O to charge/discharge the capacitive load VDD is the MCU supply voltage

fSW is the I/O switching frequency

C is the total capacitance seen by the I/O pin: C = CINT+ CEXT+CS

The test pin is configured in push-pull output mode and is toggled by software at a fixed frequency.

###### Table 37. Switching output I/O current consumption

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions(1)** | **I/O toggling frequency (fSW)** | **Typ** | **Unit** |
| ISW | I/O current consumption | VDD = 3.3 V  Cext = 0 pF  C = CINT + CEXT+ CS | 2 MHz | 0.90 | mA |
| 4 MHz | 0.93 |
| 8 MHz | 1.16 |
| 18 MHz | 1.60 |
| 36 MHz | 2.51 |
| 48 MHz | 2.97 |
| VDD = 3.3 V  Cext = 10 pF  C = CINT + CEXT +CS | 2 MHz | 0.93 |
| 4 MHz | 1.06 |
| 8 MHz | 1.47 |
| 18 MHz | 2.26 |
| 36 MHz | 3.39 |
| 48 MHz | 5.99 |
| VDD = 3.3 V  Cext = 22 pF  C = CINT + CEXT +CS | 2 MHz | 1.03 |
| 4 MHz | 1.30 |
| 8 MHz | 1.79 |
| 18 MHz | 3.01 |
| 36 MHz | 5.99 |
| VDD = 3.3 V  Cext = 33 pF  C = CINT + CEXT+ CS | 2 MHz | 1.10 |
| 4 MHz | 1.31 |
| 8 MHz | 2.06 |
| 18 MHz | 3.47 |
| 36 MHz | 8.35 |
| VDD = 3.3 V  Cext = 47 pF  C = CINT + CEXT+ CS | 2 MHz | 1.20 |
| 4 MHz | 1.54 |
| 8 MHz | 2.46 |
| 18 MHz | 4.51 |
| 36 MHz | 9.98 |

* 1. CS = 5 pF (estimated value).

##### On-chip peripheral current consumption

The MCU is placed under the following conditions:

* + - all I/O pins are in analog input configuration
    - all peripherals are disabled unless otherwise mentioned
    - the given value is calculated by measuring the current consumption
      * with all peripherals clocked off
      * with only one peripheral clocked on
    - ambient operating temperature at 25°C and VDD = VDDA = 3.3 V.

###### Table 38. Peripheral current consumption

|  |  |  |
| --- | --- | --- |
| **Peripheral** | **Typical consumption(1)** | **Unit** |
| **IDD** |
| BusMatrix (2) | 12.6 | µA/MHz |
| DMA1 | 7.6 |
| DMA2 | 6.1 |
| CRC | 2.1 |
| GPIOA | 10.0 |
| GPIOB | 10.3 |
| GPIOC | 2.2 |
| GPIOD | 8.8 |
| GPIOE | 3.3 |
| GPIOF | 3.0 |
| TSC | 5.5 |
| ADC1&2 | 17.3 |
| ADC3&4 | 18.8 |
| APB2-Bridge (3) | 3.6 |
| SYSCFG | 7.3 |
| TIM1 | 40.0 |
| SPI1 | 8.8 |
| TIM8 | 36.4 |
| USART1 | 23.3 |
| TIM15 | 17.1 |
| TIM16 | 10.1 |
| TIM17 | 11.0 |
| APB1-Bridge (3) | 6.1 |
| TIM2 | 49.1 |
| TIM3 | 38.8 |
| TIM4 | 38.3 |

**Table 38. Peripheral current consumption (continued)**

|  |  |  |
| --- | --- | --- |
| **Peripheral** | **Typical consumption(1)** | **Unit** |
| **IDD** |
| TIM6 | 9.7 | µA/MHz |
| TIM7 | 12.1 |
| WWDG | 6.4 |
| SPI2 | 40.4 |
| SPI3 | 40.0 |
| USART2 | 41.9 |
| USART3 | 40.2 |
| UART4 | 36.5 |
| UART5 | 30.8 |
| I2C1 | 10.5 |
| I2C2 | 10.4 |
| USB | 26.2 |
| CAN | 33.4 |
| PWR | 5.7 |
| DAC | 15.4 |

1. The power consumption of the analog part (IDDA) of peripherals such as ADC, DAC, Comparators, OpAmp etc. is not included. Refer to the tables of characteristics in the subsequent sections.
2. BusMatrix is automatically active when at least one master is ON (CPU, DMA1 or DMA2).
3. The APBx bridge is automatically active when at least one peripheral is ON on the same bus.

#### Wakeup time from low-power mode

The wakeup times given in [*Table 39*](#_bookmark170)are measured starting from the wakeup event trigger up to the first instruction executed by the CPU:

* For Stop or Sleep mode: the wakeup event is WFE.
* WKUP1 (PA0) pin is used to wakeup from Standby, Stop and Sleep modes.

All timings are derived from tests performed under ambient temperature and VDD supply voltage conditions summarized in [*Table 24*](#_bookmark130).

###### Table 39. Low-power mode wakeup timings

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Typ @VDD, VDD = VDDA** | | | | | | **Max** | **Unit** |
| **2.0 V** | **2.4 V** | **2.7 V** | **3 V** | **3.3 V** | **3.6 V** |
| tWUSTOP | Wakeup from Stop mode | Regulator in run mode | 4.1 | 3.9 | 3.8 | 3.7 | 3.6 | 3.5 | 4.5 | µs |
| Regulator in low-power mode | 7.9 | 6.7 | 6.1 | 5.7 | 5.4 | 5.2 | 9 |
| tWUSTANDB (1)  Y | Wakeup from Standby mode | LSI and IWDG OFF | 69.2 | 60.3 | 56.4 | 53.7 | 51.7 | 50 | 100 |
| tWUSLEEP | Wakeup from Sleep mode | - | 6 | | | | | | - | CPU  clock cycles |

1. Guaranteed by characterization results.

#### External clock source characteristics

##### High-speed external user clock generated from an external source

In bypass mode the HSE oscillator is switched off and the input pin is a standard GPIO. The external clock signal has to respect the I/O characteristics in [*Section 6.3.14*](#_bookmark208). However, the recommended clock input waveform is shown in [*Figure 14*](#_bookmark174).

###### Table 40. High-speed external user clock characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| fHSE\_ext | User external clock source frequency(1) | - | 1 | 8 | 32 | MHz |
| VHSEH | OSC\_IN input pin high level voltage | 0.7VDD | - | VDD | V |
| VHSEL | OSC\_IN input pin low level voltage | VSS | - | 0.3VDD |
| tw(HSEH) tw(HSEL) | OSC\_IN high or low time(1) | 15 | - | - | ns |
| tr(HSE) tf(HSE) | OSC\_IN rise or fall time(1) | - | - | 20 |

* + - 1. Guaranteed by design.

**Figure 14. High-speed external clock source AC timing diagram**

MS19214V2

THSE

t

tw(HSEL)

tf(HSE)

tr(HSE)

VHSEH

9O%

1O%

VHSEL

tw(HSEH)

##### Low-speed external user clock generated from an external source

In bypass mode the LSE oscillator is switched off and the input pin is a standard GPIO. The external clock signal has to respect the I/O characteristics in [*Section 6.3.14*](#_bookmark208). However, the recommended clock input waveform is shown in [*Figure 15*](#_bookmark176)

###### Table 41. Low-speed external user clock characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| fLSE\_ext | User External clock source frequency(1) | - | - | 32.768 | 1000 | kHz |
| VLSEH | OSC32\_IN input pin high level voltage | 0.7VDD | - | VDD | V |
| VLSEL | OSC32\_IN input pin low level voltage | VSS | - | 0.3VDD |
| tw(LSEH) tw(LSEL) | OSC32\_IN high or low time(1) | 450 | - | - | ns |
| tr(LSE) tf(LSE) | OSC32\_IN rise or fall time(1) | - | - | 50 |

1. Guaranteed by design.

**Figure 15. Low-speed external clock source AC timing diagram**

MS19215V2

TLSE

t

tw(LSEL)

tf(LSE)

tr(LSE)

VLSEH

9O%

1O%

VLSEL

tw(LSEH)

##### High-speed external clock generated from a crystal/ceramic resonator

The high-speed external (HSE) clock can be supplied with a 4 to 32 MHz crystal/ceramic resonator oscillator. All the information given in this paragraph are based on design simulation results obtained with typical external components specified in [*Table 42*](#_bookmark177). In the application, the resonator and the load capacitors have to be placed as close as possible to the oscillator pins in order to minimize output distortion and startup stabilization time. Refer to the crystal resonator manufacturer for more details on the resonator characteristics (frequency, package, accuracy).

###### Table 42. HSE oscillator characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions(1)** | **Min(2)** | **Typ** | **Max(2)** | **Unit** |
| fOSC\_IN | Oscillator frequency | - | 4 | 8 | 32 | MHz |
| RF | Feedback resistor | - | - | 200 |  | k |
| IDD | HSE current consumption | During startup(3) | - | - | 8.5 | mA |
| VDD=3.3 V, Rm= 30, CL=10 pF@8 MHz | - | 0.4 | - |
| VDD=3.3 V, Rm= 45, CL=10 pF@8 MHz | - | 0.5 | - |
| VDD=3.3 V, Rm= 30, CL=5 pF@32 MHz | - | 0.8 | - |
| VDD=3.3 V, Rm= 30, CL=10 pF@32 MHz | - | 1 | - |
| VDD=3.3 V, Rm= 30, CL=20 pF@32 MHz | - | 1.5 | - |
| gm | Oscillator transconductance | Startup | 10 | - | - | mA/V |
| (4)  tSU(HSE) | Startup time | VDD is stabilized | - | 2 | - | ms |

1. Resonator characteristics given by the crystal/ceramic resonator manufacturer.
2. Guaranteed by design.
3. This consumption level occurs during the first 2/3 of the tSU(HSE) startup time.
4. tSU(HSE) is the startup time measured from the moment it is enabled (by software) to a stabilized 8 MHz oscillation is reached. This value is measured for a standard crystal resonator and it can vary significantly with the crystal manufacturer.

For CL1 and CL2, it is recommended to use high-quality external ceramic capacitors in the 5 pF to 25 pF range (typ.), designed for high-frequency applications, and selected to match the requirements of the crystal or resonator (see [*Figure 16*](#_bookmark179)). CL1 and CL2 are usually the same size. The crystal manufacturer typically specifies a load capacitance which is the series combination of CL1 and CL2. PCB and MCU pin capacitance must be included (10 pF can be used as a rough estimate of the combined pin and board capacitance) when sizing CL1 and CL2.

*Note: For information on selecting the crystal, refer to the application note AN2867 “Oscillator design guide for ST microcontrollers” available from the ST website* [*www.st.com.*](http://www.st.com/)

###### Figure 16. Typical application with an 8 MHz crystal



MS19876V1

OSC\_OUT

REXT (1)

CL2

Bias

RF controlled gain

8 MHz

resonator

fHSE

OSC\_IN

Resonator with integrated capacitors

CL1

1. REXT value depends on the crystal characteristics.

##### Low-speed external clock generated from a crystal/ceramic resonator

The low-speed external (LSE) clock can be supplied with a 32.768 kHz crystal/ceramic resonator oscillator. All the information given in this paragraph are based on design simulation results obtained with typical external components specified in [*Table 43*](#_bookmark180). In the application, the resonator and the load capacitors have to be placed as close as possible to the oscillator pins in order to minimize output distortion and startup stabilization time. Refer to the crystal resonator manufacturer for more details on the resonator characteristics (frequency, package, accuracy).

###### Table 43. LSE oscillator characteristics (fLSE = 32.768 kHz)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions(1)** | **Min(2)** | **Typ** | **Max(2)** | **Unit** |
| IDD | LSE current consumption | LSEDRV[1:0]=00  lower driving capability | - | 0.5 | 0.9 | µA |
| LSEDRV[1:0]=01  medium low driving capability | - | - | 1 |
| LSEDRV[1:0]=10  medium high driving capability | - | - | 1.3 |
| LSEDRV[1:0]=11  higher driving capability | - | - | 1.6 |
| gm | Oscillator transconductance | LSEDRV[1:0]=00  lower driving capability | 5 | - | - | µA/V |
| LSEDRV[1:0]=01  medium low driving capability | 8 | - | - |
| LSEDRV[1:0]=10  medium high driving capability | 15 | - | - |
| LSEDRV[1:0]=11  higher driving capability | 25 | - | - |
| tSU(LSE)(3) | Startup time | VDD is stabilized | - | 2 | - | s |

1. Refer to the note and caution paragraphs below the table, and to the application note AN2867 “Oscillator design guide for ST microcontrollers”.
2. Guaranteed by design.
3. tSU(LSE) is the startup time measured from the moment it is enabled (by software) to a stabilized 32.768 kHz oscillation is reached. This value is measured for a standard crystal and it can vary significantly with the crystal manufacturer.

*Note: For information on selecting the crystal, refer to the application note AN2867 “Oscillator design guide for ST microcontrollers” available from the ST website* [*www.st.com.*](http://www.st.com/)

###### Figure 17. Typical application with a 32.768 kHz crystal



MS3O253V2

CL2

OSC32\_OUT

Drive programmable amplifier

32.768 kHz

resonator

fLSE

OSC32\_IN

Resonator with integrated capacitors

CL1

*Note: An external resistor is not required between OSC32\_IN and OSC32\_OUT and it is forbidden to add one.*

#### Internal clock source characteristics

The parameters given in [*Table 44*](#_bookmark184)are derived from tests performed under ambient temperature and supply voltage conditions summarized in [*Table 24*](#_bookmark130).

##### High-speed internal (HSI) RC oscillator

###### Table 44. HSI oscillator characteristics(1)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| fHSI | Frequency | - | - | 8 | - | MHz |
| TRIM | HSI user trimming step | - | - | - | 1(2) | % |
| DuCy(HSI) | Duty cycle | - | 45(2) | - | 55(2) | % |
| ACCHSI | Accuracy of the HSI oscillator | TA = -40 to 105°C | -2.8(3) | - | 3.8[(3)](#_bookmark186) | % |
| TA = -10 to 85°C | -1.9[(3)](#_bookmark186) | - | 2.3[(3)](#_bookmark186) |
| TA = 0 to 85°C | -1.9[(3)](#_bookmark186) | - | 2[(3)](#_bookmark186) |
| TA = 0 to 70°C | -1.3[(3)](#_bookmark186) | - | 2[(3)](#_bookmark186) |
| TA = 0 to 55°C | -1[(3)](#_bookmark186) | - | 2[(3)](#_bookmark186) |
| TA = 25°C(4) | -1 | - | 1 |
| tsu(HSI) | HSI oscillator startup time | - | 1(2) | - | 2(2) | µs |
| IDDA(HSI) | HSI oscillator power consumption | - | - | 80 | 100(2) | µA |

* + - 1. VDDA = 3.3 V, TA = –40 to 105 °C unless otherwise specified.
      2. Guaranteed by design.
      3. Guaranteed by characterization results.
      4. Factory calibrated, parts not soldered.

**Figure 18.** **HSI oscillator accuracy characterization results for soldered parts**



4%

3%

0

-2%

-3%

-4%

TA[ºc]

120

100

80

60

40

20

MS3O985V4

-20

2%

1%

0%

-40

-1%

MAX

MIN

##### Low-speed internal (LSI) RC oscillator

###### Table 45. LSI oscillator characteristics(1)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Min** | **Typ** | **Max** | **Unit** |
| fLSI | Frequency | 30 | 40 | 50 | kHz |
| tsu(LSI)(2) | LSI oscillator startup time | - | - | 85 | µs |
| (2)  IDD(LSI) | LSI oscillator power consumption | - | 0.75 | 1.2 | µA |

1. VDDA = 3.3 V, TA = –40 to 105 °C unless otherwise specified.
2. Guaranteed by design.

#### PLL characteristics

The parameters given in [*Table 46*](#_bookmark191)are derived from tests performed under ambient temperature and supply voltage conditions summarized in [*Table 24*](#_bookmark130).

###### Table 46. PLL characteristics

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Value** | | | **Unit** |
| **Min** | **Typ** | **Max** |
| fPLL\_IN | PLL input clock(1) | 1(2) | - | 24(2) | MHz |
| PLL input clock duty cycle | 40(2) | - | 60(2) | % |
| fPLL\_OUT | PLL multiplier output clock | 16(2) | - | 72 | MHz |
| tLOCK | PLL lock time | - | - | 200(2) | µs |
| Jitter | Cycle-to-cycle jitter | - | - | 300(2) | ps |

* + - 1. Take care of using the appropriate multiplier factors so as to have PLL input clock values compatible with the range defined by fPLL\_OUT.
      2. Guaranteed by design.

#### Memory characteristics

##### Flash memory

The characteristics are given at TA = –40 to 105 °C unless otherwise specified.

###### Table 47. Flash memory characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max(1)** | **Unit** |
| tprog | 16-bit programming time | TA  –40 to +105 °C | 40 | 53.5 | 60 | µs |
| tERASE | Page (2 KB) erase time | TA  –40 to +105 °C | 20 | - | 40 | ms |
| tME | Mass erase time | TA  –40 to +105 °C | 20 | - | 40 | ms |
| IDD | Supply current | Write mode | - | - | 10 | mA |
| Erase mode | - | - | 12 | mA |

* + - 1. Guaranteed by design.

###### Table 48. Flash memory endurance and data retention

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Value** | **Unit** |
| **Min(1)** |
| NEND | Endurance | TA = –40 to +85 °C (6 suffix versions)  TA = –40 to +105 °C (7 suffix versions) | 10 | kcycles |
| tRET | Data retention | 1 kcycle(2) at TA = 85 °C | 30 | Years |
| 1 kcycle(2) at TA = 105 °C | 10 |
| 10 kcycles(2) at TA = 55 °C | 20 |

1. Guaranteed by characterization results.
2. Cycling performed over the whole temperature range.

#### EMC characteristics

Susceptibility tests are performed on a sample basis during device characterization.

##### Functional EMS (electromagnetic susceptibility)

While a simple application is executed on the device (toggling 2 LEDs through I/O ports). the device is stressed by two electromagnetic events until a failure occurs. The failure is indicated by the LEDs:

* **Electrostatic discharge (ESD)** (positive and negative) is applied to all device pins until a functional disturbance occurs. This test is compliant with the IEC 61000-4-2 standard.
* **FTB**: A Burst of Fast Transient voltage (positive and negative) is applied to VDD and VSS through a 100 pF capacitor, until a functional disturbance occurs. This test is compliant with the IEC 61000-4-4 standard.

A device reset allows normal operations to be resumed.

The test results are given in [*Table 49*](#_bookmark197). They are based on the EMS levels and classes defined in the application note AN1709.

**Table 49. EMS characteristics**

|  |  |  |  |
| --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Level/ Class** |
| VFESD | Voltage limits to be applied on any I/O pin to induce a functional disturbance | VDD = 3.3 V, LQFP100, TA = +25°C, fHCLK = 72 MHz  conforms to IEC 61000-4-2 | 3B |
| VEFTB | Fast transient voltage burst limits to be applied through 100 pF on VDD and VSS pins to induce a functional disturbance | VDD = 3.3 V, LQFP100, TA = +25°C, fHCLK = 72 MHz  conforms to IEC 61000-4-4 | 4A |

##### Designing hardened software to avoid noise problems

EMC characterization and optimization are performed at component level with a typical application environment and simplified MCU software. It should be noted that good EMC performance is highly dependent on the user application and the software in particular.

Therefore it is recommended that the user applies EMC software optimization and prequalification tests in relation with the EMC level requested for his application.

###### Software recommendations

The software flowchart must include the management of runaway conditions such as:

* Corrupted program counter
* Unexpected reset
* Critical Data corruption (control registers...)

###### Prequalification trials

Most of the common failures (unexpected reset and program counter corruption) can be reproduced by manually forcing a low state on the NRST pin or the Oscillator pins for 1 second.

To complete these trials, ESD stress can be applied directly on the device, over the range of specification values. When unexpected behavior is detected, the software can be hardened to prevent unrecoverable errors occurring (see application note AN1015).

##### Electromagnetic Interference (EMI)

The electromagnetic field emitted by the device are monitored while a simple application is executed (toggling 2 LEDs through the I/O ports). This emission test is compliant with

IEC 61967-2 standard which specifies the test board and the pin loading.

**Table 50.** **EMI characteristics**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Monitored frequency band** | **Max vs. [fHSE/fHCLK]** | **Unit** |
| **8/72 MHz** |
|  |  | VDD  3.6 V, TA  25 °C, | 0.1 to 30 MHz | **7** | dBµV |
| 30 to 130 MHz | **20** |
| SEMI | Peak level | LQFP100 package  compliant with IEC |
| 130 MHz to 1GHz | **27** |
|  |  | 61967-2 |
| SAE EMI Level | **4** | - |

#### Electrical sensitivity characteristics

Based on three different tests (ESD, LU) using specific measurement methods, the device is stressed in order to determine its performance in terms of electrical sensitivity.

##### Electrostatic discharge (ESD)

Electrostatic discharges (a positive then a negative pulse separated by 1 second) are applied to the pins of each sample according to each pin combination. The sample size depends on the number of supply pins in the device (3 parts × (n+1) supply pins). This test conforms to the JESD22-A114/C101 standard.

###### Table 51. ESD absolute maximum ratings

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Ratings** | **Conditions** | **Class** | **Maximum value(1)** | **Unit** |
| VESD(HBM) | Electrostatic discharge voltage (human body model) | TA  +25 °C, conforming to JESD22-A114 | 2 | 2000 | V |
| VESD(CDM) | Electrostatic discharge voltage (charge device model) | TA  +25 °C, conforming to ANSI/ESD STM5.3.1 | II | 500 |

* + - 1. Guaranteed by characterization results.

##### Static latch-up

Two complementary static tests are required on six parts to assess the latch-up performance:

* + - * + A supply overvoltage is applied to each power supply pin
        + A current injection is applied to each input, output and configurable I/O pin These tests are compliant with EIA/JESD 78A IC latch-up standard.

**Table 52.** **Electrical sensitivities**

|  |  |  |  |
| --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Class** |
| LU | Static latch-up class | TA  +105 °C conforming to JESD78A | II level A |

#### I/O current injection characteristics

As a general rule, current injection to the I/O pins, due to external voltage below VSS or above VDD (for standard, 3 V-capable I/O pins) should be avoided during normal product operation. However, in order to give an indication of the robustness of the microcontroller in cases when abnormal injection accidentally happens, susceptibility tests are performed on a sample basis during device characterization.

##### Functional susceptibility to I/O current injection

While a simple application is executed on the device, the device is stressed by injecting current into the I/O pins programmed in floating input mode. While current is injected into the I/O pin, one at a time, the device is checked for functional failures.

The failure is indicated by an out of range parameter: ADC error above a certain limit (higher than 5 LSB TUE), out of conventional limits of induced leakage current on adjacent pins (out of –5 µA/+0 µA range), or other functional failure (for example reset occurrence or oscillator frequency deviation).

The test results are given in [*Table 53*](#_bookmark206).

##### Table 53. I/O current injection susceptibility

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Symbol** | **Description** | **Functional susceptibility** | | **Unit** |
| **Negative injection** | **Positive injection** |
| IINJ | Injected current on BOOT0 | – 0 | NA | mA |
| Injected current on PC0, PC1, PC2, PC3, PF2, PA0, PA1, PA2, PA3, PF4, PA4, PA5, PA6, PA7, PC4, PC5,  PB2 with induced leakage current on other pins from this group less than -50 µA | – 5 | - |
| Injected current on PB0, PB1, PE7, PE8, PE9, PE10, PE11, PE12, PE13, PE14, PE15, PB12, PB13, PB14, PB15, PD8, PD9, PD10, PD11, PD12, PD13, PD14 with  induced leakage current on other pins from this group less than -50 µA | – 5 | - |
| Injected current on PC0, PC1, PC2, PC3, PF2, PA0, PA1, PA2, PA3, PF4, PA4, PA5, PA6, PA7, PC4, PC5, PB2, PB0, PB1, PE7, PE8, PE9, PE10, PE11, PE12, PE13, PE14, PE15, PB12, PB13, PB14, PB15, PD8, PD9, PD10, PD11, PD12, PD13, PD14 with induced  leakage current on other pins from this group less than 400 µA | - | +5 |
| Injected current on any other FT and FTf pins | – 5 | NA |
| Injected current on any other pins | – 5 | +5 |

*Note: It is recommended to add a Schottky diode (pin to ground) to analog pins which may potentially inject negative currents.*

#### I/O port characteristics

##### General input/output characteristics

Unless otherwise specified, the parameters given in [*Table 54*](#_bookmark210)are derived from tests performed under the conditions summarized in [*Table 24*](#_bookmark130). All I/Os are CMOS and TTL compliant.

###### Table 54. I/O static characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| VIL | Low level input voltage | TC and TTa I/O | - | - | 0.3 VDD+0.07 (1) | V |
| FT and FTf I/O | - | - | 0.475 VDD-0.2 (1) |
| BOOT0 | - | - | 0.3 VDD–0.3 (1) |
| All I/Os except BOOT0 | - | - | 0.3 VDD (2) |
| VIH | High level input voltage | TC and TTa I/O | 0.445 VDD+0.398 (1) | - | - |
| FT and FTf I/O | 0.5 VDD+0.2 (1) | - | - |
| BOOT0 | 0.2 VDD+0.95 (1) | - | - |
| All I/Os except BOOT0 | 0.7 VDD (2) | - | - |
| Vhys | Schmitt trigger hysteresis | TC and TTa I/O | - | 200 (1) | - | mV |
| FT and FTf I/O | - | 100 (1) | - |
| BOOT0 | - | 300 (1) | - |
| Ilkg | Input leakage current (3) | TC, FT and FTf I/O TTa I/O in digital mode  VSS  VIN  VDD | - | - | ±0.1 | µA |
| TTa I/O in digital mode  VDD  VIN  VDDA | - | - | 1 |
| TTa I/O in analog mode  VSS  VIN  VDDA | - | - | ±0.2 |
| FT and FTf I/O(4) VDD  VIN  5 V | - | - | 10 |
| RPU | Weak pull-up equivalent resistor(5) | VIN  VSS | 25 | 40 | 55 | k |
| RPD | Weak pull-down equivalent resistor(5) | VIN  VDD | 25 | 40 | 55 | k |
| CIO | I/O pin capacitance | - | - | 5 | - | pF |

1. Data based on design simulation.
2. Tested in production.
3. Leakage could be higher than the maximum value. if negative current is injected on adjacent pins. Refer to [*Table 53: I/O*](#_bookmark206)[*current injection susceptibility*](#_bookmark206).
4. To sustain a voltage higher than VDD +0.3 V, the internal pull-up/pull-down resistors must be disabled.
5. Pull-up and pull-down resistors are designed with a true resistance in series with a switchable PMOS/NMOS. This PMOS/NMOS contribution to the series resistance is minimum (~10% order).

All I/Os are CMOS and TTL compliant (no software configuration required). Their characteristics cover more than the strict CMOS-technology or TTL parameters. The coverage of these requirements is shown in [*Figure 19*](#_bookmark212)and [*Figure 20*](#_bookmark213)for standard I/Os.

**Figure 19. TC and TTa I/O input characteristics - CMOS port**



MS3O255V2

3.6

3.3

3.O

2.7

2.O

VDD (V)

O.6

CMOS standard requirements VILmax = O.3VDD

VILmax O.7

Area not determined

1.3

VIHmin 2.O

VIL/VIH (V)

Based on design simulations

Based on design simulations

V = O.445V +O.398

V = O.3V +O.O7

IHmin

DD

ILmax

DD

CMOS standard requirements V

IHmin

= O.7 V

DD

Tested in production

**Figure 20. TC and TTa I/O input characteristics - TTL port**



MS3O256V2

3.6

3.3

3.O

2.7

2.O

VDD (V)

TTL standard requirements VILmax = O.8 V

O.7

VILmax O.8

Area not determined

1.3

TTL standard requirements VIHmin = 2 V

VIHmin 2.O

VIL/VIH (V)

Based on design simulations

Based on design simulations

V = O.445V +O.398

V = O.3V +O.O7

IHmin

DD

DD

ILmax

Tested in production

**Figure 21. Five volt tolerant (FT and FTf) I/O input characteristics - CMOS port**



VIL/VIH (V)

2.O

1.O

Area not determined

CMOS standard requirements VILmax = O.3VDD

O.5

VDD (V)

2.O

3.6

MS3O257V2

Based on design simulations

Based on design simulations

V = O.5V +O.2

V = O.475V -O.2

IHmin

DD

DD

ILmax

CMOS standard requirements V

IHmin

= O.7 V

DD

Tested in production

**Figure 22. Five volt tolerant (FT and FTf) I/O input characteristics - TTL port**



VIL/VIH (V)

2.O

TTL standard requirements VIHmin = 2 V

Area not determined

1.O

O.8

TTL standard requirements VILmax = O.8 V

O.5

VDD (V)

2.O

2.7

3.6

MS3O258V2

Based on design simulations

Based on design simulations

V = O.5V +O.2

V = O.475V -O.2

IHmin

DD

DD

ILmin

Tested in production

##### Output driving current

The GPIOs (general purpose input/outputs) can sink or source up to +/-8 mA, and sink or source up to +/- 20 mA (with a relaxed VOL/VOH).

In the user application, the number of I/O pins which can drive current must be limited to respect the absolute maximum rating specified in [*Section 6.2*](#_bookmark122):

* The sum of the currents sourced by all the I/Os on VDD, plus the maximum Run consumption of the MCU sourced on VDD, cannot exceed the absolute maximum rating

IVDD (see [*Table 22*](#_bookmark125)).

* The sum of the currents sunk by all the I/Os on VSS plus the maximum Run consumption of the MCU sunk on VSS cannot exceed the absolute maximum rating

IVSS (see [*Table 22*](#_bookmark125)).

##### Output voltage levels

Unless otherwise specified, the parameters given in [*Table 55*](#_bookmark217)are derived from tests performed under ambient temperature and VDD supply voltage conditions summarized in [*Table 24*](#_bookmark130). All I/Os (FT, TTa and TC unless otherwise specified) are CMOS and TTL compliant.

###### Table 55. Output voltage characteristics

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Max** | **Unit** |
| VOL(1) | Output low level voltage for an I/O pin | CMOS port(2) IIO = +8 mA  2.7 V < VDD < 3.6 V | - | 0.4 | V |
| VOH(3) | Output high level voltage for an I/O pin | VDD–0.4 | - |
| VOL (1) | Output low level voltage for an I/O pin | TTL port(2) IIO = +8 mA  2.7 V < VDD < 3.6 V | - | 0.4 |
| VOH (3) | Output high level voltage for an I/O pin | 2.4 | - |
| V (1)(4) OL | Output low level voltage for an I/O pin | IIO = +20 mA  2.7 V < VDD < 3.6 V | - | 1.3 |
| V (3)(4) OH | Output high level voltage for an I/O pin | VDD–1.3 | - |
| V (1)(4) OL | Output low level voltage for an I/O pin | IIO = +6 mA  2 V < VDD < 2.7 V | - | 0.4 |
| V (3)(4) OH | Output high level voltage for an I/O pin | VDD–0.4 | - |
| V (1)(4)  OLFM+ | Output low level voltage for an FTf I/O pin in FM+ mode | IIO = +20 mA  2.7 V < VDD < 3.6 V | - | 0.4 |

1. The IIO current sunk by the device must always respect the absolute maximum rating specified in [*Table 22*](#_bookmark125)and the sum of IIO (I/O ports and control pins) must not exceed IIO(PIN).
2. TTL and CMOS outputs are compatible with JEDEC standards JESD36 and JESD52.
3. The IIO current sourced by the device must always respect the absolute maximum rating specified in [*Table 22*](#_bookmark125)and the sum of IIO (I/O ports and control pins) must not exceed IIO(PIN).
4. Data based on design simulation.

##### Input/output AC characteristics

The definition and values of input/output AC characteristics are given in [*Figure 23*](#_bookmark222)and

[*Table 56*](#_bookmark219), respectively.

Unless otherwise specified, the parameters given are derived from tests performed under ambient temperature and VDD supply voltage conditions summarized in [*Table 24*](#_bookmark130).

###### Table 56. I/O AC characteristics(1)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **OSPEEDRy [1:0]**  **value(1)** | **Symbol** | **Parameter** | **Conditions** | **Min** | **Max** | **Unit** |
| x0 | fmax(IO)out | Maximum frequency(2) | CL = 50 pF, VDD = 2 V to 3.6 V | - | 2(3) | MHz |
| tf(IO)out | Output high to low level fall time | CL = 50 pF, VDD = 2 V to 3.6 V | - | 125(3) | ns |
| tr(IO)out | Output low to high level rise time | - | 125(3) |
| 01 | fmax(IO)out | Maximum frequency(2) | CL = 50 pF, VDD = 2 V to 3.6 V | - | 10(3) | MHz |
| tf(IO)out | Output high to low level fall time | CL = 50 pF, VDD = 2 V to 3.6 V | - | 25(3) | ns |
| tr(IO)out | Output low to high level rise time | - | 25(3) |
| 11 | fmax(IO)out | Maximum frequency(2) | CL = 30 pF, VDD = 2.7 V to 3.6 V | - | 50(3) | MHz |
| CL = 50 pF, VDD = 2.7 V to 3.6 V | - | 30(3) | MHz |
| CL = 50 pF, VDD = 2 V to 2.7 V | - | 20(3) | MHz |
| tf(IO)out | Output high to low level fall time | CL = 30 pF, VDD = 2.7 V to 3.6 V | - | 5(3) | ns |
| CL = 50 pF, VDD = 2.7 V to 3.6 V | - | 8(3) |
| CL = 50 pF, VDD = 2 V to 2.7 V | - | 12(3) |
| tr(IO)out | Output low to high level rise time | CL = 30 pF, VDD = 2.7 V to 3.6 V | - | 5(3) |
| CL = 50 pF, VDD = 2.7 V to 3.6 V | - | 8(3) |
| CL = 50 pF, VDD = 2 V to 2.7 V | - | 12(3) |
| FM+  configuration(4) | fmax(IO)out | Maximum frequency(2) | CL = 50 pF, VDD = 2 V to 3.6 V | - | 2[(4)](#_bookmark221) | MHz |
| tf(IO)out | Output high to low level fall time | - | 12[(4)](#_bookmark221) | ns |
| tr(IO)out | Output low to high level rise time | - | 34[(4)](#_bookmark221) |
| - | tEXTIpw | Pulse width of external signals detected by the EXTI controller | - | 10(3) | - | ns |

1. The I/O speed is configured using the OSPEEDRx[1:0] bits. Refer to the RM0316 reference manual for a description of GPIO Port configuration register.
2. The maximum frequency is defined in [*Figure 23*](#_bookmark222).
3. Guaranteed by design.
4. The I/O speed configuration is bypassed in FM+ I/O mode. Refer to the STM32F303x STM32F313xx reference manual RM0316 for a description of FM+ I/O mode configuration.

**Figure 23. I/O AC characteristics definition**

ai14131c

Maximum frequency is achieved if (tr + tf) ≤ 2/3)T and if the duty cycle is (45-55%)

when loaded by 5OpF

T

tf(IO)out

tr(IO)out

EXTERNAL OUTPUT

ON 5OpF

9O%

1O%

5O% 5O%

1O%

9O%

#### NRST pin characteristics

The NRST pin input driver uses CMOS technology. It is connected to a permanent pull-up resistor, RPU (see [*Table 54*](#_bookmark210)).

Unless otherwise specified, the parameters given in [*Table 57*](#_bookmark224)are derived from tests performed under ambient temperature and VDD supply voltage conditions summarized in [*Table 24*](#_bookmark130).

###### Table 57. NRST pin characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| VIL(NRST)(1) | NRST Input low level voltage | - | - | - | 0.3VDD+  0.07(1) | V |
| VIH(NRS (1)  T) | NRST Input high level voltage | - | 0.445VDD+  0.398(1) | - | - |
| Vhys(NRST) | NRST Schmitt trigger voltage hysteresis | - | - | 200 | - | mV |
| RPU | Weak pull-up equivalent resistor(2) | VIN  VSS | 25 | 40 | 55 | k |
| (1)  VF(NRST) | NRST Input filtered pulse | - | - | - | 100(1) | ns |
| (1)  VNF(NRST) | NRST Input not filtered pulse | - | 500(1) | - | - | ns |

1. Guaranteed by design.
2. The pull-up is designed with a true resistance in series with a switchable PMOS. This PMOS contribution to the series resistance must be minimum (~10% order).

###### Figure 24. Recommended NRST pin protection

VDD

RPU

Internal reset

Filter

External

reset circuitry (1)

NRST (2)

O.1 µF

MS19878V1

* 1. The reset network protects the device against parasitic resets.
  2. The user must ensure that the level on the NRST pin can go below the VIL(NRST) max level specified in

[*Table 57*](#_bookmark224). Otherwise the reset will not be taken into account by the device.

#### Timer characteristics

The parameters given in [*Table 58*](#_bookmark228)are guaranteed by design.

Refer to [*Section 6.3.14: I/O port characteristics*](#_bookmark208)for details on the input/output alternate function characteristics (output compare, input capture, external clock, PWM output).

###### Table 58. TIMx(1)(2) characteristics

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Max** | **Unit** |
| tres(TIM) | Timer resolution time | - | 1 | - | tTIMxCLK |
| fTIMxCLK = 72 MHz | 13.9 | - | ns |
| fTIMxCLK = 144 MHz x=1.8 | 6.95 | - | ns |
| fEXT | Timer external clock frequency on CH1 to CH4 | - | 0 | fTIMxCLK/2 | MHz |
| fTIMxCLK = 72 MHz | 0 | 36 | MHz |
| ResTIM | Timer resolution | TIMx (except TIM2) | - | 16 | bit |
| TIM2 | - | 32 |
| tCOUNTER | 16-bit counter clock period | - | 1 | 65536 | tTIMxCLK |
| fTIMxCLK = 72 MHz | 0.0139 | 910 | µs |
| fTIMxCLK = 144 MHz x=1.8 | 0.0069 | 455 | µs |
| tMAX\_COUNT | Maximum possible count with 32-bit counter | - | - | 65536 × 65536 | tTIMxCLK |
| fTIMxCLK = 72 MHz | - | 59.65 | s |
| fTIMxCLK = 144 MHz x=1.8 | - | 29.825 | s |

* + - 1. TIMx is used as a general term to refer to the TIM1, TIM2, TIM3, TIM4, TIM8, TIM15, TIM16 and TIM17 timers.
      2. Guaranteed by design.

###### Table 59. IWDG min/max timeout period at 40 kHz (LSI) (1)

|  |  |  |  |
| --- | --- | --- | --- |
| **Prescaler divider** | **PR[2:0] bits** | **Min timeout (ms) RL[11:0]= 0x000** | **Max timeout (ms) RL[11:0]= 0xFFF** |
| /4 | 0 | 0.1 | 409.6 |
| /8 | 1 | 0.2 | 819.2 |
| /16 | 2 | 0.4 | 1638.4 |
| /32 | 3 | 0.8 | 3276.8 |
| /64 | 4 | 1.6 | 6553.6 |
| /128 | 5 | 3.2 | 13107.2 |
| /256 | 7 | 6.4 | 26214.4 |

1. These timings are given for a 40 kHz clock but the microcontroller’s internal RC frequency can vary from 30 to 60 kHz. Moreover, given an exact RC oscillator frequency, the exact timings still depend on the phasing of the APB interface clock versus the LSI clock so that there is always a full RC period of uncertainty.

###### Table 60. WWDG min-max timeout value @72 MHz (PCLK)(1)

|  |  |  |  |
| --- | --- | --- | --- |
| **Prescaler** | **WDGTB** | **Min timeout value** | **Max timeout value** |
| 1 | 0 | 0.05687 | 3.6409 |
| 2 | 1 | 0.1137 | 7.2817 |
| 4 | 2 | 0.2275 | 14.564 |
| 8 | 3 | 0.4551 | 29.127 |

1. Guaranteed by design.

#### Communications interfaces

##### I2C interface characteristics

The I2C interface meets the timings requirements of the I2C-bus specification and user manual rev.03 for:

* Standard-mode (Sm) : with a bit rate up to 100 Kbits/s
* Fast-mode (Fm) : with a bit rate up to 400 Kbits/s
* Fast-mode Plus (Fm+) : with a bit rate up to 1Mbits/s

The I2C timings requirements are guaranteed by design when the I2C peripheral is properly configured (refer to Reference manual).

The SDA and SCL I/O requirements are met with the following restrictions: the SDA and SCL I/O pins are “true” open-drain. When configured as open-drain, the PMOS connected between the I/O pin and VDDIOx is disabled, but is still present. Only FTf I/O pins support Fm+ low level output current maximum requirement. Refer to [*Section 6.3.14: I/O port*](#_bookmark208)[*characteristics*](#_bookmark208).

All I2C I/Os embed an analog filter. refer to the[*Table 62: I2C analog filter characteristics*](#_bookmark236).

###### Table 61. I2C timings specification (see I2C specification, rev.03, June 2007)(1)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Standard mode** | | **Fast mode** | | **Fast Mode Plus** | | **Unit** |
| **Min** | **Max** | **Min** | **Max** | **Min** | **Max** |
| **fSCL** | SCL clock frequency | 0 | 100 | 0 | 400 | 0 | 1000 | KHz |
| **tLOW** | Low period of the SCL clock | 4.7 | - | 1.3 | - | 0.5 | - | µs |
| **tHIGH** | High Period of the SCL clock | 4 |  | 0.6 |  | 0.26 | - | µs |
| **tr** | Rise time of both SDA and SCL signals | - | 1000 | - | 300 | - | 120 | ns |
| **tf** | Fall time of both SDA and SCL signals | - | 300 | - | 300 | - | 120 | ns |
| **tHD;DAT** | Data hold time | 0 | - | 0 | - | 0 | - | µs |
| **tVD;DAT** | Data valid time | - | 3.45(2) | - | 0.9(2) | - | 0.45(2) | µs |
| **tVD;ACK** | Data valid acknowledge time | - | 3.45(2) | - | 0.9(2) | - | 0.45(2) | µs |
| **tSU;DAT** | Data setup time | 250 | - | 100 | - | 50 | - | ns |
| **tHD:STA** | Hold time (repeated) START condition | 4.0 | - | 0.6 | - | 0.26 | - | µs |
| **tSU:STA** | Set-up time for a repeated START condition | 4.7 | - | 0.6 | - | 0.26 |  | µs |
| **tSU:STO** | Set-up time for STOP condition | 4.0 | - | 0.6 | - | 0.26 | - | µs |
| **tBUF** | Bus free time between a STOP and START condition | 4.7 | - | 1.3 | - | 0.5 | - | µs |
| **Cb** | Capacitive load for each bus line | - | 400 | - | 400 | - | 550 | pF |
| **tSP** | Pulse width of spikes that are suppressed by the analog filter for Standard and Fast mode | 0 | 50(3) | 0 | 50(3) | - | - | ns |

1. The I2C characteristics are the requirements from I2C bus specification rev03. They are guaranteed by design when I2Cx\_TIMING register is correctly programmed (Refer to the RM0316 reference manual).
2. The maximum tHD;DAT could be 3.45 µs, 0.9 µs and 0.45 µs for standard mode, fast mode and fast mode plus, but must be less than the maximum of tVD;DAT or tVD;ACK by a transition time.
3. The minimum width of the spikes filtered by the analog filter is above tSP(max).

###### Table 62. I2C analog filter characteristics(1)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Min** | **Max** | **Unit** |
| tAF | Pulse width of spikes that are suppressed by the analog filter | 50 | 260 | ns |

* 1. Guaranteed by design.

###### Figure 25. I2C bus AC waveforms and measurement circuit



tBUF

P

**MCU**

SDA SCL

70%

30%

MS19879V3

70%

30%

continued

tHD;STA S

1 / fScL

1st clock cycle

tLOW

9th clock

S

SDA

tSU;STA tHD;STA

tSP

tVD;AcK

tSU;STO

ScL

Sr

9th clock

tf

tr

tSU;DAT

VDD\_I2C

VDD\_I2C

Rp

Rp

Rs

I2C bus

Rs

tVD;DAT

ScL

70%

30%

70%

SDA 30%

70%

30%

tHD;DAT

70%

30%

continued

tf

tr

tHIGH

1. Rs: Series protection resistors, Rp: Pull-up resistors, VDD\_I2C: I2C bus supply.

##### SPI/I2S characteristics

Unless otherwise specified, the parameters given in [*Table 63*](#_bookmark240)for SPI or in [*Table 64*](#_bookmark245)for I2S are derived from tests performed under ambient temperature, fPCLKx frequency and VDD supply voltage conditions summarized in [*Table 24*](#_bookmark130).

Refer to [*Section 6.3.14: I/O port characteristics*](#_bookmark208)for more details on the input/output alternate function characteristics (NSS, SCK, MOSI, MISO for SPI and WS, CK, SD for I2S).

###### Table 63. SPI characteristics(1)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| fSCK  1/tc(SCK) | SPI clock frequency | Master mode, SPI1 2.7<VDD<3.6 | - | - | 24 | MHz |
| Slave mode, SPI1 2.7<VDD<3.6 | 24 |
| Master mode, SPI1/2/3 2<VDD<3.6 | 18 |
| Slave mode, SPI1/2/3 2<VDD<3.6 | 18 |
| DuCy(SCK) | Duty cycle of SPI clock frequency | Slave mode | 30 | 50 | 70 | % |
| tsu(NSS) | NSS setup time | Slave mode, SPI presc = 2 | 4\*Tpclk | - | - | ns |
| th(NSS) | NSS hold time | Slave mode, SPI presc = 2 | 2\*Tpclk | - | - |
| tw(SCKH) tw(SCKL) | SCK high and low time | Master mode | Tpclk-2 | Tpclk | Tpclk+2 |
| tsu(MI) | Data input setup time | Master mode | 5.5 | - | - |
| tsu(SI) | Slave mode | 6.5 | - | - |
| th(MI) | Data input hold time | Master mode | 5 | - | - |
| th(SI) | Slave mode | 5 | - | - |
| ta(SO) | Data output access time | Slave mode | 0 | - | 4\*Tpclk |
| tdis(SO) | Data output disable time | Slave mode | 0 | - | 24 |
| tv(SO) | Data output valid time | Slave mode | - | 12 | 27 |
| Slave mode, SPI1 2.7<VDD<3.6V | - | 12 | 18 |
| tv(MO) | Master mode | - | 1.5 | 3 |
| th(SO) | Data output hold time | Slave mode | 11 | - | - |
| th(MO) | Master mode | 0 | - | - |

1. Guaranteed by characterization results.

###### Figure 26. SPI timing diagram - slave mode and CPHA = 0

ai14134c

LSB IN

BIT1 IN

MSB IN

th(SI)

LSB OUT

BIT6 OUT

MSB OUT

MISO

OUTPUT

tsu(SI)

MOSI INPUT

tdis(SO)

tf(SCK)

tr(SCK)

th(SO)

tV(SO)

a(SO)

t

tw(SCKH) tw(SCKL)

CPHA=O CPOL=O

CPHA=O CPOL=1

th(NSS)

tc(SCK)

NSS input

tSU(NSS)

SCK Input

**Figure 27. SPI timing diagram - slave mode and CPHA = 1(1)**

ai14135

LSB IN

BIT1 IN

LSB OUT

BI T6 OUT

MS B O UT

th(SI)

M SB IN

MOSI

INPUT

tsu(SI)

MISO OUT PUT

tdis(SO)

tr(SCK) tf(SCK)

th(SO)

tv(SO)

a(SO)

t

tw(SCKH) tw(SCKL)

CPHA=1 CPOL=O

CPHA=1 CPOL=1

th(NSS)

tc(SC~~K)~~

tSU(NSS)

NSS input

SCK Input

1. Measurement points are done at 0.5VDD and with external CL = 30 pF.

###### Figure 28. SPI timing diagram - master mode(1)

High

NSS input

tc(SC~~K)~~

CPHA= O CPOL=O

CPHA= O CPOL=1

CPHA=1 CPOL=O

CPHA=1 CPOL=1

tsu(MI)

MISO

INP UT

tw(SCKH) tw(SCKL)

MSB IN

th(MI)

MSB OUT

tv(MO)

BIT6 IN

tr(SCK) tf(SCK)

LSB IN

MOSI

OUTPUT

B IT1 OUT

th(MO)

LSB OUT

ai14136c

SCK Output

SCK Output

1. Measurement points are done at 0.5VDD and with external CL = 30 pF.

###### Table 64. I2S characteristics(1)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Max** | **Unit** |
| fCK 1/tc(CK) | I2S clock frequency | Master data: 16 bits, audio freq=48 kHz | 1.496 | 1.503 | MHz |
| Slave | 0 | 12.288 |
| tr(CK)  tf(CK) | I2S clock rise and fall time | Capacitive load CL = 30 pF | - | 8 | ns |
| tw(CKH) | I2S clock high time | Master fPCLK= 36 MHz, audio frequency =  48 kHz | 331 | - |
| tw(CKL) | I2S clock low time | 332 | - |
| tv(WS) | WS valid time | Master mode | 4 | - |
| th(WS) | WS hold time | Master mode | 4 | - |
| tsu(WS) | WS setup time | Slave mode | 4 | - |
| th(WS) | WS hold time | Slave mode | 0 | - |
| Duty Cycle | I2S slave input clock duty cycle | Slave mode | 30 | 70 | % |
| tsu(SD\_MR) | Data input setup time | Master receiver | 9 | - | ns |
| tsu(SD\_SR) | Data input setup time | Slave receiver | 2 | - |
| th(SD\_MR) | Data input hold time | Master receiver | 0 | - |
| th(SD\_SR) | Slave receiver | 0 | - |
| tv(SD\_ST) | Data output valid time | Slave transmitter (after enable edge) | - | 29 |
| th(SD\_ST) | Data output hold time | Slave transmitter (after enable edge) | 12 | - |
| tv(SD\_MT) | Data output valid time | Master transmitter (after enable edge) | - | 3 |
| th(SD\_MT) | Data output hold time | Master transmitter (after enable edge) | 2 | - |

* 1. Guaranteed by characterization results.

###### Figure 29. I2S slave timing diagram (Philips protocol)(1)

ai14881b

LSB receive

MSB receive

SDreceive

th(SD\_ST)

LSB transmit

tv(SD\_ST)

Bitn transmit th(SD\_SR)

Bitn receive

LSB transmit(2) MSB transmit

tsu(SD\_SR) LSB receive(2)

SDtransmit

tsu(WS)

WS input

th(WS)

tw(CKL)

tw(CKH)

CPOL = 1

CPOL = O

tc(CK)

CK Input

1. Measurement points are done at 0.5VDD and with external CL=30 pF.
2. LSB transmit/receive of the previously transmitted byte. No LSB transmit/receive is sent before the first byte.

###### Figure 30. I2S master timing diagram (Philips protocol)(1)

ai14884b

LSB receive

Bitn receive

LSB transmit(2)

tsu(SD\_MR)

LSB receive(2) MSB receive

SDreceive

th(SD\_MT)

LSB transmit

tv(SD\_MT)

MSB transmit Bitn transmit th(SD\_MR)

SDtransmit

WS output

th(WS)

tw(CKL)

tv(WS)

CPOL = 1

tw(CKH)

CPOL = O

tc(CK)

tr(CK)

tf(CK)

CK output

1. Measurement points are done at 0.5VDD and with external CL=30 pF.
2. LSB transmit/receive of the previously transmitted byte. No LSB transmit/receive is sent before the first byte.

##### USB characteristics

###### Table 65. USB startup time

|  |  |  |  |
| --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Max** | **Unit** |
| (1)  tSTARTUP | USB transceiver startup time | 1 | µs |

1. Guaranteed by design.

###### Table 66. USB DC electrical characteristics

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min.(1)** | **Max.(1)** | **Unit** |
| **Input levels** | | | | | |
| VDD | USB operating voltage(2) | - | 3.0(3) | 3.6 | V |
| (4)  VDI | Differential input sensitivity | I(USB\_DP, USB\_DM) | 0.2 | - | V |
| VCM(4) | Differential common mode range | Includes VDI range | 0.8 | 2.5 |
| (4)  VSE | Single ended receiver threshold | - | 1.3 | 2.0 |
| **Output levels** | | | | | |
| VOL | Static output level low | RL of 1.5 k to 3.6 V(5) | - | 0.3 | V |
| VOH | Static output level high | RL of 15 k to V (5)  SS | 2.8 | 3.6 |

1. All the voltages are measured from the local ground potential.
2. To be compliant with the USB 2.0 full-speed electrical specification, the USB\_DP (D+) pin should be pulled up with a 1.5 k resistor to a 3.0-to-3.6 V voltage range.
3. The STM32F303xB/STM32F303xC USB functionality is ensured down to 2.7 V but not the full USB electrical characteristics which are degraded in the 2.7-to-3.0 V VDD voltage range.
4. Guaranteed by design.
5. RL is the load connected on the USB drivers.

###### Figure 31. USB timings: definition of data signal rise and fall time

ai14137

tr

tf

Crossover points

Differential data lines

VCRS VSS

**Table 67. USB: Full-speed electrical characteristics(1)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| **Driver characteristics** | | | | | | |
| tr | Rise time(2) | CL = 50 pF | 4 | - | 20 | ns |
| tf | Fall time(2) | CL = 50 pF | 4 | - | 20 | ns |
| trfm | Rise/ fall time matching | tr/tf | 90 | - | 110 | % |
| VCRS | Output signal crossover voltage | - | 1.3 | - | 2.0 | V |
| Output driver Impedance(3) | ZDRV | driving high and low | 28 | 40 | 44 |  |

1. Guaranteed by design.
2. Measured from 10% to 90% of the data signal. For more detailed informations, please refer to USB Specification - Chapter 7 (version 2.0).
3. No external termination series resistors are required on USB\_DP (D+) and USB\_DM (D-), the matching impedance is already included in the embedded driver.

##### CAN (controller area network) interface

Refer to [*Section 6.3.14: I/O port characteristics*](#_bookmark208)for more details on the input/output alternate function characteristics (CAN\_TX and CAN\_RX).

#### ADC characteristics

Unless otherwise specified, the parameters given in [*Table 68*](#_bookmark254)to [*Table 70*](#_bookmark262)are guaranteed by design, with conditions summarized in [*Table 24*](#_bookmark130).

###### Table 68. ADC characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| VDDA | Analog supply voltage for ADC | - | 2 | - | 3.6 | V |
| IDDA | ADC current consumption on VDDA pin  (see [*Figure 32*](#_bookmark256)) | Single-ended mode, 5 MSPS | - | 907 | 1033.0 | µA |
| Single-ended mode, 1 MSPS | - | 194 | 285.5 |
| Single-ended mode, 200 KSPS | - | 51.5 | 70 |
| Differential mode, 5 MSPS | - | 887.5 | 1009 |
| Differential mode, 1 MSPS | - | 212 | 285 |
| Differential mode, 200 KSPS | - | 51 | 69.5 |
| VREF+ | Positive reference voltage | - | 2 | - | VDDA | V |
| VREF- | Negative reference voltage | - | - | 0 | - |
| IREF | ADC current consumption on VREF+ pin  (see [*Figure 33*](#_bookmark258)) | Single-ended mode, 5 MSPS | - | 104 | 139 | µA |
| Single-ended mode, 1 MSPS | - | 20.4 | 37 |
| Single-ended mode, 200 KSPS | - | 3.3 | 11.3 |
| Differential mode, 5 MSPS | - | 174 | 235 |
| Differential mode, 1 MSPS | - | 34.6 | 52.6 |
| Differential mode, 200 KSPS | - | 6 | 13.6 |
| fADC | ADC clock frequency | - | 0.14 | - | 72 | MHz |
| f (1) S | Sampling rate | Resolution = 12 bits, Fast Channel | 0.01 | - | 5.14 | MSPS |
| Resolution = 10 bits, Fast Channel | 0.012 | - | 6 |
| Resolution = 8 bits, Fast Channel | 0.014 | - | 7.2 |
| Resolution = 6 bits, Fast Channel | 0.0175 | - | 9 |

**Table 68. ADC characteristics (continued)**

104/146 DocID023353 Rev 12

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| fTRIG(1) | External trigger frequency | fADC = 72 MHz  Resolution = 12 bits | - | - | 5.14 | MHz |
| Resolution = 12 bits | - | - | 14 | 1/fADC |
| VAIN | Conversion voltage range(2) | - | 0 | - | VREF+ | V |
| (1)  RAIN | External input impedance | - | - | - | 100 | k |
| CADC(1) | Internal sample and hold capacitor | - | - | 5 | - | pF |
| (1)  tSTAB | Power-up time | - | 0 | 0 | 1 | µs |
| tCAL(1) | Calibration time | fADC = 72 MHz | 1.56 | | | µs |
| - | 112 | | | 1/fADC |
| tlatr(1) | Trigger conversion latency Regular and injected channels without conversion abort | CKMODE = 00 | 1.5 | 2 | 2.5 | 1/fADC |
| CKMODE = 01 | - | - | 2 | 1/fADC |
| CKMODE = 10 | - | - | 2.25 | 1/fADC |
| CKMODE = 11 | - | - | 2.125 | 1/fADC |
| tlatrinj(1) | Trigger conversion latency Injected channels aborting a regular conversion | CKMODE = 00 | 2.5 | 3 | 3.5 | 1/fADC |
| CKMODE = 01 | - | - | 3 | 1/fADC |
| CKMODE = 10 | - | - | 3.25 | 1/fADC |
| CKMODE = 11 | - | - | 3.125 | 1/fADC |
| t (1) S | Sampling time | fADC = 72 MHz | 0.021 | - | 8.35 | µs |
| - | 1.5 | - | 601.5 | 1/fADC |
| TADCVREG  (1)  \_STUP | ADC Voltage Regulator Start-up time | - | - | - | 10 | µs |
| tCONV(1) | Total conversion time (including sampling time) | fADC = 72 MHz  Resolution = 12 bits | 0.19 | - | 8.52 | µs |
| Resolution = 12 bits | 14 to 614 (tS for sampling + 12.5 for successive approximation) | | | 1/fADC |

1. Data guaranteed by design.
2. VREF+ can be internally connected to VDDA and VREF- can be internally connected to VSSA, depending on the package. Refer to [*Section 4: Pinouts and pin description*](#_bookmark85)for further details.

###### Figure 32. ADC typical current consumption on VDDA pin

1OOO

9OO

8OO

7OO

6OO

5OO

4OO

3OO

2OO

1OO

O

Single-ended mode

Differential mode

5 1 O.2

Clock frequency (MSPS)

MS366O7V1

ADC current consumption (µA)

**Figure 33.** **ADC typical current consumption on VREF+ pin**

2OO

18O

16O

14O

12O

1OO

8O

6O

4O

2O O

Single-ended mode

Differential mode

5

1

Clock frequency (MSPS)

O.2

MS366O6V1

ADC current consumption (µA)

**Ta****ble 69. Maximum ADC RAIN (1)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Resolution** | **Sampling cycle @ 72 MHz** | **Sampling time [ns] @ 72 MHz** | **RAIN max (k****)** | | |
| **Fast channels(2)** | **Slow channels** | **Other channels(3)** |
| 12 bits | 1.5 | 20.83 | 0.018 | NA | NA |
| 2.5 | 34.72 | 0.150 | NA | 0.022 |
| 4.5 | 62.50 | 0.470 | 0.220 | 0.180 |
| 7.5 | 104.17 | 0.820 | 0.560 | 0.470 |
| 19.5 | 270.83 | 2.70 | 1.80 | 1.50 |
| 61.5 | 854.17 | 8.20 | 6.80 | 4.70 |
| 181.5 | 2520.83 | 22.0 | 18.0 | 15.0 |
| 601.5 | 8354.17 | 82.0 | 68.0 | 47.0 |
| 10 bits | 1.5 | 20.83 | 0.082 | NA | NA |
| 2.5 | 34.72 | 0.270 | 0.082 | 0.100 |
| 4.5 | 62.50 | 0.560 | 0.390 | 0.330 |
| 7.5 | 104.17 | 1.20 | 0.82 | 0.68 |
| 19.5 | 270.83 | 3.30 | 2.70 | 2.20 |
| 61.5 | 854.17 | 10.0 | 8.2 | 6.8 |
| 181.5 | 2520.83 | 33.0 | 27.0 | 22.0 |
| 601.5 | 8354.17 | 100.0 | 82.0 | 68.0 |

###### Table 69. Maximum ADC RAIN (1) (continued)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Resolution** | **Sampling cycle @ 72 MHz** | **Sampling time [ns] @ 72 MHz** | **RAIN max (k****)** | | |
| **Fast channels(2)** | **Slow channels** | **Other channels(3)** |
| 8 bits | 1.5 | 20.83 | 0.150 | NA | 0.039 |
| 2.5 | 34.72 | 0.390 | 0.180 | 0.180 |
| 4.5 | 62.50 | 0.820 | 0.560 | 0.470 |
| 7.5 | 104.17 | 1.50 | 1.20 | 1.00 |
| 19.5 | 270.83 | 3.90 | 3.30 | 2.70 |
| 61.5 | 854.17 | 12.00 | 12.00 | 8.20 |
| 181.5 | 2520.83 | 39.00 | 33.00 | 27.00 |
| 601.5 | 8354.17 | 100.00 | 100.00 | 82.00 |
| 6 bits | 1.5 | 20.83 | 0.270 | 0.100 | 0.150 |
| 2.5 | 34.72 | 0.560 | 0.390 | 0.330 |
| 4.5 | 62.50 | 1.200 | 0.820 | 0.820 |
| 7.5 | 104.17 | 2.20 | 1.80 | 1.50 |
| 19.5 | 270.83 | 5.60 | 4.70 | 3.90 |
| 61.5 | 854.17 | 18.0 | 15.0 | 12.0 |
| 181.5 | 2520.83 | 56.0 | 47.0 | 39.0 |
| 601.5 | 8354.17 | 100.00 | 100.0 | 100.0 |

1. Guaranteed by characterization results.
2. All fast channels, expect channels on PA2, PA6, PB1, PB12.
3. Channels available on PA2, PA6, PB1, PB12.

###### Table 70. ADC accuracy - limited test conditions, 100-pin packages (1)(2)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | | **Min**  **(3)** | **Typ** | **Max**  **(3)** | **Unit** |
|  | Total |  | Single ended | Fast channel 5.1 Ms | - | 3.5 | 4.5 |  |
| Slow channel 4.8 Ms | - | 4 | 4.5 |
| ET | unadjusted |  |  |  |
|  | Fast channel 5.1 Ms | - | 3 | 3 |
|  | error |  | Differential |  |
| Slow channel 4.8 Ms | - | 3 | 3 |
|  |  |  | Single ended | Fast channel 5.1 Ms | - | 1 | 1.5 |  |
| Slow channel 4.8 Ms | - | 1 | 2.5 |
| EO | Offset error |  |  |  |
|  | Fast channel 5.1 Ms | - | 1 | 1.5 |
|  |  |  | Differential |  |
| Slow channel 4.8 Ms | - | 1 | 1.5 |
|  |  |  | Single ended | Fast channel 5.1 Ms | - | 3 | 4 |  |
| Slow channel 4.8 Ms | - | 3.5 | 4 |
| EG | Gain error |  |  | LSB |
|  | Fast channel 5.1 Ms | - | 1.5 | 2.5 |
|  |  |  | Differential |  |
| Slow channel 4.8 Ms | - | 2 | 2.5 |
|  | Differential | ADC clock freq.  72 MHz  Sampling freq.  5 Msps | Single ended | Fast channel 5.1 Ms | - | 1 | 1.5 |  |
| Slow channel 4.8 Ms | - | 1 | 1.5 |
| ED | linearity | VDDA = VREF+ = 3.3 V |  |  |
|  | Fast channel 5.1 Ms | - | 1 | 1 |
|  | error | 25°C  100-pin package | Differential |  |
| Slow channel 4.8 Ms | - | 1 | 1 |
|  | Integral |  | Single ended | Fast channel 5.1 Ms | - | 1.5 | 2 |  |
| Slow channel 4.8 Ms | - | 1.5 | 3 |
| EL | linearity |  |  |  |
|  | Fast channel 5.1 Ms | - | 1 | 1.5 |
|  | error |  | Differential |  |
| Slow channel 4.8 Ms | - | 1 | 1.5 |
|  | Effective |  | Single ended | Fast channel 5.1 Ms | 10.7 | 10.8 | - |  |
| Slow channel 4.8 Ms | 10.7 | 10.8 | - |
| ENOB(4) | number of |  |  | bits |
|  | Fast channel 5.1 Ms | 11.2 | 11.3 | - |
|  | bits |  | Differential |  |
| Slow channel 4.8 Ms | 11.1 | 11.3 | - |
|  | Signal-to- |  | Single ended | Fast channel 5.1 Ms | 66 | 67 | - |  |
| Slow channel 4.8 Ms | 66 | 67 | - |
| SINAD[(4)](#_bookmark265) | noise and  distortion |  |  | dB |
|  | Fast channel 5.1 Ms | 69 | 70 | - |
|  | ratio |  | Differential |  |
| Slow channel 4.8 Ms | 69 | 70 | - |

**Table 70. ADC accuracy - limited test conditions, 100-pin packages (1)(2) (continued)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | | **Min**  **(3)** | **Typ** | **Max**  **(3)** | **Unit** |
|  |  |  | Single ended | Fast channel 5.1 Ms | 66 | 67 | - |  |
| Slow channel 4.8 Ms | 66 | 67 | - |
| SNR[(4)](#_bookmark265) | Signal-to- noise ratio | ADC clock freq.  72 MHz Sampling freq  5 Msps |  |  |
| Differential | Fast channel 5.1 Ms | 69 | 70 | - |
| Slow channel 4.8 Ms | 69 | 70 | - |
|  |  | VDDA = VREF+ = 3.3 V |  | dB |
|  |  |  | Fast channel 5.1 Ms | - | -76 | -76 |
| THD[(4)](#_bookmark265) | Total harmonic | 25°C  100-pin package | Single ended |  |
| Slow channel 4.8 Ms | - | -76 | -76 |
|  | Fast channel 5.1 Ms | - | -80 | -80 |
|  | distortion |  | Differential |  |
| Slow channel 4.8 Ms | - | -80 | -80 |

1. ADC DC accuracy values are measured after internal calibration.
2. ADC accuracy vs. negative Injection Current: Injecting negative current on any analog input pins should be avoided as this significantly reduces the accuracy of the conversion being performed on another analog input. It is recommended to add a Schottky diode (pin to ground) to analog pins which may potentially inject negative current.

Any positive injection current within the limits specified for IINJ(PIN) and IINJ(PIN) in [*Section 6.3.14*](#_bookmark208)does not affect the ADC accuracy.

1. Guaranteed by characterization results.
2. Value measured with a -0.5 dB full scale 50 kHz sine wave input signal.

###### Table 71. ADC accuracy, 100-pin packages(1)(2)(3)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | | **Min (4)** | **Max(4)** | **Unit** |
| ET | Total unadjusted error | ADC clock freq.  72 MHz, Sampling freq.  5 Msps  2 V  VDDA , VREF+  3.6 V  100-pin package | Single Ended | Fast channel 5.1 Ms | - | 6.5 | LSB |
| Slow channel 4.8 Ms | - | 6.5 |
| Differential | Fast channel 5.1 Ms | - | 4 |
| Slow channel 4.8 Ms | - | 4 |
| EO | Offset error | Single Ended | Fast channel 5.1 Ms | - | 3 |
| Slow channel 4.8 Ms | - | 3 |
| Differential | Fast channel 5.1 Ms | - | 2 |
| Slow channel 4.8 Ms | - | 2 |
| EG | Gain error | Single Ended | Fast channel 5.1 Ms | - | 6 |
| Slow channel 4.8 Ms | - | 6 |
| Differential | Fast channel 5.1 Ms | - | 3 |
| Slow channel 4.8 Ms | - | 3 |
| ED | Differential linearity error | Single Ended | Fast channel 5.1 Ms | - | 1.5 |
| Slow channel 4.8 Ms | - | 1.5 |
| Differential | Fast channel 5.1 Ms | - | 1.5 |
| Slow channel 4.8 Ms | - | 1.5 |
| EL | Integral linearity error | Single Ended | Fast channel 5.1 Ms | - | 2 |
| Slow channel 4.8 Ms | - | 3 |
| Differential | Fast channel 5.1 Ms | - | 2 |
| Slow channel 4.8 Ms | - | 2 |
| ENOB  (5) | Effective number of bits | Single Ended | Fast channel 5.1 Ms | 10.4 | - | bits |
| Slow channel 4.8 Ms | 10.2 | - |
| Differential | Fast channel 5.1 Ms | 10.8 | - |
| Slow channel 4.8 Ms | 10.8 | - |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | | **Min (4)** | **Max(4)** | **Unit** |
| SINAD  [(5)](#_bookmark268) | Signal-to- noise and distortion ratio | ADC clock freq.  72 MHz, Sampling freq.  5 Msps,  2 V  VDDA, VREF+  3.6 V  100-pin package | Single Ended | Fast channel 5.1 Ms | 64 | - | dB |
| Slow channel 4.8 Ms | 63 | - |
| Differential | Fast channel 5.1 Ms | 67 | - |
| Slow channel 4.8 Ms | 67 | - |
| SNR[(5)](#_bookmark268) | Signal-to- noise ratio | Single Ended | Fast channel 5.1 Ms | 64 | - |
| Slow channel 4.8 Ms | 64 | - |
| Differential | Fast channel 5.1 Ms | 67 | - |
| Slow channel 4.8 Ms | 67 | - |
| THD[(5)](#_bookmark268) | Total harmonic distortion | Single Ended | Fast channel 5.1 Ms | - | -74 |
| Slow channel 4.8 Ms | - | -74 |
| Differential | Fast channel 5.1 Ms | - | -78 |
| Slow channel 4.8 Ms | - | -76 |

1. ADC DC accuracy values are measured after internal calibration.
2. ADC accuracy vs. negative Injection Current: Injecting negative current on any analog input pins should be avoided as this significantly reduces the accuracy of the conversion being performed on another analog input. It is recommended to add a Schottky diode (pin to ground) to analog pins which may potentially inject negative current.

Any positive injection current within the limits specified for IINJ(PIN) and IINJ(PIN) in [*Section 6.3.14*](#_bookmark208)does not affect the ADC accuracy.

1. Better performance may be achieved in restricted VDDA, frequency and temperature ranges.
2. Guaranteed by characterization results.
3. Value measured with a -0.5 dB full scale 50 kHz sine wave input signal.

###### Table 72. ADC accuracy - limited test conditions, 64-pin packages(1)(2)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | | **Min**  **(3)** | **Typ** | **Max**  **(3)** | **Unit** |
|  | Total |  | Single ended | Fast channel 5.1 Ms | - | ±4 | ±4.5 |  |
| Slow channel 4.8 Ms | - | ±5.5 | ±6 |
| ET | unadjusted |  |  |  |
|  | Fast channel 5.1 Ms | - | ±3.5 | ±4 |
|  | error |  | Differential |  |
| Slow channel 4.8 Ms | - | ±3.5 | ±4 |
|  |  |  | Single ended | Fast channel 5.1 Ms | - | ±2 | ±2 |  |
| Slow channel 4.8 Ms | - | ±1.5 | ±2 |
| EO | Offset error |  |  |  |
|  | Fast channel 5.1 Ms | - | ±1.5 | ±2 |
|  |  |  | Differential |  |
| Slow channel 4.8 Ms | - | ±1.5 | ±2 |
|  |  |  | Single ended | Fast channel 5.1 Ms | - | ±3 | ±4 |  |
| Slow channel 4.8 Ms | - | ±5 | ±5.5 |
| EG | Gain error |  |  | LSB |
|  | Fast channel 5.1 Ms | - | ±3 | ±3 |
|  |  |  | Differential |  |
| Slow channel 4.8 Ms | - | ±3 | ±3.5 |
|  | Differential | ADC clock freq.  72 MHz  Sampling freq.  5 Msps | Single ended | Fast channel 5.1 Ms | - | ±1 | ±1 |  |
| Slow channel 4.8 Ms | - | ±1 | ±1 |
| ED | linearity | VDDA = 3.3 V |  |  |
|  | Fast channel 5.1 Ms | - | ±1 | ±1 |
|  | error | 25°C  64-pin package | Differential |  |
| Slow channel 4.8 Ms | - | ±1 | ±1 |
|  | Integral |  | Single ended | Fast channel 5.1 Ms | - | ±1.5 | ±2 |  |
| Slow channel 4.8 Ms | - | ±2 | ±3 |
| EL | linearity |  |  |  |
|  | Fast channel 5.1 Ms | - | ±1.5 | ±1.5 |
|  | error |  | Differential |  |
| Slow channel 4.8 Ms | - | ±1.5 | ±2 |
|  | Effective number of bits |  | Single ended | Fast channel 5.1 Ms | 10.8 | 10.8 | - | bit |
| Slow channel 4.8 Ms | 10.8 | 10.8 | - |
| ENOB |  |  |
| (4) |  |
|  | Fast channel 5.1 Ms | 11.2 | 11.3 | - |
|  |  | Differential |
| Slow channel 4.8 Ms | 11.2 | 11.3 | - |
|  | Signal-to- |  | Single ended | Fast channel 5.1 Ms | 66 | 67 | - | dB |
| Slow channel 4.8 Ms | 66 | 67 | - |
| SINAD | noise and |  |  |
| (4) | distortion |  |
|  | Fast channel 5.1 Ms | 69 | 70 | - |
|  | ratio |  | Differential |
| Slow channel 4.8 Ms | 69 | 70 | - |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | | **Min**  **(3)** | **Typ** | **Max**  **(3)** | **Unit** |
|  |  |  | Single ended | Fast channel 5.1 Ms | 66 | 67 | - |  |
| Slow channel 4.8 Ms | 66 | 67 | - |
| SNR(4) | Signal-to- noise ratio | ADC clock freq.  72 MHz Sampling freq  5 Msps |  |  |
| Differential | Fast channel 5.1 Ms | 69 | 70 | - |
| Slow channel 4.8 Ms | 69 | 70 | - |
|  |  | VDDA = 3.3 V |  | dB |
|  |  |  | Fast channel 5.1 Ms | - | -80 | -80 |
| THD(4) | Total harmonic | 25°C  64-pin package | Single ended |  |
| Slow channel 4.8 Ms | - | -78 | -77 |
|  | Fast channel 5.1 Ms | - | -83 | -82 |
|  | distortion |  | Differential |  |
| Slow channel 4.8 Ms | - | -81 | -80 |

1. ADC DC accuracy values are measured after internal calibration.
2. ADC accuracy vs. negative Injection Current: Injecting negative current on any analog input pins should be avoided as this significantly reduces the accuracy of the conversion being performed on another analog input. It is recommended to add a Schottky diode (pin to ground) to analog pins which may potentially inject negative current.

Any positive injection current within the limits specified for IINJ(PIN) and IINJ(PIN) in [*Section 6.3.14*](#_bookmark208)does not affect the ADC accuracy.

1. Guaranteed by characterization results.
2. Value measured with a -0.5 dB full scale 50 kHz sine wave input signal.

###### Table 73. ADC accuracy, 64-pin packages(1)(2)(3)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | | **Min(4)** | **Max**  [**(4)**](#_bookmark273) | **Unit** |
|  | Total |  | Single ended | Fast channel 5.1 Ms | - | ±6.5 |  |
| Slow channel 4.8 Ms | - | ±6.5 |
| ET | unadjusted |  |  |  |
|  | Fast channel 5.1 Ms | - | ±4 |
|  | error |  | Differential |  |
| Slow channel 4.8 Ms | - | ±4.5 |
|  |  |  | Single ended | Fast channel 5.1 Ms | - | ±3 |  |
| Slow channel 4.8 Ms | - | ±3 |
| EO | Offset error |  |  |  |
|  | Fast channel 5.1 Ms | - | ±2.5 |
|  |  |  | Differential |  |
| Slow channel 4.8 Ms | - | ±2.5 |
|  |  |  | Single ended | Fast channel 5.1 Ms | - | ±6 |  |
| Slow channel 4.8 Ms | - | ±6 |
| EG | Gain error |  |  | LSB |
|  | Fast channel 5.1 Ms | - | ±3.5 |
|  |  |  | Differential |  |
| Slow channel 4.8 Ms | - | ±4 |
| ED | Differential linearity error | ADC clock freq.  72 MHz, Sampling freq.  5 Msps  2.0 V  VDDA  3.6 V  64-pin package | Single ended | Fast channel 5.1 Ms | - | ±1.5 |  |
| Slow channel 4.8 Ms | - | ±1.5 |
| Differential | Fast channel 5.1 Ms | - | ±1.5 |
| Slow channel 4.8 Ms | - | ±1.5 |
|  | Integral |  | Single ended | Fast channel 5.1 Ms | - | ±3 |  |
| Slow channel 4.8 Ms | - | ±3.5 |
| EL | linearity |  |  |  |
|  | Fast channel 5.1 Ms | - | ±2 |
|  | error |  | Differential |  |
| Slow channel 4.8 Ms | - | ±2.5 |
|  | Effective number of bits |  | Single ended | Fast channel 5.1 Ms | 10.4 | - | bits |
| Slow channel 4.8 Ms | 10.4 | - |
| ENOB |  |  |
| (5) |  |
|  | Fast channel 5.1 Ms | 10.8 | - |
|  |  | Differential |
| Slow channel 4.8 Ms | 10.8 | - |
|  | Signal-to- |  | Single ended | Fast channel 5.1 Ms | 64 | - | dB |
| Slow channel 4.8 Ms | 63 | - |
| SINAD | noise and |  |  |
| (5) | distortion |  |
|  | Fast channel 5.1 Ms | 67 | - |
|  | ratio |  | Differential |
| Slow channel 4.8 Ms | 67 | - |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | | **Min(4)** | **Max**  **(4)** | **Unit** |
| SNR(5) | Signal-to- noise ratio | ADC clock freq.  72 MHz, Sampling freq  5 Msps,  2 V  VDDA  3.6 V  64-pin package | Single ended | Fast channel 5.1 Ms | 64 | - | dB |
| Slow channel 4.8 Ms | 64 | - |
| Differential | Fast channel 5.1 Ms | 67 | - |
| Slow channel 4.8 Ms | 67 | - |
| THD(5) | Total harmonic distortion | Single ended | Fast channel 5.1 Ms | - | -75 |
| Slow channel 4.8 Ms | - | -75 |
| Differential | Fast channel 5.1 Ms | - | -79 |
| Slow channel 4.8 Ms | - | -78 |

1. ADC DC accuracy values are measured after internal calibration.
2. ADC accuracy vs. negative Injection Current: Injecting negative current on any analog input pins should be avoided as this significantly reduces the accuracy of the conversion being performed on another analog input. It is recommended to add a Schottky diode (pin to ground) to analog pins which may potentially inject negative current.

Any positive injection current within the limits specified for IINJ(PIN) and IINJ(PIN) in [*Section 6.3.14*](#_bookmark208)does not affect the ADC accuracy.

1. Better performance may be achieved in restricted VDDA, frequency and temperature ranges.
2. Guaranteed by characterization results.
3. Value measured with a -0.5 dB full scale 50 kHz sine wave input signal.

###### Table 74. ADC accuracy at 1MSPS(1)(2)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Test conditions** | | **Typ** | **Max(3)** | **Unit** |
| ET | Total unadjusted error |  | Fast channel | ±2.5 | ±5 |  |
| Slow channel | ±3.5 | ±5 |
| EO | Offset error |  | Fast channel | ±1 | ±2.5 |  |
| Slow channel | ±1.5 | ±2.5 |
|  |  | ADC Freq ≤ 72 MHz |  |
|  |  | Fast channel | ±2 | ±3 |
| EG | Gain error | Sampling Freq ≤ 1MSPS  2.4 V ≤ VDDA = VREF+ ≤ 3.6 V | LSB |
| Slow channel | ±3 | ±4 |
|  |  | Single-ended mode |  |
|  |  | Fast channel | ±0.7 | ±2 |
| ED | Differential linearity error |  |  |
| Slow channel | ±0.7 | ±2 |
| EL | Integral linearity error |  | Fast channel | ±1 | ±3 |  |
| Slow channel | ±1.2 | ±3 |

1. ADC DC accuracy values are measured after internal calibration.
2. ADC accuracy vs. negative Injection Current: Injecting negative current on any analog input pins should be avoided as this significantly reduces the accuracy of the conversion being performed on another analog input. It is recommended to add a Schottky diode (pin to ground) to analog pins which may potentially inject negative current.. Any positive injection current within the limits specified for IINJ(PIN) and ∑IINJ(PIN) in [*Section 6.3.14: I/O port characteristics*](#_bookmark208)does not affect the ADC accuracy.
3. Guaranteed by characterization results.

###### Figure 34. ADC accuracy characteristics



El

ai14395e

4O93 4O94 4O95 4O96

Vdda

3 4 5 6 7

1 2

O

Vssa

ET = Total unadjusted Error: maximum deviation between the actual and the ideal transfer curves. EO = Offset Error: deviation between the first actual transition and the last actual one.

EG = Gain Error: deviation between the last ideal transition and the last actual one.

ED = Differential Linearity Error: maximum deviation between actual steps and the ideal one.

EL = Integral Linearity Error: maximum deviation between any actual transition and the end-point correlation line.

1 LSB IDEAL

Ed

[1LSB IDEAL = VREF+ (or VDDA depending on package)

Eo

(1)

(3)

7

6

5

4

3

2

1

Et

(2)

1. Example of an actu al transfer curve
2. The ideal transfer cu rve
3. End point correlation line

Eg

4O95

4O94

4O93

4O96

4O96

**Figure 35. Typical connection diagram using the ADC**



MS19881V3

Cadc

Cparasitic

VT IL ± 1 µA

VAIN O.6 V

12-bit converter

Radc

AINx

Rain(1)

Sample and hold ADC converter

Vt

O.6 V

Vdd

* 1. Refer to [*Table 68*](#_bookmark254)for the values of RAIN.
  2. Cparasitic represents the capacitance of the PCB (dependent on soldering and PCB layout quality) plus the pad capacitance (roughly 7 pF). A high Cparasitic value will downgrade conversion accuracy. To remedy this, fADC should be reduced.

##### General PCB design guidelines

Power supply decoupling should be performed as shown in [*Figure 11*](#_bookmark118). The 10 nF capacitor should be ceramic (good quality) and it should be placed as close as possible to the chip.

#### DAC electrical specifications

###### Table 75. DAC characteristics

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| VDDA | Analog supply voltage | DAC output buffer ON | 2.4 | - | 3.6 | V |
| RLOAD(1) | Resistive load | DAC output buffer ON | 5 | - | - | k |
| (1)  RO | Output impedance | DAC output buffer ON | - | - | 15 | k |
| CLOAD(1) | Capacitive load | DAC output buffer ON | - | - | 50 | pF |
| VDAC\_OUT (1) | Voltage on DAC\_OUT output | Corresponds to 12-bit input code (0x0E0) to (0xF1C) at VDDA = 3.6 V  and (0x155) and (0xEAB) at  VDDA = 2.4 V DAC output buffer ON. | 0.2 | - | VDDA – 0.2 | V |
| DAC output buffer OFF | - | 0.5 | VDDA - 1LSB | mV |
| IDD [(3)](#_bookmark281) A | DAC DC current consumption in quiescent mode (Standby mode)(2) | With no load, middle code (0x800) on the input. | - | - | 380 | µA |
| With no load, worst code (0xF1C) on the input. | - | - | 480 | µA |
| DNL(3) | Differential non linearity Difference between two consecutive code-1LSB) | Given for a 10-bit input code | - | - | ±0.5 | LSB |
| Given for a 12-bit input code | - | - | ±2 | LSB |
| INL[(3)](#_bookmark281) | Integral non linearity (difference between measured value at Code i and the value at Code i on a line drawn between Code 0 and last Code 4095) | Given for a 10-bit input code | - | - | ±1 | LSB |
| Given for a 12-bit input code | - | - | ±4 | LSB |
| Offset[(3)](#_bookmark281) | Offset error (difference between measured value at Code (0x800) and the ideal value = VDDA/2) | - | - | - | ±10 | mV |
| Given for a 10-bit input code at VDDA = 3.6 V | - | - | ±3 | LSB |
| Given for a 12-bit input code at VDDA = 3.6 V | - | - | ±12 | LSB |
| Gain error[(3)](#_bookmark281) | Gain error | Given for a 12-bit input code | - | - | ±0.5 | % |
| tSETTLING[(3)](#_bookmark281) | Settling time (full scale: for a 12-bit input code transition between the lowest and the highest input codes when DAC\_OUT reaches final value ±1LSB | CLOAD  50 pF,  RLOAD  5 k | - | 3 | 4 | µs |
| Update rate[(3)](#_bookmark281) | Max frequency for a correct DAC\_OUT change when small variation in the input code (from code i to i+1LSB) | CLOAD  50 pF,  RLOAD  5 k | - | - | 1 | MS/s |

**Table 75. DAC characteristics (continued)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | **Min** | **Typ** | **Max** | **Unit** |
| tWAKEU [(3)](#_bookmark281)  P | Wakeup time from off state (Setting the ENx bit in the DAC Control register) | CLOAD  50 pF,  RLOAD  5 k | - | 6.5 | 10 | µs |
| PSRR+ (1) | Power supply rejection ratio (to VDDA) (static DC measurement | CLOAD  50 pF,  No RLOAD  5 k | - | –67 | –40 | dB |

1. Guaranteed by design.
2. Quiescent mode refers to the state of the DAC a keeping steady value on the output, so no dynamic consumption is involved.
3. Guaranteed by characterization results.

###### Figure 36. 12-bit buffered /non-buffered DAC

Buffered/Non-buffered DAC

R L

DAC\_OUTx

C L

ai17157V3

Buffer(1)

12-bit digital to analog converter

1. The DAC integrates an output buffer that can be used to reduce the output impedance and to drive external loads directly without the use of an external operational amplifier. The buffer can be bypassed by configuring the BOFFx bit in the DAC\_CR register.

#### Comparator characteristics

###### Table 76. Comparator characteristics(1)


|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | **Min** | **Typ** | **Max** | **Unit** |
| VDDA | Analog supply voltage | - | | 2 | - | 3.6 | V |
| VIN | Comparator input voltage range | - | | 0 | - | VDDA |
| VBG | Scaler input voltage | - | | - | 1.2 | - |
| VSC | Scaler offset voltage | - | | - | ±5 | ±10 | mV |
| tS\_SC | VREFINT scaler startup time from power down | First VREFINT scaler activation after device power on | | - | - | 1(2) | s |
| Next activations | | - | - | 0.2 | ms |
| tSTART | Comparator startup time | Startup time to reach propagation delay specification | | - | - | 60 | µs |
| tD | Propagation delay for 200 mV step with 100 mV overdrive | Ultra-low-power mode | | - | 2 | 4.5 | µs |
| Low-power mode | | - | 0.7 | 1.5 |
| Medium power mode | | - | 0.3 | 0.6 |
| High speed mode | VDDA  2.7 V | - | 50 | 100 | ns |
| VDDA  2.7 V | - | 100 | 240 |
| Propagation delay for full range step with 100 mV overdrive | Ultra-low-power mode | | - | 2 | 7 | µs |
| Low-power mode | | - | 0.7 | 2.1 |
| Medium power mode | | - | 0.3 | 1.2 |
| High speed mode | VDDA  2.7 V | - | 90 | 180 | ns |
| VDDA  2.7 V | - | 110 | 300 |
| Voffset | Comparator offset error | - | | - | 4 | 10 | mV |
| dVoffset/dT | Offset error temperature coefficient | - | | - | 18 | - | µV/° C |
| IDD(COMP) | COMP current consumption | Ultra-low-power mode | | - | 1.2 | 1.5 | µA |
| Low-power mode | | - | 3 | 5 |
| Medium power mode | | - | 10 | 15 |
| High speed mode | | - | 75 | 100 |

**Table 76. Comparator characteristics(1) (continued)**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Conditions** | | **Min** | **Typ** | **Max** | **Unit** |
| Vhys | Comparator hysteresis | No hysteresis (COMPxHYST[1:0]=00) | - | - | 0 | - | mV |
| Low hysteresis (COMPxHYST[1:0]=01) | High speed mode | 3 | 8 | 13 |
| All other power modes | 5 | 10 |
| Medium hysteresis (COMPxHYST[1:0]=10) | High speed mode | 7 | 15 | 26 |
| All other power modes | 9 | 19 |
| High hysteresis (COMPxHYST[1:0]=11) | High speed mode | 18 | 31 | 49 |
| All other power modes | 19 | 40 |

1. Data guaranteed by design.
2. For more details and conditions, see [*Figure 37*](#_bookmark287)Maximum VREFINT scaler startup time from power down.

**Figure 37.** **Maximum VREFINT scaler startup time from power down**



MS36682V1

#### Operational amplifier characteristics

###### Table 77. Operational amplifier characteristics(1)


|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | | **Condition** | **Min** | **Typ** | **Max** | **Unit** |
| VDDA | Analog supply voltage | | - | 2.4 | - | 3.6 | V |
| CMIR | Common mode input range | | - | 0 | - | VDDA | V |
| VIOFFSET | Input offset voltage | Maximum calibration range | 25°C, No Load on output. | - | - | 4 | mV |
| All voltage/Temp. | - | - | 6 |
| After offset calibration | 25°C, No Load on output. | - | - | 1.6 |
| All voltage/Temp. | - | - | 3 |
| VIOFFSET | Input offset voltage drift | | - | - | 5 | - | µV/°C |
| ILOAD | Drive current | | - | - | - | 500 | µA |
| IDDOPAMP | Consumption | | No load, quiescent mode | - | 690 | 1450 | µA |
| TS\_OPAMP\_VOUT | ADC sampling time when reading the OPAMP output. | | - | 400 | - | - | ns |
| CMRR | Common mode rejection ratio | | - | - | 90 | - | dB |
| PSRR | Power supply rejection ratio | | DC | 73 | 117 | - | dB |
| GBW | Bandwidth | | - | - | 8.2 | - | MHz |
| SR | Slew rate | | - | - | 4.7 | - | V/µs |
| RLOAD | Resistive load | | - | 4 | - | - | k |
| CLOAD | Capacitive load | | - | - | - | 50 | pF |
| VOHSAT | High saturation voltage | | Rload = min, Input at VDDA. | - | - | 100 | mV |
| Rload = 20K, Input at VDDA. | - | - | 20 |
| VOLSAT | Low saturation voltage | | Rload = min, input at 0V | - | - | 100 |
| Rload = 20K, input at 0V. | - | - | 20 |
| m | Phase margin | | - | - | 62 | - | ° |
| tOFFTRIM | Offset trim time: during calibration, minimum time needed between two steps to have 1 mV accuracy | | - | - | - | 2 | ms |
| tWAKEUP | Wake up time from OFF state. | | CLOAD  50 pf,  RLOAD  4 k Follower  configuration | - | 2.8 | 5 | µs |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Condition** | **Min** | **Typ** | **Max** | **Unit** |
| PGA gain | Non inverting gain value | - | - | 2 | - | - |
| - | 4 | - | - |
| - | 8 | - | - |
| - | 16 | - | - |
| Rnetwork | R2/R1 internal resistance values in PGA mode (2) | Gain=2 | - | 5.4/5.4 | - | k |
| Gain=4 | - | 16.2/5.4 | - |
| Gain=8 | - | 37.8/5.4 | - |
| Gain=16 | - | 40.5/2.7 | - |
| PGA gain error | PGA gain error | - | -1% | - | 1% |  |
| Ibias | OPAMP input bias current | - | - | - | 0.2(3) | µA |
| PGA BW | PGA bandwidth for different non inverting gain | PGA Gain = 2, Cload = 50pF, Rload = 4 K | - | 4 | - | MHz |
| PGA Gain = 4, Cload = 50pF, Rload = 4 K | - | 2 | - |
| PGA Gain = 8, Cload = 50pF, Rload = 4 K | - | 1 | - |
| PGA Gain = 16,  Cload = 50pF, Rload = 4 K | - | 0.5 | - |
| en | Voltage noise density | @ 1KHz, Output loaded with  4 K | - | 109 | - | *nV*  -----------  *Hz* |
| @ 10KHz,  Output loaded with 4 K | - | 43 | - |

1. Guaranteed by design.
2. R2 is the internal resistance between OPAMP output and OPAMP inverting input. R1 is the internal resistance between OPAMP inverting input and ground.

The PGA gain =1+R2/R1

1. Mostly TTa I/O leakage, when used in analog mode.

******Figure 38. OPAMP voltage noise versus frequency**

#### Temperature sensor characteristics

###### Table 78. TS characteristics

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Min** | **Typ** | **Max** | **Unit** |
| TL(1) | VSENSE linearity with temperature | - | 1 | 2 | °C |
| Avg\_Slope(1) | Average slope | 4.0 | 4.3 | 4.6 | mV/°C |
| V25 | Voltage at 25 °C | 1.34 | 1.43 | 1.52 | V |
| (1)  tSTART | Startup time | 4 | - | 10 | µs |
| T (1)(2)  S\_temp | ADC sampling time when reading the temperature | 2.2 | - | - | µs |

* + - 1. Guaranteed by design.
      2. Shortest sampling time can be determined in the application by multiple iterations.

###### Table 79. Temperature sensor calibration values

|  |  |  |
| --- | --- | --- |
| **Calibration value name** | **Description** | **Memory address** |
| TS\_CAL1 | TS ADC raw data acquired at temperature of 30 °C,  VDDA= 3.3 V | 0x1FFF F7B8 - 0x1FFF F7B9 |
| TS\_CAL2 | TS ADC raw data acquired at temperature of 110 °C  VDDA= 3.3 V | 0x1FFF F7C2 - 0x1FFF F7C3 |

**Table 80. VBAT monitoring characteristics**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Min** | **Typ** | **Max** | **Unit** |
| R | Resistor bridge for VBAT | - | 50 | - | K |
| Q | Ratio on VBAT measurement | - | 2 | - |  |
| Er(1) | Error on Q | -1 | - | +1 | % |
| TS\_vbat(1)(2) | ADC sampling time when reading the VBAT 1mV accuracy | 2.2 | - | - | µs |

1. Guaranteed by design.
2. Shortest sampling time can be determined in the application by multiple iterations.



# Package information

In order to meet environmental requirements, ST offers these devices in different grades of ECOPACK® packages, depending on their level of environmental compliance. ECOPACK® specifications, grade definitions and product status are available at: [*www.st.com*.](http://www.st.com/)

ECOPACK® is an ST trademark.

## LQFP100 – 14 x 14 mm, low-profile quad flat package information

###### Figure 39. LQFP100 – 14 x 14 mm, low-profile quad flat package outline



1L\_ME\_V5

e

25

1

PIN 1 IDENTIFICATION

26

1OO

5O

76

75 51

L

L1

D D1

D3

ccc C

O.25 mm

GAUGE PLANE

SEATING PLANE

C

A

A2 A1

A1

c

K

1. Drawing is not to scale.

b

E3 E1 E

###### Table 81. LQPF100 – 14 x 14 mm, low-profile quad flat package mechanical data

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **millimeters** | | | **inches(1)** | | |
| **Min** | **Typ** | **Max** | **Min** | **Typ** | **Max** |
| A | - | - | 1.60 | - | - | 0.063 |
| A1 | 0.05 | - | 0.15 | 0.002 | - | 0.0059 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **millimeters** | | | **inches(1)** | | |
| **Min** | **Typ** | **Max** | **Min** | **Typ** | **Max** |
| A2 | 1.35 | 1.40 | 1.45 | 0.0531 | 0.0551 | 0.0571 |
| b | 0.17 | 0.22 | 0.27 | 0.0067 | 0.0087 | 0.0106 |
| c | 0.09 | - | 0.2 | 0.0035 | - | 0.0079 |
| D | 15.80 | 16.00 | 16.2 | 0.622 | 0.6299 | 0.6378 |
| D1 | 13.80 | 14.00 | 14.2 | 0.5433 | 0.5512 | 0.5591 |
| D3 | - | 12.00 | - | - | 0.4724 | - |
| E | 15.80 | 16.00 | 16.2 | 0.622 | 0.6299 | 0.6378 |
| E1 | 13.80 | 14.00 | 14.2 | 0.5433 | 0.5512 | 0.5591 |
| E3 | - | 12.00 | - | - | 0.4724 | - |
| e | - | 0.50 | - | - | 0.0197 | - |
| L | 0.45 | 0.60 | 0.75 | 0.0177 | 0.0236 | 0.0295 |
| L1 | - | 1.00 | - | - | 0.0394 | - |
| K | 0° | 3.5° | 7° | 0° | 3.5° | 7° |
| ccc | - | - | 0.08 | - | - | 0.0031 |

1. Values in inches are converted from mm and rounded to 4 decimal digits.

###### Figure 40. LQFP100 – 14 x 14 mm, low-profile quad flat package recommended footprint

1.2

ai149O6c

12.3

16.7

25

1

75

26

1OO

16.7 14.3

O.3

5O

O.5

76

51

* 1. Dimensions are in millimeters.

##### Device marking

The following figure gives an example of topside marking orientation versus pin 1 identifier location.

###### Figure 41. LQFP100 – 14 x 14 mm, low-profile quad flat package top view example



Product identification(1)

Revision code

Date code

Y WW

Pin 1 indentifier

MSv365O1V2

vCT6 R

STM32F303

1. Parts marked as “ES”, “E” or accompanied by an Engineering Sample notification letter, are not yet qualified and therefore not yet ready to be used in production and any consequences deriving from such usage will not be at ST charge. In no event, ST will be liable for any customer usage of these engineering samples in production. ST Quality has to be contacted prior to any decision to use these Engineering samples to run qualification activity.

## LQFP64 – 10 x 10 mm, low-profile quad flat package information

###### Figure 42. LQFP64 – 10 x 10 mm, low-profile quad flat package outline



5W\_ME\_V3

16

e

1

PIN 1 IDENTIFICATION

17

64

b

32

49

48 33

L

L1

D D1

D3

ccc C

O.25 mm GAUGE PLANE

SEATING PLANE

C

K

A A2

A1

c

A1

1. Drawing is not to scale.

E3 E1

E

###### Table 82. LQFP64 – 10 x 10 mm, low-profile quad flat package mechanical data

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **millimeters** | | | **inches(1)** | | |
| **Min** | **Typ** | **Max** | **Min** | **Typ** | **Max** |
| A | - | - | 1.60 | - | - | 0.0630 |
| A1 | 0.05 | - | 0.15 | 0.0020 | - | 0.0059 |
| A2 | 1.350 | 1.40 | 1.45 | 0.0531 | 0.0551 | 0.0571 |
| b | 0.17 | 0.22 | 0.27 | 0.0067 | 0.0087 | 0.0106 |
| c | 0.09 | - | 0.20 | 0.0035 |  | 0.0079 |
| D | - | 12.00 | - | - | 0.4724 | - |
| D1 | - | 10.00 | - | - | 0.3937 | - |
| D3 | - | 7.50 | - | - | 0.2953 | - |
| E | - | 12.00 | - | - | 0.4724 | - |

**Table 82. LQFP64 – 10 x 10 mm, low-profile quad flat package mechanical data (continued)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **millimeters** | | | **inches(1)** | | |
| **Min** | **Typ** | **Max** | **Min** | **Typ** | **Max** |
| E1 | - | 10.00 | - | - | 0.3937 | - |
| E3 | - | 7.50 | - | - | 0.2953 | - |
| e | - | 0.50 | - | - | 0.0197 | - |
| K | 0° | 3.5° | 7° | 0° | 3.5° | 7° |
| L | 0.45 | 0.60 | 0.75 | 0.0177 | 0.0236 | 0.0295 |
| L1 | - | 1.00 | - | - | 0.0394 | - |
| ccc | - | - | 0.08 | - | - | 0.0031 |

1. Values in inches are converted from mm and rounded to 4 decimal digits.

###### Figure 43. LQFP64 – 10 x 10 mm, low-profile quad flat package recommended footprint

17

ai149O9c

7.8

12.7

16

1

1.2

48

64

1O.3

1O.3

12.7

32

O.5

49

O.3

33

1. Dimensions are in millimeters.

##### Device marking

The following figure gives an example of topside marking orientation versus pin 1 identifier location.

###### Figure 44. LQFP64 – 10 x 10 mm, low-profile quad flat package top view example

Product identification(1)

Revision code

Date code

Y WW

Pin 1 indentifier

MSv365O2V1



RCT6

STM32F303

R

1. Parts marked as “ES”, “E” or accompanied by an Engineering Sample notification letter, are not yet qualified and therefore not yet ready to be used in production and any consequences deriving from such usage will not be at ST charge. In no event, ST will be liable for any customer usage of these engineering samples in production. ST Quality has to be contacted prior to any decision to use these Engineering samples to run qualification activity.

## LQFP48 – 7 x 7 mm, low-profile quad flat package information

###### Figure 45. LQFP48 – 7 x 7 mm, low-profile quad flat package outline



12

5B\_ME\_V2

e

GAUGE PLANE

O.25 mm

SEATING PLANE

PIN 1

IDENTIFICATION 1

13

48

b

24

37

36 25

L

L1

D

D1 D3

C

K

A

A2

A1

c

A1

|  |  |  |
| --- | --- | --- |
|  | ccc | C |

1. Drawing is not to scale.

E3 E1

E

###### Table 83. LQFP48 – 7 x 7 mm, low-profile quad flat package mechanical data

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **millimeters** | | | **inches(1)** | | |
| **Min** | **Typ** | **Max** | **Min** | **Typ** | **Max** |
| A | - | - | 1.60 | - | - | 0.0630 |
| A1 | 0.05 | - | 0.15 | 0.0020 | - | 0.0059 |
| A2 | 1.35 | 1.40 | 1.45 | 0.0531 | 0.0551 | 0.0571 |
| b | 0.17 | 0.22 | 0.27 | 0.0067 | 0.0087 | 0.0106 |
| c | 0.09 | - | 0.20 | 0.0035 | - | 0.0079 |
| D | 8.80 | 9.00 | 9.20 | 0.3465 | 0.3543 | 0.3622 |
| D1 | 6.80 | 7.00 | 7.20 | 0.2677 | 0.2756 | 0.2835 |
| D3 | - | 5.50 | - | - | 0.2165 | - |
| E | 8.80 | 9.00 | 9.20 | 0.3465 | 0.3543 | 0.3622 |

**Table 83. LQFP48 – 7 x 7 mm, low-profile quad flat package mechanical data (continued)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **millimeters** | | | **inches(1)** | | |
| **Min** | **Typ** | **Max** | **Min** | **Typ** | **Max** |
| E1 | 6.80 | 7.00 | 7.20 | 0.2677 | 0.2756 | 0.2835 |
| E3 | - | 5.50 | - | - | 0.2165 | - |
| e | - | 0.50 | - | - | 0.0197 | - |
| L | 0.45 | 0.60 | 0.75 | 0.0177 | 0.0236 | 0.0295 |
| L1 | - | 1.00 | - | - | 0.0394 | - |
| K | 0° | 3.5° | 7° | 0° | 3.5° | 7° |
| ccc | - | - | 0.08 | - | - | 0.0031 |

1. Values in inches are converted from mm and rounded to 4 decimal digits.

###### Figure 46. LQFP48 - 7 x 7 mm, low-profile quad flat package recommended footprint

7.3O

ai14911d

5.8O

9.7O

1.2O

13

12

1

48

O.5O

7.3O

9.7O 5.8O

O.2O

24

37

O.3O

25

36

1.2O

1. Dimensions are in millimeters.

##### Device marking

The following figure gives an example of topside marking orientation versus pin 1 identifier location.

###### Figure 47. LQFP48 - 7 x 7 mm, low-profile quad flat package top view example

Product identification (1)

STM32F3O3

CCT6

Date code

Y WW

Pin 1 identification

Revision code

MS366O5V1





R

1. Parts marked as “ES”, “E” or accompanied by an Engineering Sample notification letter, are not yet qualified and therefore not yet ready to be used in production and any consequences deriving from such usage will not be at ST charge. In no event, ST will be liable for any customer usage of these engineering samples in production. ST Quality has to be contacted prior to any decision to use these Engineering samples to run qualification activity.

## WLCSP100 - 0.4 mm pitch wafer level chip scale package information

###### Figure 48.WLCSP100 – 100L, 4.166 x 4.628 mm 0.4 mm pitch wafer level chip scale package outline



BOTTOM VIEW

SIDE VIEW

FRONT VIEW

DETAIL A ROTATED 9O°

A1 BALL LOCATION

aaa

(4X)

A

WLCSP1OOL\_AO1Q\_ME\_V1

A1 ORIENTATION REFERENCE

K

DETAIL A

TOP VIEW WAFER BACK SIDE


1. Drawing is not to scale.

###### Table 84. WLCSP100 – 100L, 4.166 x 4.628 mm 0.4 mm pitch wafer level chip scale package mechanical data

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Symbol** | **millimeters** | | | **inches(1)** | | |
| **Min** | **Typ** | **Max** | **Typ** | **Min** | **Max** |
| A | 0.525 | 0.555 | 0.585 | 0.0207 | 0.0219 | 0.0230 |
| A1 | - | 0.17 | - | - | 0.0067 | - |
| A2 | - | 0.38 | - | - | 0.0150 | - |
| A3(2) | - | 0.025 | - | - | 0.0010 | - |
| Ø b(3) | 0.22 | 0.25 | 0.28 | - | 0.0098 | 0.0110 |
| D | 4.166 | 4.201 | 4.236 | - | 0.1654 | 0.1668 |
| E | 4.628 | 4.663 | 4.698 | - | 0.1836 | 0.1850 |
| e | - | 0.4 | - | - | 0.0157 | - |
| e1 | - | 3.6 | - | - | 0.1417 | - |
| e2 | - | 3.6 | - | - | 0.1417 | - |
| F | - | 0.3005 | - | - | 0.0118 | - |
| G | - | 0.5315 | - | - | 0.0209 | - |
| N | - | 100 | - | - | 3.9370 | - |
| aaa | - | 0.1 | - | - | 0.0039 | - |
| bbb | - | 0.1 | - | - | 0.0039 | - |
| ccc | - | 0.1 | - | - | 0.0039 | - |
| ddd | - | 0.05 | - | - | 0.0020 | - |
| eee | - | 0.05 | - | - | 0.0020 | - |

1. Values in inches are converted from mm and rounded to 4 decimal digits.
2. Back side coating.
3. Dimension is measured at the maximum bump diameter parallel to primary datum Z.

**Figure 49. WLCSP100 – 100L, 4.166 x 4.628 mm 0.4 mm pitch wafer level chip scale package recommended footprint**



Dpad

Dsm

WLCSP1OOL\_AO1Q\_FP\_V1

**Table 85. WLCSP100 recommended PCB design rules (0.4 mm pitch)**

|  |  |
| --- | --- |
| **Dimension** | **Recommended values** |
| Pitch | 0.4 mm |
| Dpad | 0.225 mm |
| Dsm | 0.290 mm |
| Stencil thickness | 0.1 mm |

##### Marking of engineering samples

The following figure gives an example of topside marking orientation versus ball A1 identifier location.

###### Figure 50. WLCSP100, 0.4 mm pitch wafer level chip scale package top view example



Ball A1 identifier

Product identification(1)

ZĞǀiƐiŽŶ cŽĚĞ

MSv4O444V1

R

WW

Y

32F303vC6

1. Parts marked as “ES”, “E” or accompanied by an Engineering Sample notification letter, are not yet qualified and therefore not yet ready to be used in production and any consequences deriving from such usage will not be at ST charge. In no event, ST will be liable for any customer usage of these engineering samples in production. ST Quality has to be contacted prior to any decision to use these Engineering samples to run qualification activity.

## Thermal characteristics

The maximum chip junction temperature (TJmax) must never exceed the values given in

[*Table 24: General operating conditions on page 59*](#_bookmark131).

The maximum chip-junction temperature, TJ max, in degrees Celsius, may be calculated using the following equation:

TJ max = TA max + (PD max x JA)

Where:

* TA max is the maximum ambient temperature in °C,
* JA is the package junction-to-ambient thermal resistance, in C/W,
* PD max is the sum of PINT max and PI/O max (PD max = PINT max + PI/Omax),
* PINT max is the product of IDD and VDD, expressed in Watts. This is the maximum chip internal power.

PI/O max represents the maximum power dissipation on output pins where: PI/O max =  (VOL × IOL) + ((VDD – VOH) × IOH),

taking into account the actual VOL / IOL and VOH / IOH of the I/Os at low and high level in the application.

**Table 86.** **Package thermal characteristics**

|  |  |  |  |
| --- | --- | --- | --- |
| **Symbol** | **Parameter** | **Value** | **Unit** |
| JA | **Thermal resistance junction-ambient**  LQFP64 - 10 × 10 mm / 0.5 mm pitch | 45 | °C/W |
| **Thermal resistance junction-ambient**  LQFP48 - 7 × 7 mm | 55 |
| **Thermal resistance junction-ambient**  LQFP100 - 14 × 14 mm / 0.5 mm pitch | 41 |
| **Thermal resistance junction-ambient**  WLCSP100 - 0.4 mm pitch | 40 |

#### Reference document

JESD51-2 Integrated Circuits Thermal Test Method Environment Conditions - Natural Convection (Still Air). Available from [www.jedec.org](http://www.jedec.org/)

#### Selecting the product temperature range

When ordering the microcontroller, the temperature range is specified in the ordering information scheme shown in [*Section 8: Part numbering*](#_bookmark332).

Each temperature range suffix corresponds to a specific guaranteed ambient temperature at maximum dissipation and, to a specific maximum junction temperature.

As applications do not commonly use the STM32F303xB/STM32F303xC at maximum dissipation, it is useful to calculate the exact power consumption and junction temperature to determine which temperature range will be best suited to the application.

The following examples show how to calculate the temperature range needed for a given application.

##### Example 1: High-performance application

Assuming the following application conditions:

Maximum ambient temperature TAmax = 82 °C (measured according to JESD51-2), IDDmax = 50 mA, VDD = 3.5 V, maximum 3 I/Os used at the same time in output at low level with IOL = 8 mA, VOL= 0.4 V and maximum 2 I/Os used at the same time in output at low level with IOL = 20 mA, VOL= 1.3 V

PINTmax = 50 mA × 3.5 V= 175 mW

PIOmax = 3 × 8 mA × 0.4 V + 2 × 20 mA × 1.3 V = 61.6 mW

This gives: PINTmax = 175 mW and PIOmax = 61.6 mW: PDmax = 175 + 61.6 = 236.6 mW

Thus: PDmax = 236.6 mW

Using the values obtained in [*Table 86*](#_bookmark328)TJmax is calculated as follows:

– For LQFP64, 45°C/W

TJmax = 82 °C + (45°C/W × 236.6 mW) = 82 °C + 10.65 °C = 92.65 °C

This is within the range of the suffix 6 version parts (–40 < TJ < 105 °C).

In this case, parts must be ordered at least with the temperature range suffix 6 (see

[*Section 8: Part numbering*](#_bookmark332)).

##### Example 2: High-temperature application

Using the same rules, it is possible to address applications that run at high ambient temperatures with a low dissipation, as long as junction temperature TJ remains within the specified range.

Assuming the following application conditions:

Maximum ambient temperature TAmax = 115 °C (measured according to JESD51-2), IDDmax = 20 mA, VDD = 3.5 V, maximum 9 I/Os used at the same time in output at low level with IOL = 8 mA, VOL= 0.4 V

PINTmax = 20 mA × 3.5 V= 70 mW

PIOmax = 9 × 8 mA × 0.4 V = 28.8 mW

This gives: PINTmax = 70 mW and PIOmax = 28.8 mW:

PDmax = 70 + 28.8 = 98.8 mW

Thus: PDmax = 98.8 mW

Using the values obtained in [*Table 86*](#_bookmark328)TJmax is calculated as follows:

– For LQFP100, 41°C/W

TJmax = 115 °C + (41°C/W × 98.8 mW) = 115 °C + 4.05 °C = 119.05 °C

This is within the range of the suffix 7 version parts (–40 < TJ < 125 °C).

In this case, parts must be ordered at least with the temperature range suffix 7 (see

[*Section 8: Part numbering*](#_bookmark332)).

###### Table 87. Ordering information scheme

Example: STM32 F 303 R B T 6 xxx

6 = Industrial temperature range, –40 to 85 °C

7 = Industrial temperature range, –40 to 105 °C

**Options**

**Device family**

STM32 = ARM-based 32-bit microcontroller

**Product type**

F = general-purpose

**Device subfamily**

303 = STM32F303xx

**Pin count**

C = 48 pins R = 64 pins V = 100 pins

**Flash memory size**

B = 128 Kbytes of Flash memory

C = 256 Kbytes of Flash memory

**Package**

T = LQFP

Y = WLCSP

**Temperature range**

xxx = programmed parts TR = tape and reel

For a list of available options (speed, package, etc.) or for further information on any aspect of this device, please contact your nearest ST sales office.

# 9 Revision history

**Table 88. Document revision history**

|  |  |  |
| --- | --- | --- |
| **Date** | **Revision** | **Changes** |
| 22-Jun-2012 | 1 | Initial release |
| 07-Sep-2012 | 2 | Modified [*Features*](#_bookmark0)on cover page.  Modified *Table 2: STM32F301xx family device features and peripheral counts*  Added clock tree to [*Section 3.9: Clocks and startup*](#_bookmark28)  Added [*Table 7: STM32F303xB/STM32F303xC I2C implementation*](#_bookmark63)  Added [*Table 8: USART features*](#_bookmark67)  Added [*Table 9: STM32F303xB/STM32F303xC SPI/I2S implementation*](#_bookmark70)Modified [*Table 10: Capacitive sensing GPIOs available on*](#_bookmark79)[*STM32F303xB/STM32F303xC devices*](#_bookmark79)  Modified [*Figure 4*](#_bookmark87), [*Figure 5*](#_bookmark89)and [*Figure 6: STM32F303xB/STM32F303xC*](#_bookmark91)[*LQFP100 pinout*](#_bookmark91)  Modified [*Table 13: STM32F303xB/STM32F303xC pin definitions*](#_bookmark96)  Modified [*Figure 11: Power supply scheme*](#_bookmark119)Modified [*Table 21: Voltage characteristics*](#_bookmark124)Modified [*Table 22: Current characteristics*](#_bookmark126)  Modified [*Table 25: Operating conditions at power-up / power-down*](#_bookmark135)Added footnote to [*Table 31: Typical and maximum current consumption*](#_bookmark150)[*from the VDDA supply*](#_bookmark150)  Added footnote to [*Table 35*](#_bookmark161)and [*Table 36: Typical current consumption in*](#_bookmark163)[*Sleep mode, code running from Flash or RAM*](#_bookmark163)  Removed table “Switching output I/O current consumption” and table “Peripheral current consumption”  Added note under [*Figure 17: Typical application with a 32.768 kHz*](#_bookmark182)[*crystal*](#_bookmark182)  Updated *Table 49: HSI oscillator characteristics*  Updated [*Wakeup time from low-power mode*](#_bookmark169)and [*Table 39: Low-power*](#_bookmark171)[*mode wakeup timings*](#_bookmark171)  Updated [*Table 47: Flash memory characteristics*](#_bookmark194)  Updated [*Table 52: Electrical sensitivities*](#_bookmark204)  Updated [*Table 53: I/O current injection susceptibility*](#_bookmark207)Updated [*Table 54: I/O static characteristics*](#_bookmark211)Updated [*Table 55: Output voltage characteristics*](#_bookmark218)Updated [*Table 57: NRST pin characteristics*](#_bookmark225)Updated [*Table 63: SPI characteristics*](#_bookmark241)  Updated [*Table 64: I2S characteristics*](#_bookmark246)  Corrected LQFP100 in *Section 7.2.3: Selecting the product temperature range* |
| 21-Sep-2012 | 3 | Updated [*Table 63: SPI characteristics*](#_bookmark241) |

|  |  |  |
| --- | --- | --- |
| **Date** | **Revision** | **Changes** |
| 05-Dec-2012 | 4 | Updated first page  Removed references to VDDSDx and VSSSD Added reference to PM0214 in [*Section 1*](#_bookmark3)  Moved Temp. sensor calibartion values to[*Table 79*](#_bookmark296)and VREF calibration values to [*Table 29*](#_bookmark144)  Updated *Table 3: STM32F303xx family device features and peripheral counts*  Updated[*Section 3.4: Embedded SRAM*](#_bookmark15)  Updated [*Section 3.2: Memory protection unit (MPU)*](#_bookmark12)Updated [*Section 3.24: Universal serial bus (USB)*](#_bookmark73)Modified [*Section 3.26: Touch sensing controller (TSC)*](#_bookmark77)Updated heading of [*Table 8: USART features*](#_bookmark67)  Updated [*Table 13: STM32F303xB/STM32F303xC pin definitions*](#_bookmark96)Added notes to PC13, PC14 and PC15 in [*Table 13:*](#_bookmark96)[*STM32F303xB/STM32F303xC pin definitions*](#_bookmark96)  Updated [*Figure 11: Power supply scheme*](#_bookmark119)Modified [*Table 21: Voltage characteristics*](#_bookmark124)Modified [*Table 22: Current characteristics*](#_bookmark126)Modified [*Table 24: General operating conditions*](#_bookmark131)  Modified [*Figure 13: Typical VBAT current consumption (LSE and RTC*](#_bookmark159)[*ON/LSEDRV[1:0] = ’00’)*](#_bookmark159)  Updated [*Section 6.3.14: I/O port characteristics*](#_bookmark209)  Updated [*Table 30: Typical and maximum current consumption from VDD*](#_bookmark147)[*supply at VDD = 3.6V*](#_bookmark147)and [*Table 31: Typical and maximum current*](#_bookmark150)[*consumption from the VDDA supply*](#_bookmark150)  Updated [*Table 32: Typical and maximum VDD consumption in Stop and*](#_bookmark153)[*Standby modes*](#_bookmark153)and [*Table 33: Typical and maximum VDDA consumption*](#_bookmark155)[*in Stop and Standby modes*](#_bookmark155)  Updated [*Table 34: Typical and maximum current consumption from*](#_bookmark157)[*VBAT supply*](#_bookmark157)  Added [*Figure 13: Typical VBAT current consumption (LSE and RTC*](#_bookmark159)[*ON/LSEDRV[1:0] = ’00’)*](#_bookmark159)  Updated [*Table 35: Typical current consumption in Run mode, code with*](#_bookmark161)[*data processing running from Flash*](#_bookmark161)and [*Table 36: Typical current*](#_bookmark163)[*consumption in Sleep mode, code running from Flash or RAM*](#_bookmark163)  Added [*Table 38: Peripheral current consumption*](#_bookmark167)  Added [*Table 37: Switching output I/O current consumption*](#_bookmark165)Updated [*Section 6.3.6: Wakeup time from low-power mode*](#_bookmark169)Modified [*ESD absolute maximum ratings*](#_bookmark202)  Modified [*Table 55: Output voltage characteristics*](#_bookmark218)  Updated [*EMI characteristics*](#_bookmark199)  Updated [*Table 56: I/O AC characteristics*](#_bookmark220)  Updated [*Table 53: I/O current injection susceptibility*](#_bookmark207)  Updated [*Table 58: TIMx characteristics*](#_bookmark229)  Updated [*Section 7.4: WLCSP100 - 0.4 mm pitch wafer level chip scale*](#_bookmark320)[*package information*](#_bookmark320)  Added [*Table 69: Maximum ADC RAIN*](#_bookmark261)  Added [*Table 70: ADC accuracy - limited test conditions, 100-pin*](#_bookmark263)[*packages*](#_bookmark263)  Updated *Table 64: ADC accuracy - limited test conditions 2)*  Updated [*Table 75: DAC characteristics*](#_bookmark280)  Updated [*Table 77: Operational amplifier characteristics*](#_bookmark291)  Updated figures and tables in [*Section 7: Package information*](#_bookmark300) |

**Table 88. Document revision history (continued)**

|  |  |  |
| --- | --- | --- |
| **Date** | **Revision** | **Changes** |
| 08-Jan-2013 | 5 | Updated Vhys and Ilkg in [*Table 54: I/O static characteristics*](#_bookmark211). Updated VIL(NRST), VIH(NRST), and VNF(NRST) in [*Table 57: NRST pin*](#_bookmark225)[*characteristics*](#_bookmark225).  Updated [*Table 70: ADC accuracy - limited test conditions, 100-pin*](#_bookmark263)[*packages*](#_bookmark263)and *Table 64: ADC accuracy - limited test conditions 2)*. |
| 24-Jun-2013 | 6 | Replaced Cortex-M4F with Cortex M4 with FPU  Updated Core, Memories and SPI bullet points in [*Features*](#_bookmark0)Removed 8KB CCM SRAM from STM32F302xx devices, updated [*Figure 1: STM32F303xB/STM32F303xC block diagram*](#_bookmark8)and *Table 3:*  *STM32F303xx family device features and peripheral counts*  Updated [*Section 3.4: Embedded SRAM*](#_bookmark15)  Added VREF+ in [*Section 3.14: Digital-to-analog converter (DAC)*](#_bookmark46)  Removed DMA support for UART5 in [*Table 8: USART features*](#_bookmark67)  Added ‘reference clock detection’ bullet in [*Section 3.18: Real-time clock*](#_bookmark58)[*(RTC) and backup registers*](#_bookmark58)  Added paragraph ‘The touch sensing controller is fully...’ in [*Section 3.26:*](#_bookmark77)[*Touch sensing controller (TSC)*](#_bookmark77)  Updated [*Comparison of I2C analog and digital filters*](#_bookmark61)  Updated [*Section 3.10: General-purpose input/outputs (GPIOs)*](#_bookmark32)Added ‘EVENTOUT’ in [*Table 13: STM32F303xB/STM32F303xC pin*](#_bookmark96)[*definitions*](#_bookmark96)and added note to ‘VREF+’ pin  Updated IVDD in [*Table 22: Current characteristics*](#_bookmark126)and [*Output driving*](#_bookmark216)[*current*](#_bookmark216)  Updated [*Table 61: I2C timings specification (see I2C specification,*](#_bookmark235)[*rev.03, June 2007)*](#_bookmark235)and [*Figure 25: I2C bus AC waveforms and*](#_bookmark239)[*measurement circuit*](#_bookmark239)  Added VREF+ row to [*Table 68: ADC characteristics*](#_bookmark255), replaced VDDA with VREF+, updated tconv and added note to ‘conversion voltage range Added VREF+ row to [*Table 75: DAC characteristics*](#_bookmark280)and replaced VDDA with VREF+  Added ‘PGA BW’ and ‘en’ in [*Table 77: Operational amplifier*](#_bookmark291)[*characteristics*](#_bookmark291) |
| 13-Nov-2013 | 7 | Removed STM32F302xB/STM32F302xC products (now in a separate datasheet).  Added I2S feature for SPI2 and SPI3  Added tSP to [*Table 61: I2C timings specification (see I2C specification,*](#_bookmark235)[*rev.03, June 2007)*](#_bookmark235).  Renamed tSP to tAN in[*Table 62: I2C analog filter characteristics*](#_bookmark237). Added tSTAB in [*Table 68: ADC characteristics*](#_bookmark255)  Renamed VOPAMPx to VREFOPAMPx  Updated [*Table 71: ADC accuracy, 100-pin packages*](#_bookmark267).  Updated ADC channel names in [*Section 3.13.1*](#_bookmark39), [*Section 3.13.2*](#_bookmark41)and  [*Section 3.13.3*](#_bookmark43). |

|  |  |  |
| --- | --- | --- |
| **Date** | **Revision** | **Changes** |
| 18-Apr-2014 | 8 | Updated [*Table 50: EMI characteristics*](#_bookmark199)conditions :3.3v replaced by 3.6V. Updated [*Section 6.3.17: Communications interfaces*](#_bookmark233)I2C interface.  Updated [*Table 77: Operational amplifier characteristics*](#_bookmark291)adding TS\_OPAMP\_VOUT row.  Updated [*Section 3.13: Fast analog-to-digital converter (ADC)*](#_bookmark37). updated ARM and Cortex trademark.  Updated [*Table 32: Typical and maximum VDD consumption in Stop and*](#_bookmark153)[*Standby modes*](#_bookmark153)with Max value at 85°C and 105°C.  Updated [*Table 70: ADC accuracy - limited test conditions, 100-pin*](#_bookmark263)[*packages*](#_bookmark263)and [*Table 71: ADC accuracy, 100-pin packages*](#_bookmark267)for 100-pin package.  Added [*Table 72: ADC accuracy - limited test conditions, 64-pin*](#_bookmark270)[*packages*](#_bookmark270)and [*Table 73: ADC accuracy, 64-pin packages*](#_bookmark272)for 64-pin package.  Added [*Table 74: ADC accuracy at 1MSPS*](#_bookmark275)for 1MSPS sampling frequency.  Updated [*Table 63: SPI characteristics*](#_bookmark241). Updated [*Table 75: DAC characteristics*](#_bookmark280). |
| 09-Dec-2014 | 9 | Updated core description in cover page.  Updated HSI characteristics [*Table 44: HSI oscillator characteristics*](#_bookmark185)and [*Figure 18: HSI oscillator accuracy characterization results for soldered*](#_bookmark188)[*parts*](#_bookmark188).  Updated [*Table 58: TIMx characteristics*](#_bookmark229).  Updated [*Table 13: STM32F303xB/STM32F303xC pin definitions*](#_bookmark96)adding note for I/Os featuring an analog output function (DAC\_OUT,OPAMP\_OUT).  Updated [*Table 68: ADC characteristics*](#_bookmark255)adding IDDA & IREF consumptions.  Added [*Figure 32: ADC typical current consumption on VDDA pin*](#_bookmark257)and  [*Figure 33: ADC typical current consumption on VREF+ pin*](#_bookmark259). Added [*Section 3.8: Interconnect matrix*](#_bookmark25).  Updated [*Figure 2: Clock tree*](#_bookmark30).  Added note after [*Table 32: Typical and maximum VDD consumption in*](#_bookmark153)[*Stop and Standby modes*](#_bookmark153).  Updated [*Section : In order to meet environmental requirements, ST*](#_bookmark301)[*offers these devices in different grades of ECOPACK® packages, depending on their level of environmental compliance. ECOPACK® specifications, grade definitions and product status are available at:*](#_bookmark301)[*www*](#_bookmark301)[*.st.com.*](http://www.st.com/)[*ECOPACK® is an ST trademark.*](#_bookmark301)with new LQFP100, LQFP64, LQFP48 package marking.  Updated [*Table 13: STM32F303xB/STM32F303xC pin definitions*](#_bookmark96)and alternate functions tables replacing usart\_rts by usart\_rts\_de. |
| 29-Jan-2015 | 10 | Updated [*Section 6.3.20: Comparator characteristics*](#_bookmark284)modifying ts\_sc characteristics in [*Table 76*](#_bookmark286)and adding [*Figure 37: Maximum VREFINT*](#_bookmark288)[*scaler startup time from power down*](#_bookmark288).  Updated IDD data in [*Table 42: HSE oscillator characteristics*](#_bookmark178). |

**Table 88. Document revision history (continued)**

|  |  |  |
| --- | --- | --- |
| **Date** | **Revision** | **Changes** |
| 17-Apr-2015 | 11 | Updated [*Section 7: Package information*](#_bookmark300): with new package information structure adding 1 sub paragraph for each package.  Updated [*Figure 41: LQFP100 – 14 x 14 mm, low-profile quad flat*](#_bookmark307)[*package top view example*](#_bookmark307)removing gate mark.  Added note for all packages about the device marking orientation: “the following figure gives an example of topside marking orientation versus pin 1 identifier location”.  Updated [*Table 82: LQFP64 – 10 x 10 mm, low-profile quad flat package*](#_bookmark311)[*mechanical data*](#_bookmark311). |
| 11-Dec-2015 | 12 | Added WLCSP100:   * Updated cover page. * Updated [*Table 2: STM32F303xB/STM32F303xC family device*](#_bookmark6)[*features and peripheral counts*](#_bookmark6). * Added [*Figure 7: STM32F303xB/STM32F303xC WLCSP100 pinout*](#_bookmark93). * Updated [*Table 13: STM32F303xB/STM32F303xC pin definitions*](#_bookmark96). * Updated [*Table 24: General operating conditions*](#_bookmark131). * Added [*Section 7.4: WLCSP100 - 0.4 mm pitch wafer level chip scale*](#_bookmark320)[*package information*](#_bookmark320). * Updated [*Table 86: Package thermal characteristics*](#_bookmark329). * Updated [*Table 87: Ordering information scheme*](#_bookmark334).   Updated [*Figure 4*](#_bookmark87), [*Figure 5*](#_bookmark89), [*Figure 6*](#_bookmark91), [*Table 13*](#_bookmark96)and [*Table 22*](#_bookmark126)removing all VDD and VSS indexes.  Updated all the notes removing ‘not tested in production’.  Updated [*Table 68: ADC characteristics*](#_bookmark255)adding VREF- negative voltage reference.  Update [*Table 21: Voltage characteristics*](#_bookmark124)adding table note 4. |

**IMPORTANT NOTICE – PLEASE READ CAREFULLY**

STMicroelectronics NV and its subsidiaries (“ST”) reserve the right to make changes, corrections, enhancements, modifications, and improvements to ST products and/or to this document at any time without notice. Purchasers should obtain the latest relevant information on ST products before placing orders. ST products are sold pursuant to ST’s terms and conditions of sale in place at the time of order acknowledgement.

Purchasers are solely responsible for the choice, selection, and use of ST products and ST assumes no liability for application assistance or the design of Purchasers’ products.

No license, express or implied, to any intellectual property right is granted by ST herein.

Resale of ST products with provisions different from the information set forth herein shall void any warranty granted by ST for such product.

ST and the ST logo are trademarks of ST. All other product or service names are the property of their respective owners.

Information in this document supersedes and replaces information previously supplied in any prior versions of this document.

© 2015 STMicroelectronics – All rights reserved